IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Specification Framework for TGah | | | | |
| Date: 2012-5-17 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Minyoung Park | Intel | 2111 NE 25th Ave, Hillsboro OR 97124, USA | 503-712-4705 | [minyoung.park@intel.com](mailto:minyoung.park@intel.com) |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document provides the framework from which the draft TGah amendment will be developed. The document provides an outline of each the functional blocks that will be a part of the final amendment. The document is intended to reflect the working consensus of the group on the broad outline for the draft specification. As such it is expected to begin with minimal detail reflecting agreement on specific techniques and highlighting areas on which agreement is still required. It may also begin with an incomplete feature list with additional features added as they are justified. The document will evolve over time until it includes sufficient detail on all the functional blocks and their inter-dependencies so that work can begin on the draft amendment itself.

# 0 Revision Notes

|  |  |
| --- | --- |
| R0 | Initial draft document with a table of content |
| R1 | Added supporting bandwidth modes [11/1294r0]  Added the number of tones for 2MHz PHY transmission and the tone spacing for all other bandwidth modes [11/1311r0] |
| R2 | Added max number of space-time streams [11/1275r1]  Added channelization [11/1329r1] |
| R3 | Modified South Korea channelization [11/1422r0]  Added support for a new frame format for a short beacon [11/1503r1] |
| R4/5 | Added the motions passed in January 2012 |
| R6 | Added the motions passed in March 2012 |
| R7 | Added the motions passed in May 2012 |

# 1 Definitions

# 2 Abbreviations and Acronyms

S1G sub 1 GHz

PLCP physical layer convergence procedure

STA station

MAC medium access control

MCS0 BPSK, ½ code rate

SUBF single user beamforming

# 3 S1G Physical Layer

This section describes the functional blocks of the physical layer.

## 3.1 Channelization

R.3.1.A: The draft specification shall include support for 1 MHz, 2 MHz, 4 MHz, 8 MHz, and 16 MHz PHY transmissions. [11/1294r0]


R.3.1.B: An 802.11ah STA shall support reception of 1 MHz and 2 MHz PHY transmissions. [11/1294r0]

R.3.1.C: The 2 MHz PHY transmission shall be an OFDM based waveform consisting of a total of 64 tones (including tones allocated as pilot, guard and DC). Note: This implies a tone spacing of 31.25 kHz. [11/1311r0]


R.3.1.D: The tone spacing for all other bandwidths PHY transmissions shall be same as the tone spacing in the 2 MHz PHY transmission. [11/1311r0]

R.3.1.E: The draft specification shall include the following channelization [11/1329r1]


1. South Korea [11/1422r0]




1. Europe




1. Japan




1. China



1. Singapore [12/111r1]:
2. Supporting bands: 866-869 MHz, 920-925MHz



1. United States [May 2012 meeting minutes, 12/0613r0]
2. 26 1MHz channels, 13 2MHz channels, 6 4MHz channels, 3 8MHz channels and one 16MHz channel



### 3.1.1 Transmission rules

R.3.1.1.A: The draft specification shall support the following 1 MHz transmission rules [12/309r1].

* In 2MHz BSS, 1MHz waveform is only allowed at the lower side.
* In 4/8/16MHz BSS, when primary 2MHz is at lower most of the overall band, then 1MHz is only allowed at upper side of the 2MHz primary channel; when primary 2MHz is at upper most of the overall band, 1MHz is only allowed at lower side of the 2MHz primary channel; when primary 2MHz is in the middle of the overall band, 1MHz waveform position is TBD.

## 3.2 S1G PLCP Sublayer

R.3.2.A: 11ah defines single stream pilots in the LTF, SIG and Data fields of short preamble packets, using the first column of P matrix for multi-stream mapping, as below:

1. For SIG field in Short Preamble Format, the transmitted pilot tone signals, in the k-th tone and n-th OFDM symbol in each 2MHz subband of the >=2MHz short preamble format SIG field is expressed as: [May 2012 meeting minutes, 12/363r2]





1. For SIGA Field in >=2MHz Long Preamble Format, the transmitted pilot tone signals, in the k-th tone and n-th OFDM symbol in each 2MHz subband of the >=2MHz long preamble format SIGA field is expressed as:





1. For **>=**2MHz LTFs in Short Preamble format, and D-LTFs in the Long preamble format, the transmitted pilot tone signals, in the k-th tone of each LTF field in the >=2MHz short preamble format, and of each D-LTF field in the >=2MHz long preamble format is expressed as:





1. For **>=**2MHz SIGB/Data, the transmitted pilot tone signals, in the k-th tone and n-th OFDM symbol in SIGB (when applicable) and Data fields in >=2MHz PPDUs is expressed as:





The pilot mapping and values for 2/4/8/16 MHz transmissions, respectively, refer those for 20/40/80/160 MHz transmissions in section 22.3.10.10 (Pilot subcarriers) of IEEE P802.11ac™/D2.0. [12/xxxr0, 12/363r2-motion2]

1. For 1MHz LTFs, the transmitted pilot tone signals, in the k-th tone and in each LTFs for 1MHz PPDU is expressed as:





1. For 1MHz SIG field and Data Field, the transmitted pilot tone signals, in the k-th tone and n-th OFDM symbol of 1MHz SIG and Data fields is expressed as:





For a 1MHz transmission, two pilot tones shall be inserted in. The pilot mapping for subcarrier *k* for symbol *n* shall be as specified in the following equation. [12/xxxr0, 12/363r2-motion1]

where, is given in Table 22-20 of IEEE P802.11ac™/D2.0 and where *n* is the DATA symbol index.

### 3.2.1 Preamble

R.3.2.1.A: In any 11ah short GI packet, short GI starts from the 2nd Data symbol, and the 1st Data symbol is always long GI.

* Include Multi-stream or MU packets

R.3.2.1.B: STF and LTF sequences for higher FFT sizes are based on 11ac [12/115r0,slide7]

R.3.2.1.C: The draft specification shall include 2-bit Ack Indication (00: Ack; 01: BA; 10: No Ack; 11: reserved) in SIG.

R.3.2.1.D: The draft specification shall use the 4 LSB of the 11n HTSIG field 8-bit CRC for the 4-bit CRC in 11ah 2MHz and 1MHz SIG(A) fields, and use the same 11n HTSIG field 8-bit CRC in SIGB field of the >=2MHz long preamble [May 2012 meeting minutes, 12/596r0].

### 3.2.1.1 PHY greater than or equal to 2 MHz

R.3.2.1.1.A: The general structure for short preamble open-loop packet is similar to 11n green field preamble, as below:



Each field is defined as follows:

1. STF Field
   1. Use the same tone design as in 11n, i.e. in each 2MHz, STF occupies 12 non-zero tones in {±4 ±8 ±12 ±16 ±20 ±24}.
   2. None-zero tones are mapped to space-time streams using the first column of P matrix, the same way as in 11n GF preamble.



1. LTF Fields
   1. Define the 11ah LTF signs for >= 2MHz PPDUs the same as the VHTLTF signs in the corresponding 11ac packets with the same FFT sizes.
      1. This is also applicable to the LTF1 and D-LTFs fields in the long preamble format. [12/597r0 –motion1]
   2. In data tones of LTF, the mapping from NSTS space-time streams to NLTF LTFs is the same as in 11n green field preamble, with the P matrix.




### SIG Field

* 1. 2 symbols, each modulated using Q-BPSK, same as in 11n green field preamble.
  2. 48 data tones occupying tones {-26:26} within each 2MHz subband, and modulated using 11n/11ac MCS0. [12/308r2, Motion1]
  3. Data tones are mapped to multiple space-time streams using the first column of P matrix—the same as in 11n GF preamble.



R.3.2.1.1.B: The general long preamble structure packets use a “mixed-mode” format shown below:

* This frame format can also be used for SUBF [12/373r0]



1. Omni Portion
   1. SIGA field has 48 data tones, occupying tones {-26:26} as in 11n/11ac SIG fields [12/597r0-motion1]
   2. STF/LTF1/SIG fields applies single stream in each subcarrier (without the 1st column P matrix mapping as seen in short preamble), similar to the legacy portion of 11n MM preamble and 11ac preamble.



* 1. SIG field subfield definition is different from short preamble, and the two symbols in SIG field are modulated using QBPSK and BPSK respectively
     1. Refer to R.3.2.1.1.C.

1. Data Portion
   1. D-STF is the same as (downclocked) 11ac VHT-STF.
   2. Modulation flows of D-STF, D-LTFs, and SIGB are the same as 11ac MU packets.
      1. i.e. all streams for all users are trained by D-LTFs.
      2. Up to 4 space-time stream across all users (refer to [11/1275r1]).

R.3.2.1.1.C: Short and long preamble autodetection

1. For >=2MHz short preamble and long preamble packets, the 1st SIG symbol is always QBPSK
   1. Used for autodetection between 1MHz and 2MHz preamble—refer to [11/1482r3].
2. The 2nd SIG symbol is used for autodetection between short preamble and long preamble packets.



R.3.2.1.1.D: 4/8/16 MHz frame format

1. For 4MHz, 8MHz, and 16MHz packets, the STF/LTF/SIG field designs are similar to 11ac 40/80/160MHz.
   1. STF/SIG fields are repeated and phase rotated (same as in 11ac) over each 2MHz subband.

R.3.2.1.1.E: SIG field content for >=2MHz

1. 2MHz SIGA [12/308r2, Motion2]


|  |  |  |
| --- | --- | --- |
|  | **Short Preamble** | **Long Preamble** |
| Length / Duration | 9 | 9 |
| MCS | 4 |  |
| BW | 2 | 2 |
| Aggregation | 1 |  |
| STBC | 1 | 1 |
| Coding | 2 | 5 |
| SGI | 1 | 1 |
| GID |  | 6 |
| Nsts | 2 | 8 |
| PAID | 9 |  |
| Ack Indication | 2 | 2 |
| Reserved | 5~~7~~ | 4~~6~~ |
| CRC | 4 | 4 |
| Tail | 6 | 6 |
| **Total** | **48** | **48** |

* 1. LENGTH/DURATION: in num of symbols when aggregation is 1, is in num of bytes when aggregation is 0, Mandate AMPDU for packet sizes > 511 bytes and for long preamble.
  2. STBC: Same as in 11ac (Alamouti code on all streams or none).
  3. Nsts: for short preamble (2 bits), represents 1~4 STS; for long preamble (8 bits), represents 0~3 STS per user for the 4 users.
  4. Coding: for short preamble 1 bit indicates BCC/LDPC, the other bits indicates additional symbol during LDPC encoding process; for long preamble, 4 bits indicates BCC/LDPC of 4 clients, and 1 bit indicates whether additional symbols happens for any user when encoding LDPC (same as 11ac).
  5. MCS: for short preamble, 4 bit MCS index; for long preamble, reuse 3 bits for BCC/LDPC indicator for users 2~4—similar as in 11ac VHTSIGA.
  6. Aggregation: Mainly applicable for short preamble, reserved for long preamble.
  7. CRC: 4 bits of CRC should be enough as shown in the Appendix
  8. GID: 6-bit GID as in 11ac for long preamble, not needed for short preamble.
  9. PAID: 9 bits PAID, not needed for long preamble.
  10. Ack Indication: 2 bits [refer to R.3.2.1.C]

1. 2MHz SIGB (long preamble)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **BW (MHz)** | | | |
|  | **2** | **4** | **8** | **16** |
| MCS | 4 | 4 | 4 | 4 |
| Tail | 6 | 6 | 6 | 6 |
| CRC | 8 | 8 | 8 | 8 |
| Reserved | 8 | 9 | 11 | 11 |
| **Total** | 26 | 27 | 29 | 29 |

R.3.2.1.1.F: The draft specification shall include the following 11ah NDP format [May 2012 meeting minutes, 617r0-motion1]



The 11ah NDP format is same with 2MHz PHY short frame format defined in R.3.2.1.1.A.

1. The SIG field of 11ah NDP shall include following fields [May 2012 meeting minutes, 617r0-motion2]:
   1. MCS : set to 0
   2. Length/Duration: set to 0
   3. BW : set to the same value as the TXVECTOR parameter CH\_BANDWIDTH in the preceding VHT NDP Announcement frame
   4. Nsts : indicates two or more space-time streams

R.3.2.1.1.G: The draft specification shall support that all NDP frames sent in >=2MHz use the short preamble format, including Short-ACK, and all future NDP short MAC frames [May 2012 meeting minutes, 617r0-motion3].

### 3.2.1.2 1 MHz mode PHY

R.3.2.1.2.A: The 802.11ah specification shall use the following STF and LTF sequences for 32 FFT:


1. STF sequence [12/115r0,slide4]
   * Tone index=[-12 -8 -4 4 8 12]
   * Values: [0.5, -1, 1, -1, -1, -0.5]x(1+j)x γ   where γ is a normalization factor
   * γ = 2.4 for MCS0 rep2, 1.7 otherwise
2. LTF sequence [12/115r0, slide7]
   * Tone index is [-16 -15 -14 …. -1 0 1 ….. 14 15]   
     =[0 0 0 1 -1 1 -1 -1 1 -1 1 1 -1 1 1 1 0 -1 -1 -1 1 -1 -1 -1 1 -1 1 1 1 -1 0 0]

R.3.2.1.2.B: The 802.11ah draft specification shall have a 4 symbol packet detection section for the 1 MHz mode [11/1482r4, motion2].

1. A 3 dB power boost is only applied for 2x repetition MCS
2. Have same periodicity as 2 MHz STF with following tone allocations:
   1. For 2MHz {±4 ±8 ±12 ±16 ±20 ±24}
   2. For 1MHz {±4 ±8 ±12}.

R.3.2.1.2.C: The 802.11ah draft specification shall have the general preamble structure for 1MHz SU open loop packet as in the figure below [11/1482r4, motion3].

1. The relationship between NSTS and NLTF is the same as 11n/11ac (for 2 through 4 streams), using the same P matrix (for 1 through 4 streams)



R.3.2.1.2.D: The 802.11ah draft specification shall have 1MHz SIG field contents as follows.

|  |  |  |
| --- | --- | --- |
| **SIG Field** | **Bits** | **Comments** |
| STBC | 1 | Same as in 11ac |
| Num SS | 2 | Number of spatial streams for SU |
| SGI | 1 | Short Guard Interval |
| Coding | 2 | 1st bit is coding type (LDPC/BCC), 2nd bit is for LDPC Nsym ambiguity |
| MCS | 4 | MCS |
| Aggregation bit | 1 | Signals use of AMPDU |
| Length | 9 | Length field (in symbols when aggregation is ON, is in bytes when aggregation is OFF, Mandate AMPDU for packet sizes > 511 bytes |
| Ack Indication | 2 | 00: Ack; 01: BA; 10: No Ack; 11: reserved [refer to R.3.2.1.C] |
| Reserved | 4 (TBD) | Some possible uses are MAC bits or any other new features etc. Details TBD |
| CRC | 4 | 4 bits of CRC should be enough |
| Tail | 6 (TBD) | Tail-biting can be explored |
| **Total** | **36** |  |


* **SIG goes at BPSK-rate ½ -rep 2**
* **No MU transmissions for the 1MHz mode**
* **No AID supported**

### 3.2.2 Transmission flow

3.2.2.1 Transmission flow for 11ah regular non-repetition MCSs

R.3.2.2.1.A: The general transmission flow for 11ah regular non-repetition MCSs is shown below.


* Apply the same Tx flowin 11ac in the data tones for the data field.



R.3.2.2.1.B: The 11ah stream parser is the same as 11ac.

R.3.2.2.1.C: The 11ah encoder parser and segment parser (16MHz only) are the same as 11ac; NES in the MCSs of 2/4/8/16MHz is the same as the corresponding values in 11ac; and NES = 1 in all the MCSs of 1MHz.

R.3.2.2.1.D: The 802.11ah specification framework shall have the following transmission flow for MCS0-Rep2 mode.[12/1484r6]



* MCS0 Rep2 is applied only for single space-time stream.
  + NSS=1, no STBC
* The “2x block-wise repetition”performed on a per-OFDM symbol basis:
  + Cout=[C1….C2NDBPS , C1….C2NDBPS ], where [C1….C2NDBPS] are the FEC output bits per symbol.
  + Interleaver parameters are the same as regular MCS0.
* Receiver may conduct MRC combining to improve SNR.


### 3.2.3 Tone plans

**3.2.3.1 >= 2MHz PHY**

R.3.2.3.1.A: >=2MHz follows the same tone plans as the corresponding FFT sizes in 11ac [11/1484r6].

**3.2.3.2 1 MHz PHY**

R.3.2.3.2.A: Define the 1MHz tone allocation as: 24 Data tones, 2 Pilot tones at tone indices +/-7, 3 Guard tones on left and 2 guard tones on right, and 1 DC tone [11/1484r6].



R.3.2.3.2.B: The 802.11ah specification shall use Ncol=8, Nrot=2 as the 32 FFT interleaver choice. [12/369r0]

## 3.3 Modulation and Coding Scheme (MCS)

R.3.3.A: The 802.11ah specification shall allow following 11ah MCSs [11/1484r6]:

1. For 1MHz, 11ac MCS0~9, as well as an MCS0-rep2 mode and more modes TBD.
2. For >=2MHz, the MCS tables for BCC are the same as the corresponding tables in 11ac before downclocking, i.e. same MCS exclusions for BCC as in 11ac.

R.3.3.B: The 802.11ah specification shall adopt MCS0 rep 2 as the lowest rate for 1 MHz [11/1484r4, motion1].

## 3.4 Spatial Multiplexing

R.3.4.1.A: The maximum number of space-time streams (NSTS) in a data PPDU transmission shall be less than or equal to 4. [11/1275r1]

## 3.5 Transmit Beamforming

R.3.5.A: The 802.11ah specification shall support, for all applicable BW, the SUBF and MU-MIMO feedback structure and protocol as specified in the following sections of IEEE P802.11ac™/D2.0, as an optional feature [12/371r0]:

* 8.4.1.46 VHT MIMO Control field
* 8.4.1.47 VHT Compressed Beamforming Report field - contents of feedback frame
* 8.4.1.48 MU Exclusive Beamforming Report field - contents of MU frame
* 9.31.5 VHT sounding protocol
* 22.3.11 and its subsections: SU-MIMO and MU-MIMO Beamforming

# 4 MAC Layer

This section describes the functional blocks of the MAC layer.

## 4.1 Power Save

R.4.1.A: An AP may provide its TSF timer accuracy information to non-AP STAs [12/130r0]**.**

R.4.1.B: The 802.11ah draft specification shall define the following operation mode. [12/127r1]

1. STA may send a PS-Poll at any time
2. AP shall respond immediately to a PS Poll with either
   1. Data for the requesting STA, or
   2. ACK frame with 1bit-field indicating
      1. 1: traffic is buffered (as indicated in the TIM map), stay awake (i.e. a service period starts)
      2. 0: no traffic is buffered, go back to sleep
      3. The bit used in current ACK frame format is the More Data field

R.4.1.C: The draft specification shall support that BSS Max Idle Period shall be able to set to a longer value (~days) by changing the unit of Max Idle Period larger than 1000 TU (1s). The sleep interval unit extension method is TBD [May 2012 meeting minutes].

R.4.1.D: The draft specification shall support that the AP shall be able to support multiple Max Idle Periods. [May 2012 meeting minutes]

R.4.1.E: The draft specification shall support the concept that a non-TIM STA shall transmit at least one PS-Poll or trigger frame every Listen Interval and the non-TIM STA is not required to wake to receive a beacon each Listen Interval. [May 2012 meeting minutes, 12/618r0]

## 4.2 Channel Access

R4.2.A: The draft specification shall support the highest channel access priority to the sensor type of STAs [May 2012 meeting minutes, 1230r1].

R.4.2.B: The draft specification shall support the concept of utilizing information from an AP to spread out uplink transmissions over a period of time to mitigate the hidden node problem [May 2012 meeting minutes, 12/606r1]

R.4.2.C: Grouping of STAs shall be introduced to the draft specification for controlling the number of STAs performing channel access and to save energy. [May 2012 meeting minutes, 12/650r0]

## 4.3 Large Number of STAs Support

### 4.3.1 Traffic Indication Map (TIM) operation

R.4.3.1.A: The complete traffic indication bitmap shall be divided into one or more segments and transmitting in one or more TIM elements for a large network [12/117r0].

R.4.3.1.B: When the complete traffic indication bitmap is divided into multiple segments, the range of the AIDs (bitmap) each segment is covering shall be known to the STAs [12/117r0].


R.4.3.1.C: 11ah STAs can choose not to have a TIM entry for the DL traffic signalling. For these stations, the AP will store the DL data and deliver it when the STA request it. [May 2012 meeting minutes, 12/610r0-motion 1]

R.4.3.1.D: 11ah STAs shall inform AP if they do not need a TIM entry for the DL signalling during the association process. [May 2012 meeting minutes, 12/610r0-motion2]

### 4.3.2 TIM structure


R.4.3.2.A: TIM shall have the three level hierarchical structure shown in the below figure [May 2012 meeting minutes, 12/388r2].

- Three level hierarchy: Page/Block/Sub-Block:



R.4.3.2.B: Based on the TIM structure shown in R.4.3.2.A, the association identifier (AID) structure shall be maintained as the below figure [May 2012 meeting minutes, 12/388r2].


- STAs are grouped into Page, Blocks, Sub-Blocks:




### 4.3.3 TIM encoding

R.4.3.3.A: The Partial Virtual Bitmap field shall be encoded in Block level as shown in the below figure [May 2012 meeting minutes, 12/388r2].

* Partial Virtual Bitmap consists of one or more encoded Blocks of a single Page.
* Basic Block encoding: Block Offset (5 bits) + Block Control(3 bits) + Block Bitmap (1 octet) + Sub-Block Bitmaps (variable)
* Block Control field: controls how the Block Bitmap and the Sub-Block Bitmap fields are used
  1. Block bitmap encoding: AID = [Page Index(2b), Block Offset(5b), n(3b), m(3b)]
     + The n-th bit position of the Block Bitmap indicates whether the n-th Sub-Block Bitmap is present in the Sub-Block field
     + The m-th bit position of the Sub-Block Bitmap indicates whether the m-th STA has data buffered at the AP
  2. Single AID: when there is a single AID in a Block, 6 bits of the Block Bitmap field is used to indicate the AID and the Sub-Block field is not present (total 2 octets): AID = [Page Index(2b), Block Offset(5b), Block Bitmap[5:0]]
  3. Inverse bitmap: if there are many 1s in the bitmap of the Block, inverse the bitmap and encode the inversed bitmap



* 1. Offset+Length+Bitmap: encodes more than 8 Sub-Block Bitmaps [20, 21]
     + The Block Bitmap field is used to indicate the *length* of Sub-Block Bitmaps following the Block Bitmap field.
     + **AID = [Page Index (2b), Block Offset(5b),zeros(6b)]+ p,** the p-th bit position of the Sub-Block Bitmap field indicates whether the p-th STA has data buffered at the AP.
     + This mode is used when more than 8 contiguous Sub-Blocks are transmitted.



## 4.4 Frame Formats

### 4.4.1 Management frames

### 4.4.1.1 Short Beacon frame format

R.4.4.1.1.A: The draft specification shall provide support for a new frame format for a short beacon (content is TBD). [11/1503r1]

R.4.4.1.1.B: The draft specification shall define a Short Beacon interval, in units of TUs, and to require that the Beacon Interval is an integer multiple of the Short Beacon Interval.

R.4.4.1.1.C: The Frame Control type/subtype indication for the Short Beacon.

* Frame Control
  + To indicate a Short Beacon we build on type/subtype field modifications proposed by 11ad
  + Propose: B3 B2 = 11  
     B7 B6 B5 B4 = 0 0 0 1 (currently reserved)  
    as indication of Short Beacon

R.4.4.1.1.D: The Short Beacon should include a compressed SSID field.

* 1. Compressed SSID is computed as the CRC of SSID. CRC is computed using the same function as used to compute the FCS of MPDUs [May 2012 meeting minutes, 12/129r3]

R.4.4.1.1.E: The Short Beacon shall include a 4 byte Timestamp containing the 4 LSBs of the AP Timestamp.


R.4.4.1.1.F: The Short Beacon shall include a 1 byte Change Sequence Field that is incremented whenever critical network information changes.

R.4.4.1.1.G: The Short Beacon shall optionally include a field indicating the time of next full beacon.

1. Time of next full beacon is indicted as the higher 3 bytes of the 4 LSBs of the AP time stamp at the next full beacon [May 2012 meeting minutes, 12/129r3]
2. The Time of Next Full Beacon field shall be always present in the short Beacon frame if an AP transmits full (long) Beacon frames periodically [May 2012 meeting minutes, 12/129r3]

R.4.4.1.1.H: The draft specification shall include an optional Access Network Options field in the short beacon [May 2012 meeting minutes, 12/129r3]

R.4.4.1.1.I: The 3 bit BW field shall be included in the FC field as shown in the figure below: [May 2012 meeting minutes, 12/129r3]



R.4.4.1.1.J: The following indications shall be in the short beacon: [May 2012 meeting minutes, 12/129r3]

* Presence of Time of Next Full Beaconfield
* Presence of Compressed SSIDfield
* Presence of Access Network Optionsfield

### 4.4.2 Control frames

### 4.4.2.1. Short ACK frame format

R.4.4.2.1.A: The draft specification shall support the following short ACK format [12/324r2, Motion1].



1. The following short ACK SIG fields are the same as those in normal SIG[12/324r2, Motion2].
   * CRC (4 bits)
   * Tail (6bits - TBD)
2. A reserved MCS value shall be used to indicate the short ACK frame[12/324r2, Motion3].
3. The short ACK SIG shall include an ACK ID field (bits TBD), and use [12/324r2, Motion4].
   * partial FCS and
   * the information from the scambling seed in the SERVICE field of the frame being acknowledged for the computation of the ACK ID for short ACK frames.

### 4.4.2.2. Short CTS frame format

R.4.4.2.2.A: The draft specification shall define a short CTS format as follows with SIG field design TBD: [May 2012 meeting minutes, 12/643r0]



### 4.4.3 Management frame body components

4.4.3.A: The specification shall support to indicate service type during association. [May 2012 meeting minutes, 12/612r0]

### 4.4.3.1 Information elements

### 4.4.3.1.1 Open-Loop Link Margin Index element

R.4.4.3.1.1.A: The draft specification shall include Open-Loop Link Margin Index element as defined below [May 2012 meeting minutes, 12/0645r1]:



where the Open-Loop Link Margin Index is computed according to the following equation.



The detailed format and description are TBD.

### 4.4.4 MAC header compression


R.4.4.4.A: The draft specification shall support the concept of storing constant MAC header information (e.g. A3/A4) at the transmitter/receiver through a management exchange as an optional feature [May 2012 meeting minutes, 12/646r0]

### 4.4.4.1. Short MAC Header

R.4.4.4.1.A: The draft specification shall include the short MAC Header Format as shown below [May 2012 meeting minutes, 12/646r0]:

- Sequence Ctrl length is TBD

-A3 is optionally present with an A3 present indication (TBD)



R.4.4.4.1.B: The draft specification shall support the addressing method in the following table (addressing interpretation indication for DL/UL/Direct is TBD; A3 is optionally present based on an indication TBD). [May 2012 meeting minutes, 12/646r0]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Data** | | | | |
| **Direction** | **Address Interpretation**  **(From-AP)** | **A1** | **A2** | **A3 (SA/DA)** |
| DL | 1 | Rx-AID | BSSID | (SA) |
| UL | 0 | BSSID | Tx-AID | (DA) |
| Direct | 0 | RA | Tx-AID |  |

**References:**

11/1294r0 Spec Framework Text for 11ah Bandwidth Modes

11/1311r0 Spec Framework Text for PHY Numerology

11/1275r1 Spatial stream support in TGah specification

11/1329r0 Motions and Strawpoll on Channelization for 11ah

11/1318r0 Japanese Channelization for 802.11ah

11/1320r1 11ah Channelization of China

May 2012 meeting minutes may 2012 tgah meeting minutes.doc