`IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LB187 - Comment Resolution | | | | |
| Date: May 4, 2012 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Chao-Chun Wang | MediaTek |  |  | Chaochun.wang@mediatek.com |
| James Yee | MediaTek |  |  | james.yee@mediatek.com |

Abstract

This document provides resolution for the following CIDs:

4542, 4545,4053,4016,4457,4990,4464,4459,4460

The comments are based on D2.0.

Edits for the proposed resolutions are based on D2.0.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4542 | 9.31.5 | 128.61 | 61 | What does "has the value true for dot11VHTSUBeamformerActivated." mean? Is it just that the value of this variable is true? | Replace "that has the value true for dot11VHTSUBeamformerActivated." with "whose attribute dot11VHTSUBeamformerActivated is true.", same for the Beamformee statement on lines 63 and 64, and also for the similar statements on page 129. |

**Discussion:**

Agree with the comment.

**Proposed Response:**

Accepted the proposed text changes.

**Proposed Resolution Text:**

[128.61- 63] A STA ~~that has the value true for dot11VHTSUBeamformerActivated~~ shall set the SU Beamformer Capable field to 1 in transmitted VHT Capabilities elements. A STA ~~that has the value true for dot11VHTSUBeamformeeActivated~~ **whose attribute dot11VHTSUBeamformerActivated is true** shall set the SU Beamformee Capable field to 1 in transmitted VHT Capabilities elements.

[129.1- 3] A STA ~~that has the value true for dot11VHTMUBeamformerActivated~~ ~~dot11VHTSUBeamformeeActivated~~ **whose attribute dot11VHTSUBeamformerActivated is true**  shall set the MU Beamformer Capable field to 1 in transmitted VHT Capabilities elements. A STA ~~that has the value true for~~ ~~dot11VHTMUBeamformeeActivated~~ **whose attribute dot11VHTSUBeamformerActivated is true** shall set the MU Beamformee Capable field to 1 in transmitted VHT Capabilities elements.

[129.9 - 12] A STA ~~that has the value true for dot11VHTMUBeamformerActivated~~ **whose attribute dot11VHTSUBeamformerActivated is true**  shall set the value of dot11VHTSUBeamformerActivated to true.

~~A STA that has the value true for dot11VHTMUBeamformeeActivated shall set the value of dot11VHTSUBeamformeeActivated to true.~~

……

[129.25- 28] A STA ~~that does not have the value true for dot11VHTSUBeamformerActivated~~ **whose attribute dot11VHTSUBeamformerActivated is not true**

shall not act in the role of a

beamformer. A STA that does not have the value true for dot11VHTSUBeamformeeActivated shall not act

in the role of a beamformee.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4545 | 9.31.5 | 131.08 | 8 | What does "has the value true for dot11VHTSUBeamformeeActivated." mean? Is it just that the value of this variable is true? | Replace "unless it has the value true for dot11VHTSUBeamformeeActivated." with "unless its attribute dot11VHTSUBeamformeeActivated is true." |

**Discussion:**

Agree with the comment.

**Proposed Response:**

Accepted the proposed text changes.

**Proposed Resolution Text:**

A STA shall ignore received NDPA, VHT NDP, and Beamforming Report Poll frames ~~unless it has the value true for dot11VHTSUBeamformeeActivated~~. unless its attribute dot11VHTSUBeamformeeActivated is true.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4053 | 9.3.2.7.1 | 93.54 | 4 | Dual CTS Protection is an HT feature that is intended to extend range, not increase throughput.  It has not proven to be a useful feature of .11n (based on its lack of support in the market). It makes even less sense in the context of .11ac.  However, there is no statement as to whether it is supportable in .11ac, and certainly no attempt to make it work. This is best handled by disallowing the use of Dual CTS Protection in a VHT BSS. | At 9.3.2.7.1 add the following at the beginning:  "Dual CTS is a mechanism that might be enabled by an HT AP that is not a VHT AP in an HT BSS. A VHT AP shall not transmit an HT Operation Element with the Dual CTS Protection field equal to 1." |

**Discussion:**

Agree with the proposed change.

Upon checking the specification, there is no section 9.3.2.7.1 in D 2.0.

But in D 2.1, the followng section is added.

“9.3.2.7.1 Dual CTS protection procedure

Insert as the first paragraph of 9.3.2.7.1:

A VHT STA shall not transmit VHT PPDUs in a TXOP protected by dual CTS protection.(#4372)

“

**Proposed Response:**

Duplicate - CID #4372

**Proposed Resolution Text:**

N/A

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4016 | 6.3.3.3.2 | 10.35 | 35 | "The STA that is creating the BSS shall be able to receive and transmit at each of the MCS values listed in the set."  Clause 6 (widely ignored) is not a good place to bury normative requirements. | Move text to Clause 10 somewhere.  Ditto at 10.44. Ditto at 11.18. |

**Discussion:**

Agree with the comment and will revise the test accordingly.

**Proposed Response:**

Accepted

**Proposed Resolution Text:**

[10.35]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| VHTBasicMCSSet | Set of integers | As defined for the VHT Basic MCS Setfield in 8.4.2.161 (VHT Operation element) | The MCS values for each number of spatial streams that must be supported by all VHTSTAs that join this BSS. ~~The STA that is creating the BSS shall be able to receive and transmit at each of the MCS values listed in the set.~~ | Adopt |

[10.44]

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| VHTOperationalMCSSet | Set of integers | As defined for the VHT Basic MCS Set field in 8.4.2.161 (VHT Operation element) | The MCS values for each number of spatial streams that the peer STA desires to use for communication within the BSS.  ~~The STA shall be able to receive at each of the data rates listed in the set. This values are a superset of those contained in the VHTBSSBasicMCSSet parameter~~. | Do not adopt |

[11.18]

|  |  |  |  |
| --- | --- | --- | --- |
| VHTOperationalMCSSett | Set of integers | As defined for the VHT Basic MCS Set field in 8.4.2.161 (VHT Operation element) | The MCS values for each number of spatial streams that the peer STA desires to use for communication within the BSS. ~~The STA shall be able to receive at each of the data rates listed in the set.~~  This values are a superset of those contained in the VHTBSSBasicMCSSet parameter. |

*Instruction to the editor: Insert the following text in to section 10.38.1, Basic VHT BSS Functionality*

The STA that is creating the BSS shall be able to receive and transmit at each of the MCS values listed in the set

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4457 | 10.22.6.4.3 | 139.35 | 35 | Channel selection should also take into account channel usage procedures as defined in 10.23.14 in the baseline | Add a reference to these additional hints |

**Discussion:**

The suggestion improves the readability of the specification.

**Proposed Response:**

Agree

**Proposed Resolution Text:**

If a TDLS peer STA chooses to start a wideband direct link, it shall follow the primary channel selection rules as defined in 10.38.2 (Channel selection methods for a VHT BSS) and 10.23.14 (Channel usage procedures) described in IEEE Std 802-11 2012.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4990 | 10.38.3 | 143.04 | 4 | Clause 10.38.3 Scanning requirements for VHT STA starts "An OBSS scan operation is a passive or active scan of a set of channels that are potentially affected by VHT BSS operation." In radar bands, it is extremely likely that active scan is prohibited. In radar bands, it is becoming very likely that initial Channel Availability Check will include adjacent channels. It is entirely appropriate for 10.38.3 VHT BSS operation to begin with meeting regulatory requirements, then discuss OBSS scans. | Include a statement that in shared bands, unlicensed devices may have to meet regulatory initial Channel Availability Check requirements. You should explicitly say [REVmb 10.1.4.1 General] "Active scanning is prohibited in some frequency bands and regulatory domains." |

**Discussion:**

The suggestion improves the readability of the specification.

**Proposed Response:**

Agree

**Proposed Resolution Text:**

[143.04]

An OBSS scan operation is a passive or active scan of a set of channels that are potentially affected by VHT BSS operation. “Active scanning is prohibited in some frequency bands and regulatory domains. The MAC of a STA receiving an MLME-SCAN.request primitive shall use the regulatory domain information it has to process the request and shall return a result code of NOT\_SUPPORTED to a request for any active scan if regulatory domain information indicates an active scan is illegal.” (REVmb D12.0 10.1.4.1)

Each channel in the set may be scanned more than once during a single OBSS scan operation.

OBSS scans are performed by STAs that start a VHT BSS.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4464 | 10.38.2 | 142.65 | 65 | The baseline usage of "channel set" differs than the usage here | Replace simply by "channel" which, without modifiers, traditionally signifies the whole 20/40/80/160/80+80 MHz |

**Discussion:**

The suggestion improves the readability of the specification.

**Proposed Response:**

Agree

**Proposed Resolution Text:**

[142.65]

NOTE—An AP operating a VHT BSS with a 40 MHz, 80 MHz, 160 MHz or 80+80 MHz operating channel width, on detecting an OBSS whose primary channel is the AP's secondary 20 MHz channel, can switch to 20 MHz BSS operation and/or can move to a different channel ~~set~~.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4459 | 10.38.1 | 139.27 | 27 | ch width cap ... 80 or 80+80 or 160 MHz | "ch width cap ... up to 80, 160 or 80+80 MHz" or "max ch width cap ... 80, 160 or 80+80 MHz" |

**Discussion:**

The suggestion improves the readability of the specification.

**Proposed Response:**

Agree

**Proposed Resolution Text:**

TDLS peer STAs may transmit up to 40 MHz, 80 MHz, 160 MHz or 80+80 MHz PPDUs on a 40 MHz, 80 MHz, 160 MHz or 80+80 MHz direct link, respectively. A TDLS peer STA shall not transmit a 20 MHz PPDU in the non-primary channel of its 80 MHz, 160 MHz or 80+80 MHz direct link.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Line** | **Comment** | **Proposed Changes** |
| 4460 | 10.38.1 | 140.56 | 56 | "not transmit a X MHz PPDU" is too broad - e.g. VHT probe requests may be sent on any 20 MHz channel | "not transmit a X MHz PPDU within its BSS". Repeat for P140L56/L64, P141L2/L9. ALso, it might be possible to compress all these paras |

**Discussion:**

The commentors is correct in point out that A VVHT STA may be probe request on any 20MHz channel when performing active scan. But the text in the specification already makes it clear that the limitation is for the BSS only.

“A VHT STA that is a member of a VHT BSS shall not transmit a 20 MHz VHT PPDU on a channel other than the primary 20 MHz channel **of the BSS**, except for a 20 MHz VHT PPDU transmission on an offchannel TDLS direct link.”

**Proposed Response:**

Reject

**Proposed Resolution Text:**

N/A.