IEEE P802.11
Wireless LANs

|  |
| --- |
| [place document subject title text here] |
| Date: 2012-05-14 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Osama Aboul-Magd | Huawei Technologies | 303 Terry Fox DriveOttawa, ONT, Canada | 613-287-1405 | Osama.aboulmagd@huawei.com |
|  |  |  |  |  |

Abstract

This submission includes proposed Resolutions to CIDs 4856, 4857, and 4859.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4856 | 304.00 | B.4.23.1 |  | AP and non-AP are swapped | For VHTM1.2 and 1.3, put CF2 in the former and CF1 in the latter |

Context:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| VHTM1.2 | Signaling of STA capabilities in Probe Request, (Re)Association Request frames | 8.4.2.94 (VHT Capabilities element (11ac)), 8.3.3.9 (Probe Request frame format), 8.3.3.5 (Association Request frame format), 8.3.3.7 (Reassociation Request frame format) | CFac and CF1:M | Yes  No  N/A  |

Discussion: Commenter is right. CF1 (AP) and CF2 (independent Station) are misplaced.

Proposed Resolution: Accept

Proposed changes: as in comment.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4857 |  | B |  | Inconsistent Booleans | Use "AND" throughout (not "and"), and don't use parentheses where not necessary (e.g. 304.36) |

Discussion: Commentor is correct. There is inconsistency in the use of “and” and “AND” in VHT PICS table.

Proposed Resolution: Accept

Instruct the Editor to replce “and” with “AND” in VHT PICS tables.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 4859 | 305.46 | B.4.23.1 |  | BFee requires BFee | Change VHTM4.1 to VHTM4.2 |

Proposed Resolution: Revised

Proposed Changes: see proposed changes to CIDs 4860 and 4861 in doc 11-12/0521r1.**References:**