IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TGac SB 01 Comment Resolution – Jonathan | | | | |
| Date: 2013-05-14 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jonathan Segev | Intel | 94 Em Hamoshavot rd. PTK, Israel | +972-54-2403587 | [jonathan.segev@intel.com](mailto:jonathan.segev@intel.com) |
|  |  |  |  |  |

Abstract

This submission included proposed resolutions to CIDs 10203, 10295.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 10203 | 139.32 | 9.7.11.1 | Rx VHT-MCS Map is a subfield, not a field. | Please replace "Rx VHT-MCS Map field" with "Rx VHT-MCS Map subfield". | Prposed Resolution: Revise. The Rx VHT-MCS Map is a subfield defined in 8.4.2.160.3 under the Supported VHT MCS and NSS set fields Replace Rx VHT MCS Map Field with subfield.  15.11, 100.61,139.31, 187.51. |

**Discussion:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 10295 | 127.54 | 9.3.7 | This NOTE ("In Figure 9-14, ... , referenced from the end of the last symbol of a PPDU on the medium.") is not a sentence. In addition, there is no "D1" in that figure, nor in the rest of the draft. | Either create a sentence that is a complete statement (probably without 'D1') or delete the whole note on lines 54 and 55. | Revise.  Rephrase the the note in line 54 to read: "Note - In Figure 9-14, when transmitting a VHT PPDU, D1 is equal to aRxPHYDelay and referenced from the end of the last symbol of a PPDU on the medium.".  That way it is consistent with D1 definition of 802.11-2012 in figure 9-14.  Removal of the sentence will be a technical change as D1 value for non VHT is aRxRFDelay+ aRxPLCPDelay. |

**Discussion:**