IEEE P802.11
Wireless LANs

|  |
| --- |
| Comment Resolution for Clause 6.3 |
| Date: 2013-06-06 |
| Author: |
| Name | Affiliation | Address | Phone | Email |
| Edward Au | Huawei Technologies | 303 Terry Fox Drive, Suite 400, K2K 3J1 Kanata Ontario  |  | edward.au@huawei.com |

##### This submission presents proposed resolution to CIDs 10220, 10147, 10221, 10222, 10189, 10223, and 10169. Changes indicated by a mixture of Word track-changes and instructions.

##### CID 10220

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10200 | 6.3.3.3.2 | 14 | 21 | The new VHT parameters need to be added to the parameter list, also | Add "VHT Capabilities, VHT Operation" to the parameter list to MLME-SCAN.confirm |

***Discussion:***

As referred to clause 6.3.3.3.2 (Semantics of the service primitives) in IEEE802.11-2012 (c.f., pages 109-114), the primitive parameters (or the parameter list the commenter mentions) are as follows:

MLME-SCAN.confirm(

 BSSDescriptionSet,

 BSSDescriptionFormMeasurementPilotSet,

 ResultCode,

 VendorSpecificInfo

 }

in which BSSDescriptionSet consists of elements such as HT Capabilities and HT Operation. The following shows a snapshot of portions of elements contained in BSSDescriptionSet.

 

As indiciated in page 14 of P802.11ac\_D5.0, VHT Capabilities and VHT Operation will be inserted “at the end of the second table”, in which the table refers to the elements of BSSDescriptionSet. The following shows the snapshot of the text.



***Proposed Resolution:***

**Rejected.** Given VHT Capabilities and VHT Option are included in BSSDescriptionSet, these two parameters are not required to be added to the parameter list of MLME-SCAN.confirm.

##### CID 10147

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10147 | 6.3.4.2.2 | 15 | 7 | Shouldn't the OperationalVHTMCS\_NSSSet be a super set of the values contained in the BSSBasicVHTMCS\_NSSSet parameter? | Add the description that this set is a superset of the <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter. |

***Discussion:***

As referred to clause 6.3.4.2.2 (Semantics of the service primitive) in IEEE802.11-2012 (c.f., page 116), both the OperationalRateSet and the HTOperationalMCSSet are explicitly described as a superset of the rates contained in the BSSBasicRateSet parameter and a superset of the MCS values in the BSSBasicMCSSet parameter, respectively. See the following snapshot for reference.



Referring to P802.11ac\_D5.0, BSSBasicVHTMCS\_NSSSet is defined as the set of MCS and number of spatial stream tuples (i.e., the set of <VHT-MCS, NSS> tuples) that are supported by all VHT STAs that are members of a VHT BSS, while OperationalVHTMCS\_NSSSet is the set of <VHT-MCS, NSS> tuples constrained so that the MCS values are expressible using the encoding described for the Supported VHT-MCS and NSS Set field. The comment is correct that OperationalVHTMCS\_NSSSet is a superset of the <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter but it is not explicitly stated in the following table in clause 6.3.4.2:



***Proposed Resolution:***

**Accepted.**

### TGac Editor: Please add the following sentence right after the first paragraph of description in line 7 of page 15:

The VHT-MCS values for each number of spatial streams that the STA desires to use for communication within the BSS. This set is a superset of the <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter.

##### CID 10221

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10221 | 6.3.7.5.2 | 18 | 23 | The VHT Capabilities here are what the AP supports | Change "STA" to "AP" in the description of the VHT Capabilities parameter in the MLME-ASSOCIATE.response |

***Discussion:***

As referred to clause 6.3.7.5 (MLME-ASSOCIATE.response) in IEEE802.11-2012 (c.f., page 130), MLME-ASSOCIATE.response primitive is sent by an AP as a response to an MLME-ASSOCIATE.indication primitive. The parameter VHT Capabilities in this primitive specifies the parameters within the VHT Capabilities element that are supported by the AP.

***Proposed Resolution:***

**Accepted.**

### TGac Editor: Please apply the following changes to line 24 of page 18 under the column “Description”:

Specifies the parameters in the VHT Capabilities element that are supported by the AP.

##### CID 10222

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10222 | 6.3.8.3.2 | 20 | 8 | The VHT Capabilities here are what the AP supports | Change "STA" to "AP" in the description of the VHT Capabilities parameter in the MLME-REASSOCIATE.confirm |

***Discussion:***

As referred to clause 6.3.8.3 (MLME-REASSOCIATE.confirm) in IEEE802.11-2012 (c.f., page 135), MLME-REASSOCIATE.confirm primitive is sent by an AP as a response to an MLME-REASSOCIATE.request primitive. The parameter VHT Capabilities in this primitive specifies the parameters within the VHT Capabilities element that are supported by the AP.

***Proposed Resolution:***

**Accepted.**

### TGac Editor: Please apply the following changes to line 8 of page 20 under the column “Description”:

Specifies the parameters in the VHT Capabilities element that are supported by the AP.

##### CID 10189

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10189 | 6.3.8.4.2 | 21 | 10 | Why is the VHT Capabilities Element present in the Association Request frame received from the STA? This subclause describes the MLME-REASSOCIATE.indication and I believe the VHT Capabilities Element be present in Reassociation Request frame received from the STA. | Please replace "Association Request frame" with "Reassociation Request frame" in the description. |

***Discussion:***

As referred to Clause 6.3.8 (Reassociate) in page 18 of P802.11ac\_D5.0, the discussion is related to reassociation, rather than association.

***Proposed Resolution:***

**Accepted.**

### TGac Editor: Please apply the following changes to line 10 of page 21 under the column “Description”:

The parameter is present if dot11VHTOptionImplemented is true and the VHT Capabilities element is present in the Reassociation Request frame received from the STA, and not present otherwise.

##### CID 10223

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10223 | 6.3.8.5.2 | 21 | 63 | The VHT Capabilities here are what the AP supports | Change "STA" to "AP" in the description of the VHT Capabilities parameter in the MLME-REASSOCIATE.response |

***Discussion:***

As referred to clause 6.3.8.5 (MLME-REASSOCIATE.response) in IEEE802.11-2012 (c.f., page 141), MLME-REASSOCIATE.response primitive is sent by an AP as a response to an MLME-REASSOCIATE.indication primitive. The parameter VHT Capabilities in this primitive specifies the parameters within the VHT Capabilities element that are supported by the AP.

***Proposed Resolution:***

**Accepted.**

### TGac Editor: Please apply the following changes to line 63 of page 21 under the column “Description”:

Specifies the parameters in the VHT Capabilities element that are supported by the AP.

##### CID 10169

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 10169 | 6.3.11.2.4 | / | / | The baseline describes the restriction of the ResultCode parameter in the resulting MLME-START.confirm primitive when there are unsupported rates or unsupported MCSs. There should be a similar restriction when there are any unsupported <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter. | Add a similar description referring to the third paragraph in 6.3.11.2.4 of IEEE Std 802.11-2012. |

***Discussion:***

In P802.11ac\_D5.0, clause 6.3.11.2.4 is cited by clause 9.3.1 (General) related to DCF:



In IEEE802.11-2012, however, BSSBasicVHTMCS\_NSSSet is not mentioned in clause 6.3.11.2.4 (c.f., page 151). In other words, the commenter is correct that a description is missing on a restriction when there are any unsupported <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter in this clause.



There are additional problems related to this comment, however.

As referred to clause 6.3.11.2 (MLME-START.request) in P802.11ac\_D5.0 (c.f., page 22), both the BSSBasicVHTMCS\_NSSSet parameter and the OperationalVHTMCS\_NSSSet parameter are missing in the MLME-START.request primitive:

MLME-START.request(

 SSID,

 SSIDEncoding,

 BSSType,

 BeaconPeriod,

 DTIMPeriod,

 CF parameter set,

 PHY parameter set,

 IBSS parameter set,

 ProbeDelay,

 CapabilityInformation,

 BSSBasicRateSet,

 OperationalRateSet,

 Country,

 IBSS DFS Recovery Interval,

 EDCAParameterSet,

 DESRegisteredLocation,

 HT Capabilities,

 HT Operation,

 BSSMembershipSelectorSet,

 BSSBasicMCSSet,

 HTOperationalMCSSet,

 Extended Capabilities,

 20/40 BSS Coexistence,

 Overlapping BSS Scan Parameters,

 MultipleBSSID,

 InterworkingInfo,

 AdvertisementProtocolInfo,

 RoamingConsortiumInfo,

 Mesh ID,

 Mesh Configuration,

 QMFPolicy,

 DMG Capabilities,

 Multi-band,

 Multiple MAC Addresses,

 DMG Operation,

 Clustering Control,

 CBAP Only.

 PCP Association Ready,

 VHT Capabilities,

 VHT Operation,

 VendorSpecificInfo

 )

Without BSSBasicVHTMCS\_NSSSet parameter and OperationalVHTMCS\_NSSSet parameter in the MLME-START.request primitive, any change to the clause 6.3.11.2.4 is meaningless.

Further, as referred to clause 6.3.4.2.4 (Effect of receipt) for MLME-JOIN.request primitive (c.f., pages 116-117), BSSBasicVHTMCS\_NSSSet is not mentioned. In other words, it is similar to the clause 6.3.11.2.4 that a description is missing on a restriction when there are any unsupported <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter in this clause:





Lastly, there is a parameter, SelectedBSS, in the MLME-JOIN.request primitive:

MLME-JOIN.request(

 SelectedBSS,

 JoinFailureTimeout,

 ProbeDelay,

 OperationalRateSet,

 HTOperationalMCSSet,

 OperationalVHTMCS\_NSSSet,

 VendorSpecificInfo

 )

It contains a number of parameters including BSSDescription (c.f., pages 109-114 of IEEE802.11-2012), which further consists of parameters, such as BSSBasicRateSet, OperationalRateSet, BSSBasicMCSSet, and HTOperationalMCSSet. Similar to the previous two clauses, both the BSSBasicVHTMCS\_NSSSet parameter and the OperationalVHTMCS\_NSSSet parameter are missing here.

***Proposed Resolution:***

**Counter.**

### TGac Editor: Please apply the following changes to Clause 6.3.11.2.2 in page 22 related to MLME-START.request primitive:

MLME-START.request(

 SSID,

 SSIDEncoding,

 BSSType,

 BeaconPeriod,

 DTIMPeriod,

 CF parameter set,

 PHY parameter set,

 IBSS parameter set,

 ProbeDelay,

 CapabilityInformation,

 BSSBasicRateSet,

 OperationalRateSet,

 Country,

 IBSS DFS Recovery Interval,

 EDCAParameterSet,

 DESRegisteredLocation,

 HT Capabilities,

 HT Operation,

 BSSMembershipSelectorSet,

 BSSBasicMCSSet,

 HTOperationalMCSSet,

 Extended Capabilities,

 20/40 BSS Coexistence,

 Overlapping BSS Scan Parameters,

 MultipleBSSID,

 InterworkingInfo,

 AdvertisementProtocolInfo,

 RoamingConsortiumInfo,

 Mesh ID,

 Mesh Configuration,

 QMFPolicy,

 DMG Capabilities,

 Multi-band,

 Multiple MAC Addresses,

 DMG Operation,

 Clustering Control,

 CBAP Only.

 PCP Association Ready,

 VHT Capabilities,

 VHT Operation,

 BSSBasicVHTMCS\_NSSSet,

 OperationalVHTMCS\_NSSSet,

 VendorSpecificInfo

 )

### TGac Editor: Please add the following entries to the table in page 23 related to MLME-START.request primitive:

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

### TGac Editor: Please add the following in page 23 related to MLME-START.request primitive:

6.3.11.2.4 Effect of receipt

*Insert as the second last paragraph:*

If the MLME of a VHT STA receives an MLME-START.request primitive with a BSSBasicVHTMCS\_NSSSet parameter containing any unsupported <VHT-MCS, NSS> tuple, the MLME response in the resulting MLME-START.confirm primitive shall contain a ResultCode parameter that is not set to the value SUCCESS.

### TGac Editor: Please add the following in page 15 related to MLME-JOIN.request primitive:

6.3.4.2.4 Effect of receipt

*Insert as the last paragraph:*

If the MLME of a VHT STA receives an MLME-JOIN.request primitive with the SelectedBSS parameter containing a BSSBasicVHTMCS\_NSSSet parameter that contains any unsupported <VHT-MCS, NSS> tuple, the MLME response in the resulting MLME-JOIN.confirm primitive shall contain a ResultCode parameter that is not set to the value SUCCESS.

### TGac Editor: Please add the following in page 14 related to MLME-JOIN.request and MLME-SCAN.confirm primitives:

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Type | Valid Range | Description |
| BSSBasicVHTMCS\_NSSSet | Set of <VHT-MCS, NSS> tuples | As defined in 8.4.2.160 | The set of MCS and NSS tuples that shall be supported by all VHT STAs to join a VHT BSS. The STA that is creating the BSS shall be able to receive and transmit at each of the MCS and NSS tuples listed in the set. |
| OperationalVHTMCS\_NSSSet | Set of <VHT-MCS, NSS> tuples, constrained so that the MCS values are expressible using the encoding described for the Supported VHT-MCS and NSS Set field in 8.4.2.160.3 (Supported VHT-MCS and NSS Set field) | As defined in the Rx VHT-MCS Map and Rx Highest Supported Long GI Data Rate fields in the Supported VHT-MCS and NSS Set field in 8.4.2.160.3 (Supported VHT-MCS and NSS Set field) | The VHT-MCS values for each number of spatial streams that the STA desires to use for communication within the BSS. This set is a superset of the <VHT-MCS, NSS> tuples contained in the BSSBasicVHTMCS\_NSSSet parameter.The parameter is present if dot11VeryHighThroughoutOptionImplemented is true, and not present otherwise. |