IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Collection 09 MAC CIDs (Comment Resolutions for CC09) | | | | |
| Date: 2013-MM-DD | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Young Hoon Kwon | Huawei |  |  | Younghoon.kwon@huawei.com |
|  |  |  |  |  |

Abstract

This document provides resolutions for CIDs: 513, 514, 714, and 715.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CIDs | Clause | Page | Line | Comment | Proposed change | Resolution |
| 513 | 8.5.23a.5 | 112 | 42 | (If Relay function is not removed) A term "relay station" shall be "Relay". | Replace "relay station" by "Relay". | Revised – Based on definition in 9.32n Relay operation, the entity that sends STA Information Announcement frame to the root AP is a Relay STA. Therefore, replace “relay station” to “Relay STA”. |
| 514 | 9.32n.3.2 | 161 | 18 | (If Relay function is not removed) A term "relay station" shall be "Relay". | Replace "relay station" by "Relay". | Accepted as proposed |
| 714 | 9.32n.3.2 | 161 | 34 | typographical error: "a AP" | an AP | Accepted as proposed. |
| 715 | 9.32n.3.2 | 161 | 46 | redundant text. | change the sentence in line 46 page 161 to the following text: For downlink implicit ACK procedure, an AP that the relay is associated with shall know PAID of STAs associated with a relay station. | Accepted as proposed. |