IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolution for Subclause 10.1.4.2 | | | | |
| Date: 2013-09-12 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yuan Zhou | I2R | 1 Fusionopolis Way, Connexis South Tower, Singapore 138632 | +65 6408 2472 | yzhou@i2r.a-star.edu.sg |
| Zander Lei | I2R | 1 Fusionopolis Way, Connexis South Tower, Singapore 138632 |  |  |

Abstract

This document provides resolutions for CID 717.

The changes are in the following subclauses: 10.1.4.2

Table of Contents

[0 Revision Notes 2](#_Toc354045214)

# 0 Revision Notes

R0: First draft

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Comment** | **Page Number** | **Subclause** | **Line Number** | **Proposed Changes** | **Proposed Resolution** |
| 717 | The Passive Scanning section requires more detail to describe the passive scanning using short beacon. | 167 | 10.1.4.2 |  | Add detail to describe passive scanning which uses a short beacon first, then scans the full beacon according to the information received in the short beacon to obtain information not received in short beacon. | **Rejected** |

**Discussion:**

The passive scanning section in the current specification does not exclude passive scanning based on short beacon. If the ScanType parameter indicates a passive scan, the STA shall still listen to each channel scanned for no longer than a maximum duration defined by the MaxChannelTime parameter, as specified in the current standard.