IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolutions for Clause 8.2.4 | | | | |
| Date: 2014-12-02 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Liwen Chu | Marvell |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes comment resolutions for subclauses under 8.2.4:

5130, 5131, 5132, 5242, 5243, and 5061***.***

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGah Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGah Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGah Editor: Editing instructions preceded by “TGah Editor” are instructions to the TGah editor to modify existing material in the TGah draft. As a result of adopting the changes, the TGah editor will execute the instructions rather than copy them to the TGah Draft.***

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Num** | **P** | **L** | **Comment** | **Propose Change** | | **Resolution** |
| 5130 | 8.2.4.1.1 | 72 | 19 | "a S1G" should be "an S1G" | | "a S1G" should be "an S1G" | Accept |
| 5131 | 8.2.4.1.1 | 72 | 38 | "a S1G" should be "an S1G" | | "a S1G" should be "an S1G" | Accept |
| 5132 | 8.2.4.1.1 | 72 | 56 | "a S1G" should be "an S1G" | | "a S1G" should be "an S1G" | Accept |
| 5242 | 8.2.4.1.1 | 73 | 30 | The fields contained in the frame control field should be described in independent subclauses of 8.2.4.1 to be inline with the baseline. | | Add new subclauses 8.2.4.1.15 (Next TBTT Present field), 8.2.4.1.16 (Compressed SSID Present field), 8.2.4.1.17 (ANO Present field), 8.2.4.1.18 (BSS BW field), 8.2.4.1.19 (Security field), and 8.2.4.1.20 (AP PM field). Move each of the sentence descriptions of these fields (starting from P73L30 till P74L19) to their corresponding subclause that is newly created. | Accept |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Num** | **P** | **L** | **Comment** | **Propose Change** | **Resolution** |
| 5243 | 8.2.4.1.8 | 76 | 31 | Any relation between the More Data field and the eventually present EOSP field of the frame, or say the type of frame carrying this field? For sure it needs to be clear that this paragraph refers to individually addressed frames while the paragraph below for the case of the MD setting for group addressed frames (by the way the case of non-AP STA is missing). | As in comment and:    Insert "in individually addressed frames" immediately after "More Data field to 1" (twice) in this paragraph.    Insert " An S1G non-AP STA sets the More Data field to 0 in group addressed frames it transmits." at the end of the last paragraph. | Revise  Discussion: Adding “in individually addressed frames” in P76L31 paragraph makes sense. However It is not necessary to insert " An S1G non-AP STA sets the More Data field to 0 in group addressed frames it transmits." at the end of the last paragraph since an S1G non-AP STA will never transmit group addressed frames (for frames with multicast/broadcast destination MAC address, a non-AP STA use unicast MAC address as R1 address).  TGah editor inserts "in individually addressed frames" immediately after "More Data field to 1" (twice) in this paragraph. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Num** | **P** | **L** | **Comment** | **Propose Change** | **Resolution** |
| 5061 | 8.2.4.6.3 | 79 | 54 | "The S1G subfield is set to 1 by an S1G STA and is set to 0 by a non-S1G STA" --- "is set to" is usually only used to emphasize the act of changing / setting the field from one value to another. Here, the statement describes the value of the S1G subfield if the frame is transmissted by S1G STAs. | Change "The S1G subfield is set to 1 by an S1G STA and is set to 0 by a non-S1G STA" to "For S1G STAs, the S1G subfield equals 1. For non-S1G STAs, the S1G subfield equals 0." | Reject.  Discussion: “xxx field is set to yyy” is widely used in clause 8 of 11mc draft. |