IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution CID 10569 |
| Date: 2015-10-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Santosh Abraham | Qualcomm | 5775 Morehouse Dr. San Diego, CA 92121 | +1-858 651 6107 | sabraham@qti.qualcomm.com |
|  |  |  |  |  |

Abstract

This submission addresses CIDs 10569

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Comment | Proposed Change | Proposed Resolution |
| 10569 | "If the STA does not receive the FILS Container frame containing an IP assignment within the IP address request timeout period, then the STA may initiate an IP address assignment procedure using mechanisms that are out of scope of this specifica- tion." ---- what happens if the STA initiates an IP address assignment using other mechanisms, gets an IP, and the AP assigns afterwards a (different) IP address? | Insert a clarifying sentence to address the issue | Accept: Clarifying sentence added as given below. |

***Instruct the editor to modify section 10.47.3.3 as indicated:***

* + - 1. **FILS IP address configuration**

***Modify Paragraph in lines 50 – 60 of page 123 as follows:***

* If the AP needs more time to assign an IP address, then the AP sets the IP address assignment pending flag in the IP Address Response Control field of the FILS IP Address Assignment element to 1 and sets the IP address request timeout to the maximum estimated time in the unit of seconds within which it (AP) tries to assign an IP address to the requesting STA in FILS Container frame. When the AP is ready with an IP address within IP address request timeout period, then AP shall send the IP address to the STA using FILS Container frame. If the STA does not receive the FILS Container frame containing an IP assignment within the IP address request timeout period, then the STA may initiate an IP address assignment procedure using mechanisms that are out of scope of this specification. If an STA has initiated an IP address assighment procedure (using mechanisms that are out of scope) due to the expiry of the timeout peried, and subsequents receives an FILS container frame containing an IP assighment, it shall discard the IP address assignment received through the FILS container frame.