IEEE P802.11  
Wireless LANs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Mandatory Max Channel Time in Probe Request | | | | | |
| Date: 2016-01-20 | | | | | |
| Author(s): | | | | | |
| Name | Company | Address | Phone | email |
| Peter Khoury | Ruckus Wireless | 350 West Java Drive,  Sunnyvale, CA 94089, USA | +1 415 517-8715 | peter.khoury@ruckuswireless.com |

Abstract

This document makes mandatory for FILS stations the inclusion of MaxChannelTime in FILS Request Parameters in a probe request frame. It makes optional the use of the FILS Request Parameters field to communicate Max Channel Time in a probe request for non FILS STAs.

This document uses Draft P802.11ai\_D6.3.pdf as a baseline.

***Modify the table in the following clause:***

* + - 1. Probe Request frame format

|  |  |  |
| --- | --- | --- |
| Table 8-33 Probe Request frame body | | |
| Order | Information | Notes |
| 18 | FILS Request Parameters | The FILS Request Parameters element is optionally present if dot11FILSActivated is true. Optionally the FILS Request Parameters element may be used to communicate Max Channel Time and only the Max Channel Time if dot11FILSActivated is false. |
| 19 | AP-CSN | The AP-CSN element is optionally present if dot11- FILSActivated is true; otherwise not present. |

***Modify and add the following paragraphs in the following subclause:***

* + - * 1. Active scanning procedure for a non-DMG STA

A FILS STA **shall** indicate its MaxChannelTime in the Max Channel Time field of the FILS Request Parameters element of the Probe Request frame to prevent the responding STA from transmitting the Probe response after the time indicated by the MaxChannelTime has elapsed.

Optionally a STA that is not a FILS STA may indicate its MaxChannelTime using the Max Channel Time field of the FILS Request Parameters element of the Probe Request frame to prevent the responding STA from transmitting the Probe response after the time indicated by the MaxChannelTime has elapsed.