IEEE P802.11  
Wireless LANs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Trigger Frame Format** | | | | | |
| **Date:** 2016-03-14 | | | | | |
| **Author(s):** | | | | | |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Simone Merlin | Qualcomm | 5775 Morehouse Dr. San Diego, CA, USA |  | [smerlin@qti.qualcomm.com](mailto:smerlin@qti.qualcomm.com) |
| Albert Van Zelst | Straatweg 66-S Breukelen, 3621 BR Netherlands |  | allert@qti.qualcomm.com |
| Alfred Asterjadhi | 5775 Morehouse Dr. San Diego, CA, USA |  | aasterja@qti.qualcomm.com |
| Arjun Bharadwaj | 5775 Morehouse Dr. San Diego, CA, USA |  | arjunb@qti.qualcomm.com |
| Bin Tian | 5775 Morehouse Dr. San Diego, CA, USA |  | btian@qti.qualcomm.com |
| Carlos Aldana | 1700 Technology Drive San Jose, CA 95110, USA |  | caldana@qca.qualcomm.com |
| George Cherian | 5775 Morehouse Dr. San Diego, CA, USA |  | gcherian@qti.qualcomm.com |
| Gwendolyn Barriac | 5775 Morehouse Dr. San Diego, CA, USA |  | gbarriac@qti.qualcomm.com |
| Hemanth Sampath | 5775 Morehouse Dr. San Diego, CA, USA |  | hsampath@qti.qualcomm.com |
| Lin Yang | 5775 Morehouse Dr. San Diego, CA, USA |  | linyang@qti.qualcomm.com |
| Menzo Wentink | Straatweg 66-S Breukelen, 3621 BR Netherlands |  | mwentink@qti.qualcomm.com |
| Naveen Kakani | 2100 Lakeside Boulevard Suite 475, Richardson TX 75082, USA |  | nkakani@qti.qualcomm.com |
| Raja Banerjea | 1060 Rincon Circle San Jose CA 95131, USA |  | rajab@qit.qualcomm.com |
| Richard Van Nee | Straatweg 66-S Breukelen, 3621 BR Netherlands |  | rvannee@qti.qualcomm.com |
| Rolf De Vegt | 1700 Technology Drive San Jose, CA 95110, USA |  | rolfv@qca.qualcomm.com |
| Sameer Vermani | 5775 Morehouse Dr. San Diego, CA, USA |  | svverman@qti.qualcomm.com |
| Alice Chen | 5775 Morehouse Dr. San Diego, CA, USA |  | alicel@qti.qualcomm.com |
| Tao Tian | 5775 Morehouse Dr. San Diego, CA, USA |  | ttian@qti.qualcomm.com |
| Tevfik Yucek | 1700 Technology Drive San Jose, CA 95110, USA |  | tyucek@qca.qualcomm.com |
| VK Jones | 1700 Technology Drive San Jose, CA 95110, USA |  | vkjones@qca.qualcomm.com |
| Youhan Kim | 1700 Technology Drive San Jose, CA 95110, USA |  | youhank@qca.qualcomm.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Ron Porat | **Broadcom** |  |  | [**rporat@broadcom.com**](mailto:rporat@broadcom.com) |
| Sriram Venkateswaran |  |
| Matthew Fischer | mfischer@broadcom.com |
| Zhou Lan |  |
| Leo Montreuil |  |
| Andrew Blanksby |  |
| Vinko Erceg |  |
| Mingyue Ji |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Robert Stacey | Intel | 2111 NE 25th Ave, Hillsboro OR 97124, USA | +1-503-724-893 | robert.stacey@intel.com |
| Shahrnaz Azizi | shahrnaz.azizi@intel.com |
| Po-Kai Huang | po-kai.huang@intel.com |
| Qinghua Li | quinghua.li@intel.com |
| Xiaogang Chen | xiaogang.c.chen@intel.com |
| Chitto Ghosh | chittabrata.ghosh@intel.com |
| Laurent Cariou | laurent.cariou@intel.com |
| Yaron Alpert | yaron.alpert@intel.com |
| Assaf Gurevitz | assaf.gurevitz@intel.com |
| Ilan Sutskover | ilan.sutskover@intel.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Hongyuan Zhang** | **Marvell** | **5488 Marvell Lane, Santa Clara, CA, 95054** | **408-222-2500** | **hongyuan@marvell.com** |
| Yakun Sun | yakunsun@marvell.com |
| Lei Wang | Leileiw@marvell.com |
| Liwen Chu | liwenchu@marvell.com |
| Jinjing Jiang | jinjing@marvell.com |
| Yan Zhang | yzhang@marvell.com |
| Rui Cao | ruicao@marvell.com |
| Sudhir Srinivasa | sudhirs@marvell.com |
| Bo Yu | boyu@marvell.com |
| Saga Tamhane | sagar@marvell.com |
| Mao Yu | my@marvel..com |
| Xiayu Zheng | xzheng@marvell.com |
| Christian Berger | crberger@marvell.com |
| Niranjan Grandhe | ngrandhe@marvell.com |
| Hui-Ling Lou | hlou@marvell.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Jianhan Liu** | **Mediatek**  **USA** | **2860 Junction Ave, San Jose, CA 95134, USA** | **+1-408-526-1899** | **jianhan.Liu@mediatek.com** |
| Thomas Pare |  |  | thomas.pare@mediatek.com |
| ChaoChun Wang |  |  | chaochun.wang@mediatek.com |
| James Wang |  |  | james.wang@mediatek.com |
| ianyu Wu |  |  | tianyu.wu@mediatek.com |
| Russell Huang |  |  | russell.huang@mediatek.com |
| James Yee | Mediatek | No. 1 Dusing 1st Road, Hsinchu, Taiwan | +886-3-567-0766 | james.yee@mediatek.com |
| Alan Jauh |  |  | alan.jauh@mediatek.com |
| Frank Hsu |  |  | frank.hsu@mediatek.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Joonsuk Kim | Apple |  |  | [joonsuk@apple.com](mailto:joonsuk@apple.com) |
| Aon Mujtaba |  |  | [mujtaba@apple.com](mailto:mujtaba@apple.com) |
| Guoqing Li |  |  | [guoqing\_li@apple.com](mailto:guoqing_li@apple.com) |
| Eric Wong |  |  | [ericwong@apple.com](mailto:ericwong@apple.com) |
| Chris Hartman |  |  | [chartman@apple.com](mailto:chartman@apple.com) |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **David X. Yang** | **Huawei** | **F1-17, Huawei Base, Bantian, Shenzhen** |  | **david.yangxun@huawei.com** |
| Jiayin Zhang | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai | +86-18601656691 | zhangjiayin@huawei.com |
| Jun Luo | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | jun.l@huawei.com |
| Yi Luo | F1-17, Huawei Base, Bantian, Shenzhen | +86-18665891036 | Roy.luoyi@huawei.com |
| Yingpei Lin | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | linyingpei@huawei.com |
| Jiyong Pang | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | pangjiyong@huawei.com |
| Zhigang Rong | 10180 Telesis Court, Suite 365, San Diego, CA  92121 NA |  | zhigang.rong@huawei.com |
| Jian Yu | F1-17, Huawei Base, Bantian, Shenzhen |  | ross.yujian@huawei.com |
| Ming Gan | F1-17, Huawei Base, Bantian, Shenzhen |  | ming.gan@huawei.com |
| Yunsong Yang | 10180 Telesis Court, Suite 365, San Diego, CA  92121 NA |  | yangyunsong@huawei.com |
| Junghoon Suh | 303 Terry Fox, Suite 400 Kanata, Ottawa, Canada |  | Junghoon.Suh@huawei.com |
| Peter Loc |  |  | peterloc@iwirelesstech.com |
| Edward Au | 303 Terry Fox, Suite 400 Kanata, Ottawa, Canada |  | edward.ks.au@huawei.com |
| Teyan Chen | F1-17, Huawei Base, Bantian, Shenzhen |  | chenteyan@huawei.com |
| Yunbo Li | F1-17, Huawei Base, Bantian, Shenzhen |  | liyunbo@huawei.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Jinmin Kim** | **LG Electronics** | **19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea** |  | **Jinmin1230.kim@lge.com** |
| Kiseon Ryu |  | kiseon.ryu@lge.com |
| Jinyoung Chun |  | jiny.chun@lge.com |
| Jinsoo Choi |  | js.choi@lge.com |
| Jeongki Kim |  | jeongki.kim@lge.com |
| Dongguk Lim |  | dongguk.lim@lge.com |
| Suhwook Kim |  | suhwook.kim@lge.com |
| Eunsung Park |  | esung.park@lge.com |
| JayH Park |  | Hyunh.park@lge.com |
| HanGyu Cho |  | hg.cho@lge.com |
| Thomas Derham | Orange |  |  | thomas.derham@orange.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Bo Sun | ZTE | #9 Wuxingduan, Xifeng  Rd., Xi'an, China |  |  |
| Kaiying Lv |  |  | [lv.kaiying@zte.com.cn](mailto:lv.kaiying@zte.com.cn) |
| Yonggang Fang |  |  | [yfang@ztetx.com](mailto:yfang@ztetx.com) |
| Ke Yao |  |  | [yao.ke5@zte.com.cn](mailto:yao.ke5@zte.com.cn) |
| Weimin Xing |  |  | [xing.weimin@zte.com.cn](mailto:xing.weimin@zte.com.cn) |
| Brian Hart | Cisco Systems | 170 W Tasman Dr, San Jose, CA 95134 |  | [brianh@cisco.com](mailto:brianh@cisco.com) |
| Pooya Monajemi |  | [pmonajem@cisco.com](mailto:pmonajem@cisco.com) |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Fei Tong** | **Samsung** | **Innovation Park,  Cambridge CB4 0DS (U.K.)** | **+44 1223 434633** | **f.tong@samsung.com** |
| Hyunjeong Kang | Maetan 3-dong; Yongtong-Gu Suwon; South Korea | +82-31-279-9028 | hyunjeong.kang@samsung.com |
| Kaushik Josiam | 1301, E. Lookout Dr,  Richardson TX 75070 | (972) 761 7437 | k.josiam@samsung.com |
| Mark Rison | Innovation Park,  Cambridge CB4 0DS (U.K.) | +44 1223 434600 | m.rison@samsung.com |
| Rakesh Taori | 1301, E. Lookout Dr,  Richardson TX 75070 | (972) 761 7470 | rakesh.taori@samsung.com |
| Sanghyun Chang | Maetan 3-dong; Yongtong-Gu Suwon; South Korea | +82-10-8864-1751 | s29.chang@samsung.com |
| Yasushi Takatori | NTT | 1-1 Hikari-no-oka, Yokosuka, Kanagawa 239-0847 Japan | +81 46 859 3135 | takatori.yasushi@lab.ntt.co.jp |
| Yasuhiko Inoue | +81 46 859 5097 | inoue.yasuhiko@lab.ntt.co.jp |
| Shoko Shinohara | +81 46 859 5107 | Shinohara.shoko@lab.ntt.co.jp |
| Yusuke Asai | +81 46 859 3494 | asai.yusuke@lab.ntt.co.jp |
| Koichi Ishihara | +81 46 859 4233 | ishihara.koichi@lab.ntt.co.jp |
| Junichi Iwatani | +81 46 859 4222 | Iwatani.junichi@lab.ntt.co.jp |
| Akira Yamada | NTT DOCOMO | 3-6, Hikarinooka, Yokosuka-shi, Kanagawa, 239-8536, Japan | +81 46 840  3759 | yamadaakira@nttdocomo.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Masahito Mori** | **Sony Corp.** |  |  | **Masahito.Mori@jp.sony.com** |
| Yusuke Tanaka | YusukeC.Tanaka@jp.sony.com |
| Yuichi Morioka | Yuichi.Morioka@jp.sony.com |
| Kazuyuki Sakoda | Kazuyuki.Sakoda@am.sony.com |
| William Carney | William.Carney@am.sony.com |
| Tomoko Adachi | Toshiba |  |  | [tomo.adachi@toshiba.co.jp](mailto:tomo.adachi@toshiba.co.jp) |
| Narendar Madhavan | [narendar.madhavan@toshiba.co.jp](mailto:narendar.madhavan@toshiba.co.jp) |
| Kentaro Taniguchi | [kentaro.taniguchi@toshiba.co.jp](mailto:kentaro.taniguchi@toshiba.co.jp) |
| Toshihisa Nabetani | [toshihisa.nabetani@toshiba.co.jp](mailto:toshihisa.nabetani@toshiba.co.jp) |
| Tsuguhide Aoki | [tsuguhide.aoki@toshiba.co.jp](mailto:tsuguhide.aoki@toshiba.co.jp) |
| Koji Horisaki | [kouji.horisaki@toshiba.co.jp](mailto:kouji.horisaki@toshiba.co.jp) |
| David Halls | [david.halls@toshiba-trel.com](mailto:david.halls@toshiba-trel.com) |
| Filippo Tosato | [filippo.tosato@toshiba-trel.com](mailto:filippo.tosato@toshiba-trel.com) |
| Zubeir Bocus | [zubeir.bocus@toshiba-trel.com](mailto:zubeir.bocus@toshiba-trel.com) |
| Fengming Cao | [fengming.cao@toshiba-trel.com](mailto:fengming.cao@toshiba-trel.com) |
| Parag Kulkarni | parag.kulkarni@toshiba-trel.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Minho Cheong | Newracom, Inc. | 9008 Research Dr, Irvine, CA 92618 | +1-949-390-7146 | minho.cheong@newracom.com |
| Reza Hedayat |  |  | reza.hedayat@newracom.com |
| Young Hoon Kwon |  |  | younghoon.kwon@newracom.com |
| Yongho Seok |  |  | yongho.seok@newracom.com |
| Daewon Lee |  |  | daewon.lee@newracom.com |
| Yujin Noh |  |  | yujin.noh@newracom.com |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Sigurd Schelstraete | Quantenna | 3450 W. Warren Ave, Fremont, CA 94538 |  | Sigurd@quantenna.com |
| Huizhao Wang |  |  | hwang@quanetnna.com |

#### Trigger frame

The Trigger frame is used to allocate resource for UL MU transmission and to solicit an UL MU transmission at SIFS after the PPDU that carries the Trigger frame. The Trigger frame also carries other information required by the responding STA to send UL MU.

The frame format for the Trigger frame is as defined in Figure 9-51a (Trigger frame).

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Frame Control | Duration | RA | TA | Common Info | Per User Info | … | Per User Info | Padding | FCS |
| Octets: | 2 | 2 | 6 | 6 | TBD | TBD |  | TBD |  | 4 |

Figure 9‑51a - Trigger frame

The Duration/ID field is set as defined in 9.2.5 (Duration/ID field (QoS STA)).

The RA field of the Trigger frame is the address of the recipient STA.The TA field value is the address of the STA transmitting the Trigger frame.

The Common Info field is defined in Figure 9-51b.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | Length | Cascade Indication | CS Required | Spatial Reuse | BW | CP and LTF Type | MU MIMO LTF  Mode | # of LTFs |
| Bits: | 12 | 1 | 1 | >=2 | TBD | TBD | 1 | 3 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| STBC | LDPC  Extra Symbol | AP TX Power | Packet  Extension | Trigger Type | Type-dependent Common Info |
| 1 | 1 | TBD | >=3 | 4 | variable |

Figure 9‑51b - Common Info field

Discussion:

The prposed modifications consider fields corresponding to functionalities that are already in the SFD and, tentatively, fields corresponding to additional functionalities being proposed at this meeting.

* We sugget to preserve the RA in the frame, for consistency with existing leacy frame formats.
* Trigger frame is supposed to include indications that responsder STAs shall inclide in SIG-A, except for the info already known by the STA.
* MU MIMO LTF mode field indicates the mode in which pilots are allocated
* # of LTFs includes the total number of LTFs the STA must include in the response TRIG PPDU.
* STBC indicates whether STBS is used (for all STAs)
* LDPC extra symbol indicates, to the STAs for which LDPC is requestd, whether the encoding should be done accounting for an extra uncoded symbol at the end of the PPDU.
* AP TX power is used in relation to the power control protocol
* Packet Extension indicates the presence and the parameters for the PE. It includes at least alpha-factor and disambiguation bit
* We suggest to use 4 bits for trigger type

The Length subfield of the Common Info field indicates the value of the L-SIG Length field of the HE trigger-based PPDU that is the response to the Trigger frame.

If the Cascade Indication subfield is 1, then a subsequent Trigger frame follows the current Trigger frame. Otherwise the Cascade Indication subfield is 0.

The CS Required subfield is set to 1 to indicate that the STAs identified in the Per User Info fields are required to use ED to sense the medium and to consider the medium state and the NAV in determining whether or not to repond. The CS Requred subfield is set to 0 to indicate that the STAs identified in the Per User Info fields are not required consider the medium state or the NAV in determining whether or not to respond.

The HE-SIG-A Info subfield of the Common Info field indicates the content of the HE-SIG-A field of the HE trigger-based PPDU response. The TBD bits in HE-SIG-A of the HE trigger-based PPDU that may be implicitly known by all responding STAs can be excluded.

The CP and LTF Type subfield of the Common Info field indicates the CP and HE-LTF type of the HE trigger-based PPDU response. The CP and LTF field encoding is defined in Table 9‑2.

Table 9‑2 - CP and LTF field encoding

|  |  |
| --- | --- |
| **CP and LTF field value** | **Description** |
| 0 | 2x LTF + 0.8 µs CP |
| 1 | 2x LTF + 1.6 µs CP |
| 2 | 4x LTF + 3.2 µs CP |
| 3-TBD | Reserved |

The Trigger Type subfield indicates the type of the Trigger frame. The Trigger frame can include an optional type-specific Common Info and optional type-specific Per User Info. Table 9‑3 defines the valid Trigger Type.

Table 9‑3 - Trigger Type field encoding

|  |  |
| --- | --- |
| **Trigger Type value** | **Trigger Type description** |
| 0 | Basic Trigger |
| 1 | Beamforming Report Poll Trigger |
| 2 | MU-BAR |
| 3 | MU-RTS |
| 4-15 | Reserved |

The Per User Info field is defined in Figure 9‑1.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | User Indentifier | RU Allocation | Coding Type | MCS | DCM | SS Allocation | Target RSSI | Type dependent Per User Info |
| Bits: | 12 | 8 | 1 | 4 | 1 | TBD | TBD | variable |

Figure 9‑1 - Per User Info field

Discussion

These are the proposed changes:

* Proposed RU allocation uses 8 bits
* Coding type only indicates BCC/LDPC, hence 1 bit is sufficient
* 4 bits MCS are sufficient
* Target RSSI is relted to the power control algorithm

The User Identifier subfield of the Per User Info field indicates the AID of the STA allocated the RU to transmit the MPDU(s) in the HE trigger-based PPDU.

The RU Allocation subfield of the Per User Info field indicates the RU used by the HE trigger-based PPDU of the STA identified by User Identifier subfield. The length and coding of RU Allocation subfield are TBD.

The Coding Type subfield of the Per User Info field indicates the code type of the HE trigger-based PPDU response of the STA identified by User Identifier subfield. Set to 0 for BCC and set to 1 for LDPC.

The MCS subfield of the Per User Info field indicates the MCS of the HE trigger-based PPDU response of the STA identified by User Identifier field. The encoding of the MCS field is as defined in Section XXX.

The DCM subfield of the Per User Info field indicates dual carrier modulation of the HE trigger-based PPDU response of the STA identified by User Identifier subfield. A value of 1 indicates that the HE trigger-based PPDU response shall use DCM as defined in section XXX. Set to 0 to indicate that DCM shall not be used.

The SS Allocation subfield of the Per User Info field indicates the spatial streams of the HE trigger-based PPDU response of the STA identified by User Identifier field.

The Padding field extends the frame length to give the recipient STAs more time to prepare a response. The length and the content of Padding field are TBD.

**Straw Poll**

**Do you agree to amend the Trigger Frame format in the SFD, as shown in this document?**