IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Text Changes for SR Fields in HE Trigger-Based PPDU | | | | |
| Date: 2016-07-25 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Minho Cheong | Newracom | 9008 Research Dr.  Irvine, CA 92618 |  | minho.cheong@newracom.com |
| Reza Hedayat |  | reza.hedayat@newracom.com |
| Young Hoon Kwon |  | younghoon.kwon@newracom.com |
| Yongho Seok |  | yongho.seok@newracom.com |
| Daewon Lee |  | daewon.lee@newracom.com |
| Yujin Noh |  | yujin.noh@newracom.com |
| Ron Porat | Broadcom |  |  | rporat@broadcom.com |
| Sriram Venkateswaran |  |  |  |
| Matthew Fischer |  |  | mfischer@broadcom.com |
| Zhou Lan |  |  |  |
| Leo Montreuil |  |  |  |
| Andrew Blanksby |  |  |  |
| Vinko Erceg |  |  |  |
| Thomas Derham |  |  |  |
| Mingyue Ji |  |  |  |
| Robert Stacey | Intel | 2111 NE 25th Ave, Hillsboro OR 97124, USA | +1-503-724-893 | robert.stacey@intel.com |
| Shahrnaz Azizi |  | shahrnaz.azizi@intel.com |
| Po-Kai Huang |  | po-kai.huang@intel.com |
| Qinghua Li |  | quinghua.li@intel.com |
| Xiaogang Chen |  | xiaogang.c.chen@intel.com |
| Chitto Ghosh |  | chittabrata.ghosh@intel.com |
| Laurent Cariou |  | laurent.cariou@intel.com |
| Yaron Alpert |  | yaron.alpert@intel.com |
| Assaf Gurevitz |  | assaf.gurevitz@intel.com |
| Ilan Sutskover |  | ilan.sutskover@intel.com |
| Feng Jiang |  | feng1.jiang@intel.com |
| Hongyuan Zhang | Marvell | 5488 Marvell Lane, Santa Clara, CA, 95054 | 408-222-2500 | hongyuan@marvell.com |
| Lei Wang |  | Leileiw@marvell.com |
| Liwen Chu |  | liwenchu@marvell.com |
| Jinjing Jiang |  | jinjing@marvell.com |
| Yan Zhang |  | yzhang@marvell.com |
| Rui Cao |  | ruicao@marvell.com |
| Sudhir Srinivasa |  | sudhirs@marvell.com |
| Bo Yu |  | boyu@marvell.com |
| Saga Tamhane |  | sagar@marvell.com |
| Mao Yu |  | my@marvel..com |
| Xiayu Zheng |  | xzheng@marvell.com |
| Christian Berger |  | crberger@marvell.com |
| Niranjan Grandhe |  | ngrandhe@marvell.com |
| Hui-Ling Lou |  | hlou@marvell.com |
| Alice Chen | Qualcomm | 5775 Morehouse Dr. San Diego, CA, USA |  | alicel@qti.qualcomm.com |
| Albert Van Zelst | Straatweg 66-S Breukelen, 3621 BR Netherlands |  | allert@qti.qualcomm.com |
| Alfred Asterjadhi | 5775 Morehouse Dr. San Diego, CA, USA |  | aasterja@qti.qualcomm.com |
| Bin Tian | 5775 Morehouse Dr. San Diego, CA, USA |  | btian@qti.qualcomm.com |
| Carlos Aldana | 1700 Technology Drive San Jose, CA 95110, USA |  | caldana@qca.qualcomm.com |
| George Cherian | 5775 Morehouse Dr. San Diego, CA, USA |  | gcherian@qti.qualcomm.com |
| Gwendolyn Barriac | 5775 Morehouse Dr. San Diego, CA, USA |  | gbarriac@qti.qualcomm.com |
| Hemanth Sampath | 5775 Morehouse Dr. San Diego, CA, USA |  | hsampath@qti.qualcomm.com |
| Lin Yang | 5775 Morehouse Dr. San Diego, CA, USA |  | linyang@qti.qualcomm.com |
| Lochan Verma | 5775 Morehouse Dr. San Diego, CA USA |  | lverma@qti.qualcomm.com |
| Menzo Wentink | Straatweg 66-S Breukelen, 3621 BR Netherlands |  | mwentink@qti.qualcomm.com |
| Naveen Kakani | 2100 Lakeside Boulevard Suite 475, Richardson TX 75082, USA |  | nkakani@qti.qualcomm.com |
| Raja Banerjea | 1060 Rincon Circle San Jose CA 95131, USA |  | rajab@qit.qualcomm.com |
| Richard Van Nee | Straatweg 66-S Breukelen, 3621 BR Netherlands |  | rvannee@qti.qualcomm.com |
| Rolf De Vegt | Qualcomm | 1700 Technology Drive San Jose, CA 95110, USA |  | rolfv@qca.qualcomm.com |
| Sameer Vermani | 5775 Morehouse Dr. San Diego, CA, USA |  | svverman@qti.qualcomm.com |
| Simone Merlin | 5775 Morehouse Dr. San Diego, CA, USA |  | smerlin@qti.qualcomm.com |
| Tevfik Yucek | 1700 Technology Drive San Jose, CA 95110, USA |  | tyucek@qca.qualcomm.com |
| VK Jones | 1700 Technology Drive San Jose, CA 95110, USA |  | vkjones@qca.qualcomm.com |
| Youhan Kim | 1700 Technology Drive San Jose, CA 95110, USA |  | youhank@qca.qualcomm.com |
| Jianhan Liu | Mediatek  USA | 2860 Junction Ave, San Jose, CA 95134, USA | +1-408-526-1899 | jianhan.Liu@mediatek.com |
| Thomas Pare |  |  | thomas.pare@mediatek.com |
| ChaoChun Wang |  |  | chaochun.wang@mediatek.com |
| James Wang |  |  | james.wang@mediatek.com |
| Tianyu Wu |  |  | tianyu.wu@mediatek.com |
| Russell Huang |  |  | russell.huang@mediatek.com |
| James Yee | Mediatek | No. 1 Dusing 1st Road, Hsinchu, Taiwan | +886-3-567-0766 | james.yee@mediatek.com |
| Frank Hsu |  |  | frank.hsu@mediatek.com |
| Joonsuk Kim | Apple |  |  | joonsuk@apple.com |
| Aon Mujtaba |  |  | mujtaba@apple.com |
| Guoqing Li |  |  | guoqing\_li@apple.com |
| Eric Wong |  |  | ericwong@apple.com |
| Chris Hartman |  |  | chartman@apple.com |
| Jarkko Kneckt |  |  | jkneckt@apple.com |
| David X. Yang | Huawei | F1-17, Huawei Base, Bantian, Shenzhen |  | david.yangxun@huawei.com |
| Jiayin Zhang | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai | +86-18601656691 | zhangjiayin@huawei.com |
| Jun Luo | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | jun.l@huawei.com |
| Yi Luo | F1-17, Huawei Base, Bantian, Shenzhen | +86-18665891036 | Roy.luoyi@huawei.com |
| Yingpei Lin | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | linyingpei@huawei.com |
| Jiyong Pang | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | pangjiyong@huawei.com |
| Zhigang Rong | 10180 Telesis Court, Suite 365, San Diego, CA  92121 NA |  | zhigang.rong@huawei.com |
| Jian Yu | F1-17, Huawei Base, Bantian, Shenzhen |  | ross.yujian@huawei.com |
| Ming Gan | F1-17, Huawei Base, Bantian, Shenzhen |  | ming.gan@huawei.com |
| Yuchen Guo | F1-17, Huawei Base, Bantian, Shenzhen |  | guoyuchen@huawei.com |
| Yunsong Yang | 10180 Telesis Court, Suite 365, San Diego, CA  92121 NA |  | yangyunsong@huawei.com |
| Junghoon Suh | 303 Terry Fox, Suite 400 Kanata, Ottawa, Canada |  | Junghoon.Suh@huawei.com |
| Peter Loc |  |  | peterloc@iwirelesstech.com |
| Edward Au | 303 Terry Fox, Suite 400 Kanata, Ottawa, Canada |  | edward.ks.au@huawei.com |
| Teyan Chen | F1-17, Huawei Base, Bantian, Shenzhen |  | chenteyan@huawei.com |
| Yunbo Li | F1-17, Huawei Base, Bantian, Shenzhen |  | liyunbo@huawei.com |
| David X. Yang | Huawei | F1-17, Huawei Base, Bantian, Shenzhen |  | david.yangxun@huawei.com |
| Jiayin Zhang | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai | +86-18601656691 | zhangjiayin@huawei.com |
| Jun Luo | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | jun.l@huawei.com |
| Yi Luo | F1-17, Huawei Base, Bantian, Shenzhen | +86-18665891036 | Roy.luoyi@huawei.com |
| Yingpei Lin | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | linyingpei@huawei.com |
| Jiyong Pang | 5B-N8, No.2222 Xinjinqiao Road, Pudong, Shanghai |  | pangjiyong@huawei.com |
| Zhigang Rong | 10180 Telesis Court, Suite 365, San Diego, CA  92121 NA |  | zhigang.rong@huawei.com |
| Jian Yu | F1-17, Huawei Base, Bantian, Shenzhen |  | ross.yujian@huawei.com |
| Ming Gan | F1-17, Huawei Base, Bantian, Shenzhen |  | ming.gan@huawei.com |
| Yuchen Guo | F1-17, Huawei Base, Bantian, Shenzhen |  | guoyuchen@huawei.com |
| Yunsong Yang | 10180 Telesis Court, Suite 365, San Diego, CA  92121 NA |  | yangyunsong@huawei.com |
| Junghoon Suh | 303 Terry Fox, Suite 400 Kanata, Ottawa, Canada |  | Junghoon.Suh@huawei.com |
| Peter Loc |  |  | peterloc@iwirelesstech.com |
| Edward Au | 303 Terry Fox, Suite 400 Kanata, Ottawa, Canada |  | edward.ks.au@huawei.com |
| Teyan Chen | F1-17, Huawei Base, Bantian, Shenzhen |  | chenteyan@huawei.com |
| Yunbo Li | F1-17, Huawei Base, Bantian, Shenzhen |  | liyunbo@huawei.com |
| Jinmin Kim | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea |  | Jinmin1230.kim@lge.com |
| Kiseon Ryu |  |  | kiseon.ryu@lge.com |
| Jinyoung Chun |  |  | jiny.chun@lge.com |
| Jinsoo Choi |  |  | js.choi@lge.com |
| Jeongki Kim |  |  | jeongki.kim@lge.com |
| Dongguk Lim |  |  | dongguk.lim@lge.com |
| Suhwook Kim |  |  | suhwook.kim@lge.com |
| Eunsung Park |  |  | esung.park@lge.com |
| JayH Park |  |  | Hyunh.park@lge.com |
| HanGyu Cho |  |  | hg.cho@lge.com |
| Bo Sun | ZTE | #9 Wuxingduan, Xifeng  Rd., Xi'an, China |  | sun.bo1@zte.com.cn |
| Kaiying Lv |  |  | lv.kaiying@zte.com.cn |
| Yonggang Fang |  |  | yfang@ztetx.com |
| Ke Yao |  |  | yao.ke5@zte.com.cn |
| Weimin Xing |  |  | xing.weimin@zte.com.cn |
| Brian Hart | Cisco Systems | 170 W Tasman Dr, San Jose, CA 95134 |  | brianh@cisco.com |
| Pooya Monajemi |  |  | pmonajem@cisco.com |
| Fei Tong | Samsung | Innovation Park,  Cambridge CB4 0DS (U.K.) | +44 1223 434633 | f.tong@samsung.com |
| Hyunjeong Kang | Maetan 3-dong; Yongtong-Gu Suwon; South Korea | +82-31-279-9028 | hyunjeong.kang@samsung.com |
| Kaushik Josiam | 1301, E. Lookout Dr,  Richardson TX 75070 | (972) 761 7437 | k.josiam@samsung.com |
| Mark Rison | Innovation Park,  Cambridge CB4 0DS (U.K.) | +44 1223 434600 | m.rison@samsung.com |
| Rakesh Taori | 1301, E. Lookout Dr,  Richardson TX 75070 | (972) 761 7470 | rakesh.taori@samsung.com |
| Sanghyun Chang | Maetan 3-dong; Yongtong-Gu Suwon; South Korea | +82-10-8864-1751 | s29.chang@samsung.com |
| Yasushi Takatori | NTT | 1-1 Hikari-no-oka, Yokosuka, Kanagawa 239-0847 Japan | +81 46 859 3135 | takatori.yasushi@lab.ntt.co.jp |
| Yasuhiko Inoue | +81 46 859 5097 | inoue.yasuhiko@lab.ntt.co.jp |
| Shoko Shinohara | +81 46 859 5107 | Shinohara.shoko@lab.ntt.co.jp |
| Yusuke Asai | +81 46 859 3494 | asai.yusuke@lab.ntt.co.jp |
| Koichi Ishihara | +81 46 859 4233 | ishihara.koichi@lab.ntt.co.jp |
| Junichi Iwatani | +81 46 859 4222 | Iwatani.junichi@lab.ntt.co.jp |
| Akira Yamada | NTT DOCOMO | 3-6, Hikarinooka, Yokosuka-shi, Kanagawa, 239-8536, Japan | +81 46 840  3759 | yamadaakira@nttdocomo.com |
| Masahito Mori | Sony Corp. |  |  | Masahito.Mori@jp.sony.com |
| Yusuke Tanaka |  |  | YusukeC.Tanaka@jp.sony.com |
| Yuichi Morioka |  |  | Yuichi.Morioka@jp.sony.com |
| Kazuyuki Sakoda |  |  | Kazuyuki.Sakoda@am.sony.com |
| William Carney |  |  | William.Carney@am.sony.com |
| Sigurd Schelstraete | Quantenna |  |  | Sigurd@quantenna.com |
| Huizhao Wang |  |  | hwang@quantenna.com |
| Narendar Madhavan | Toshiba |  |  | narendar.madhavan@toshiba.co.jp |
| Masahiro Sekiya |  |  |  |
| Toshihisa Nabetani |  |  |  |
| Tsuguhide Aoki |  |  |  |
| Tomoko Adachi |  |  |  |
| Kentaro Taniguchi |  |  |  |
| Daisuke Taki |  |  |  |
| Koji Horisaki |  |  |  |
| David Halls |  |  |  |
| Filippo Tosato |  |  |  |
| Zubeir Bocus |  |  |  |
| Fengming Cao |  |  |  |

Abstract

This document provide proposed text changes to resolve SR field interpretation ambiguity. Please refer to document “11-16/0901r2 Clarification of SR Fields in HE Trigger Based PPDU” for details of the discussion.

rev0: initial draft

rev1: added proposed text changes to the common field of the trigger frame.

rev2: clause 9 does not use shall statements, therefore, remove shall statements in the changes to clause 9.

This document shows the proposed text changes for resolving SR field ambiguity, which is discussed in document 11-16/0901r0.

**To TGax Editor:** Replace the “Spatial reuse field” in Table 26-17 of the secton 26.3.9.7.2 (Content) with four new field entries as shown below. Add a note shown below to the end of the Table 26-17 of section 26.3.9.7.2 (Content).

Details of the proposed changes are shown below.

***----- Start of proposed text changes ------***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| * Fields in the HE-SIG-A for an HE trigger-based PPDU | | | | |
| Two Parts of HE-SIG-A | Bit | Field | Number of bits | Description |
|  | B7:B10 | Spatial Reuse 1 | 4 | If Bandwidth is set to 20 MHz   * Spatial Reuse field for the 20MHz bandwidth   If Bandwidth is set to 40 MHz   * Spatial Reuse field for the first 20 MHz of the 40 MHz operating band. (See Note 1)   If Bandwidth is set to 80 MHz   * Spatial Reuse field for the first 20 MHz of the 80 MHz operating band. (See Note 1)   If Bandwidth is set to 160/80+80 MHz   * Spatial Reuse field for first 40 MHz of the 160 MHz operating band. (See Note 1)   “SR\_allowed” signaling indicates whether SR operation is allowed or not.   * Set to 0 to indicate SR is disallowed * The conditions to disallow SR are TBD   Other details are TBD.  Notes: this part needs further development.(#2169) |
|  | B11:B14 | Spatial Reuse 2 | 4 | If Bandwidth is set to 20 MHz   * Spatial Reuse field for the 20MHz bandwidth. * This field is set to same value as Spatial Reuse 1 field.   If Bandwidth is set to 40 MHz   * Spatial Reuse field for the second 20 MHz of the 40 MHz operating band. (See Note 1). * This field is set to same value as Spatial Reuse 1 field when operating in 2.4 GHz band.   If Bandwidth is set to 80 MHz   * Spatial Reuse field for the second 20 MHz of the 80 MHz operating band. (See Note 1)   If Bandwidth is set to 160/80+80 MHz   * Spatial Reuse field for second 40 MHz of the 160 MHz operating band. (See Note 1) |
|  | B15:B18 | Spatial Reuse 3 | 4 | If Bandwidth is set to 20 MHz   * Spatial Reuse field for the 20MHz bandwidth. * This field is set to same value as Spatial Reuse 1 field.   If Bandwidth is set to 40 MHz   * Spatial Reuse field for the first 20 MHz of the 40 MHz operating band. (See Note 1). * This field is set to same value as Spatial Reuse 1 field.   If Bandwidth is set to 80 MHz   * Spatial Reuse field for the third 20 MHz of the 80 MHz operating band. (See Note 1)   If Bandwidth is set to 160/80+80 MHz   * Spatial Reuse field for third 40 MHz of the 160 MHz operating band. (See Note 1). * This field is set to same value as Spatial Reuse 1 field when bandwidth of the HE PPDU is 80+80 MHz. |
|  | B19:B22 | Spatial Reuse 4 | 4 | If Bandwidth is set to 20 MHz   * Spatial Reuse field for the 20MHz bandwidth. * This field is set to same value as Spatial Reuse 1 field.   If Bandwidth is set to 40 MHz   * Spatial Reuse field for the second 20 MHz of the 40 MHz operating band. (See Note 1). * This field is set to same value as Spatial Reuse 2 field.   If Bandwidth is set to 80 MHz   * Spatial Reuse field for the fourth 20 MHz of the 80 MHz operating band. (See Note 1)   If Bandwidth is set to 160/80+80 MHz   * Spatial Reuse field for fourth 40 MHz of the 160 MHz operating band. (See Note 1). * This field is set to same value as Spatial Reuse 2 field when bandwidth of the HE PPDU is 80+80 MHz. |
| Note 1: First, second, third, and fourth 20 or 40MHz band is enumerated from the lowest frequency to highest frequency. | | | | |

***----- End of proposed text changes ------***

Following resolution is proposed changes on top of proposed changes in document 11-16/0780r1, “CIDs for: Section 9.3.1.23 Trigger Frame Format”.

**To TGax Editor:** Apply the following proposed text changes on top of the proposed changes in document 11-16/0780r1.

***----- Start of proposed text changes ------***

The Spatial Reuse bits indicates the value of the Spatial Reuse in the HE-SIGA of the HE\_TRIG PPDU transmitted as a response to the Trigger frame. For HE trigger-based PPDU, 4 SR fields are signaled:

* For 20MHz one SR field corresponding to entire 20MHz (other 3 fields indicate identical values)
* For 40MHz two SR fields for each 20MHz (other 2 fields indicate identical values)
* For 80MHz four SR fields for each 20MHz
* For 160MHz and 80+80MHz four SR fields for each 40MHz

When operating 40MHz in 2.4GHz band, two SR fields, SR field 1 and SR field 2, are set to same values. When operating 80+80MHz, SR field 3 is set to same value as SR field 1, and SR field 4 is set to to same value as SR field 2.

***----- End of proposed text changes ------***