IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution to CID 8007 | | | | |
| Date: 2016-07-21 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Assaf Kasher | Qualcomm | Nahum Het, 11 |  | assaf.kasher@qti.qualcomm.com |

Abstract

This document proposes a resolution to CID 8007 on in RevMC D6.0

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 8007 | 1519.25 | 10.38.3.1 | Figures 10-64 shows a beam refinement transaction. It contradicts the text "beam refinement transaction is complete when the initiator determines that it does not need further training and it has received a BRP frame with no training requests from the beam refinement responder." because the it does not show a packet with the responder with no requests | Fix the figure by adding a packet from the responder without any requests - a submission will be provided |

Discussion:

The figure and the text are not consistent. This **has** caused arguments between implementors. We propose to accept the comment and replace the figure:

***Editor: Replace figure 10-64 (P1519L25-46) below, with the following figure:***

***~~~~***

