IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolutions for “Obsolete?” BlockAcksBasic BlockAckReq, Basic BlockAck, NON HT BlockAck and HT Delayed BlockAck |
| Date: 2017-07 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Graham SMITH | SR Technology | Davie, FL, USA. | 916 799 9563 | gsmith@srtrl.com |

Abstract

This submission proposes resolutions for CIDs 57, 58 and 61

Green indicates material agreed to in the group,

yellow material to be discussed, red material rejected by the group and

cyan material not to be overlooked.

The “Final” view should be selected in Word.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| CID | Commenter | Clause  | Page  | Line | Comment | Proposed |
| 57 | Graham Smith | 9.3.1.8.2 | 712 | 8 | Time to remove BlockAckReq? | Remove |
| 58 | Graham Smith | 9.3.1.9.2 | 716 | 14 | Time to remove basic BlockAck variant? | Remove |
| 61 | Graham Smith | 11.5.2.4 | 1802 | 31 | Time to remove Non-HT blockack ? | Remove, also at 2949L25, 2950L6 |

CID 57 BlockAckReq variant and CID 58 Basic Block Ack variant

P711.56

*DMG STAs use only the Compressed BlockAckReq variant and the Extended Compressed BlockAckReq variant.*

So no worries there then.

No other reference to this outside of 9.3.1.8.2

9.3.1.8 “Basic BlockAckReq”

This describes the Basic BlockAckReq of which there are 5 variants. One of those variants is the “Basic BlockAckReq variant”. This, and only this is to be deleted. The term “BlockAckReq is used generally.

**712.5 “NOTE—Reference to “a BlockAckReq” frame without any other qualification from other subclauses applies to any of the variants, unless specific exclusions are called out.”**

Similarly the term “Basic BlockAck” is used to refer to the “Basic BlockAckReq variant”

So we need to remove all “Basic BlockAckReq”references.

9.3.1.8.1 “Overview”

General consensus to remove but need to check Basic BlockAckReq and Basic BlockAck

RESOLUTION

REVISED

At 711.40 in Table 9-22 replace “Basic BlockAckReq” in column 4 with “Reserved”

(Note: At 711.28 it says four variants, which was wrong but is now correct.)

At 715.42 in Table 9-24 replace “Basic BlockAck” in column 4 with “Reserved”

712.8

Delete 9.3.1.8.2 “Basic BlockAckReq variant”

715.26

“The value 1 is not used in a Basic BlockAck frame outside a PSMP sequence.” ????????

716.14

Delete 9.3.1.9.2

1453.22 delete “other than a Basic BlockAckReq or Basic BlockAck frame”

On page 1452 delete lines 26 to 32.

1453.36 delete “But the Basic BlockAckReq and Basic BlockAck frames are subject to fewer restrictions because their use at times mimics a typical data-Ack exchange, where no BSSBasicRateSet rate restriction exists on the Data frame. In addition, the Basic BlockAck frame is significantly larger than the other Control frames.”

1524.33 The originator requests acknowledgment of outstanding QoS Data frames by sending a BlockAckReq frame. The recipient shall maintain a block ack record for the block.

1524.40 Separate the block of QoS data frames and the BlockAckReq frames into separate TXOPs or SPs

1525.12

If the immediate block ack policy is used, the recipient shall respond to a BlockAckReq frame with a BlockAck frame. If the recipient sends the BlockAck frame, the originator updates its own record and retries any frames that are not acknowledged in the BlockAck frame, either in another block or individually.

1525.18

If the delayed block ack policy is used, the recipient shall respond to a BlockAckReq frame with an Ack frame. The recipient shall then send its BlockAck frame response in a subsequently obtained TXOP. Once the contents of the BlockAck frame have been prepared, the recipient shall send this frame in the earliest possible TXOP using the highest priority AC. The originator shall respond with an Ack frame upon receipt of the BlockAck frame. If delayed block ack policy is used and if the HC is the recipient, then the HC may respond with a +CF-Ack frame if the BlockAckReq frame is the final frame of the polled TXOP’s frame exchange. If delayed block ack policy is used and if the HC is the originator, then the HC may respond with a +CF-Ack frame if the BlockAck frame is the final frame of the TXOP’s frame exchange

1525.46

The subsequent BlockAckReq frame’s starting sequence number shall be higher than or equal to the starting sequence number of the immediately preceding BlockAckReq frame for the same TID.

1525.60

If there is no response (i.e., neither a BlockAck frame nor an Ack frame) to the BlockAckReq frame, the originator may retransmit the BlockAckReq frame within the current TXOP or SP (if time

1526.56

The BlockAckReq frame shall be discarded if all MSDUs

XXXXXXXXXXX e-mail sent 7/12/2017/

1564.54

10.29 PSMP operaton

Within a PSMP-DTT or PSMP-UTT between STAs where one is not an HT STA, BlockAckReq and BlockAck frames shall be exchanged through the use of an immediate block ack agreement and **shall be the basic variants**, i.e., Basic BlockAckReq and Basic BlockAck, respectively.

So my questions are:

1. In the section above from 1570.1, can I simply delete the “Basic BlockAck or” and leave it as just the Multi-TID variant?
2. What do I do with the  “***shall be the basic variants****, i.e., Basic BlockAckReq and Basic BlockAck, respectively”?  Can I substitute Multi-TID?*
3. Does anyone care?  Does anyone use PSMP?  Do we have PSMP expert(s)?
4. Does this mean that we cannot delete Basic BlockAck, and Basic BlockAckReq?

10.29 PSMP operaton

Within a PSMP-DTT or PSMP-UTT between STAs where one is not an HT STA, BlockAckReq and BlockAck frames shall be exchanged through the use of an immediate block ack agreement and shall be the multi-TID variants, i.e., Multi-TID BlockAckReq and Multi-TID BlockAck, respectively.

1570.1 (PSMP ack rules)

Acknowledgment for data transmitted under an immediate or HT-immediate block ack agreement may be requested implicitly using PSMP Ack setting of the Ack Policy field in Data frames or explicitly with a Multi-TID BlockAckReq frame. An AP that transmits Data frames with the Ack Policy field equal to PSMP Ack or that transmits a Multi-TID BlockAckReq frame addressed to a STA in a PSMP-DTT shall allocate sufficient time for the transmission of a Multi- TID BlockAck frame, respectively, in a PSMP-UTT allocated to that STA within the same PSMP sequence. A STA that has received a PSMP frame and that receives a QoS Data frame with the Ack Policy field equal to PSMP Ack or that receives a Multi-TID BlockAckReq frame shall transmit a Multi-TID BlockAck frame, respectively, in the PSMP-UTT of the same PSMP sequence.

1570.19

An AP that receives a QoS Data frame with the Ack Policy field equal to PSMP Ack during a PSMP-UTT shall transmit a response that is a Multi-TID BlockAck frame in the next PSMPDTT that it schedules for that STA, except if it has transmitted a BlockAck frame for such TIDs to the STA outside the PSMP mechanism.

2949.28, and 2950.9 (PICS)

Delete “9.3.1.8.2 (Basic BlockAckReq variant)”

2949.31, 2950.12 (PICS)

Delete “9.3.1.9.2 (Basic BlockAck variant)”

CID 61 NON\_HT Block Ack and HT Delayed Block Ack

1802.13 Table 11-4

Delete entire first row of Table

Delete entire third row of Table

Delete NOTE 1 and NOTE 2

2949L27, 2950L8

Delete

“Non-HT block ack is obsolete.

Support for this mechanism

might be removed in a later

revision of the standard.”

2949L43, 2950L24

Delete in column 3, “10.24.8 HT delayed Block Ack extensions”

154.25 to 154.29 delete all

215.11 delete “HT-delayed block ack,”

687.82 delete “10.24.8.3 (Operation of HT-delayed block ack),”

714.26

The TA field value is the address of the STA transmitting the BlockAck frame.

715.16

Delete “The value 0 is not used for data sent under HT-delayed Block Ack during a PSMP sequence.”

715.22

Delete “The value 1 in a Compressed BlockAck frame indicates HT-delayed block ack. HT-delayed block ack is obsolete and this value might be reserved in a later revision of the standard.”

1004.35 Replace text in B10 with “Reserved”

1005.45 delete entire row

1394.30 delete entire row

1394L33 and L38 delete “or HT-delayed block”

1395.7 delete entire row

1395.10 delete “or HT-delayed block”

1395.19 delete entire row

1395.35 delete entire row

1395.44 delete “or HT-delayed block”

1395.56 delete entire row

1404.1, 1404.16, delete “or HT-delayed block

1421.63 “HTimmediate Block Ack”

1459.45 delete “HT-delayed Block Ack,”

1528.43 delete “and 10.24.8 (HT-delayed block ack extensions),”

1536.34 Delete 10.24.98 in its entirety.

1569.48

Delete “A QoS Data frame transmitted under an HT-delayed block ack agreement during either a PSMPDTT or a PSMP-UTT shall have the Ack Policy field set to Block Ack”

1570.40

Delete “If a BlockAckReq frame for an HT-delayed block ack agreement is transmitted during a PSMP sequence, the BAR Ack Policy subfield of the BlockAckReq frame shall be set to the value representing No Acknowledgment”

1802.18 Delete entire row

1802.22 Delete entire row

1802.31 Delete NOTE 1 and NOTE 2

2970.6 Delete Entire row

Page 3252 Delete lines 49 to 61 (note: check MNeighborReportHTDelayedBlockAck)

3371.16 Delete “or HT-delayed block”