IEEE P802.11
Wireless LANs

|  |
| --- |
| TX-RX Vector for scrambler field indication |
| Date: 2017-08-03 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Solomon Trainin | Qualcomm |  | 972547885738 | strainin@qti.qualcomm.com |
| Carlos Cordeiro  | Intel |  |  | carlos.cordeiro@intel.com |

Abstract

Scrambler field indication is added to Tx Vector and Rx Vector

**30.2.2 TXVECTOR and RXVECTOR parameters**

*Editor, in the Table 8 replace parameter CONTROL\_TRAILER by parameter SCRAMBLER\_INIT\_SETTING*

**Table 8 —TXVECTOR and RXVECTOR parameters**

 

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| SCRAMBLER\_INIT\_SETTING | Format is NON\_EDMG | Indicates the configuration of the Scrambler Initialization field of a control mode PPDU (see Table 10)Enumeration type:Scrambler Control\_trailerEDMG-Header-AChannel\_BW  | Y | Y |
| Otherwise  | Scrambler |  |  |

**10.36.7.2 Polling period (PP)**

*Editor, in all appearances replace “TXVECTOR parameter CONTROL\_TRAILER to Present” by “TXVECTOR parameter SCRAMBLER\_INIT\_SETTING to Control\_trailer”*

**10.36.11.5 Control trailer**

*Editor, in all appearances replace “TXVECTOR parameter CONTROL\_TRAILER to Present” by “TXVECTOR parameter SCRAMBLER\_ INIT\_SETTING to Control\_trailer”*

**10.36.11.4.3 SU-MIMO channel access procedure**

*Editor, in all appearances replace “TXVECTOR parameter CONTROL\_TRAILER to Present” by “TXVECTOR parameter SCRAMBLER\_ INIT\_SETTING to Control\_trailer”*

**30.3.7 Control trailer**

*Editor, in all appearances replace “TXVECTOR parameter CONTROL\_TRAILER to Present” by “TXVECTOR parameter SCRAMBLER\_ INIT\_SETTING to Control\_trailer”*

**10.3.2.7 CTS and DMG CTS procedure**

*Editor, at P50L16 append*

If a DMG CTS frame or a DMG DTS frame is transmitted in a non-EDMG duplicate PPDU to establish a SISO transmission (CH\_BANDWIDTH\_IN\_NON\_EDMG equal to one of CBW216, CBW432, CBW638, CBW864, or CBW216+216), the transmitting EDMG STA shall set the TXVECTOR parameter SCRAMBLER\_ *INIT\_SETTING* to Channel\_BW.

**10.3.2.14 EDMG RTS procedure**

*Editor, at P50L28 append*

If a RTS frame is transmitted in a non-EDMG duplicate PPDU to establish a SISO transmission (CH\_BANDWIDTH\_IN\_NON\_EDMG equal to one of CBW216, CBW432, CBW638, CBW864, or CBW216+216), the transmitting EDMG STA shall set the TXVECTOR parameter SCRAMBLER\_ *INIT\_SETTING* to Channel\_BW.

**References:**

1. IEEE P802.11ay/D0.35, May 2017