IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Draft 0.3 CID148 comment resolution | | | | |
| Date: 2017-10-24 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Solomon Trainin | Qualcomm |  | 972547885738 | [strainin@qti.qualcomm.com](mailto:strainin@qti.qualcomm.com) |
| Assaf Kasher | Qualcomm |  |  | [akasher@qti.qualcomm.com](mailto:akasher@qti.qualcomm.com) |
| Carlos Cordeiro | Intel |  |  | [carlos.cordeiro@intel.com](mailto:carlos.cordeiro@intel.com) |

Abstract

Solutions for CID 148 is provided

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Page** | **Clause** | **Duplicate of CID** | **Resn Status** | **Comment** | **Proposed Change** | **Resolution** | **Owning Ad-hoc** | **Comment Group** |
| 148 | 47.20 | 10.7.7.7 |  |  | Resolve editor comment  ***Editor Note: need to define the rules in this subclause, similar to VHT*** | As noted | Resolve as in  11-17-10nn-00-00ay-draft-03-CID148-comment-resolution | EDITOR | Multirate |

**10.7.7.7 Control frame TXVECTOR parameter restrictions**

A STA shall not transmit a Control frame with the TXVECTOR parameter GI-LENGTH set to a value that is not equal to NormalGi.

A STA shall not transmit a Control frame with the TXVECTOR parameter EDMG-MODULATION not set to EDMG\_SC\_MODE.

A STA shall not transmit a Control frame with the TXVECTOR parameter NUM-STS set to a value greater than one.

A STA shall not transmit a Control frame with the TXVECTOR parameter NUM-USERS is set to a value greater than one.

A STA shall not transmit a Control frame with the TXVECTOR parameter LDPC\_CW\_TYPE set LONG.

A STA shall not transmit a Control frame with the TXVECTOR parameter NUC\_MOD is set to NUCApplied.

**References:**

1. IEEE P802.11ay/D0.3, March 2017