IEEE P802.11
Wireless LANs

|  |
| --- |
| PHY CID 17895 Resolution |
| Date: 2017-11-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Hongyuan Zhang | Marvell |  |  | hongyuan@marvell.com |

Abstract: This document addresses the following CID:

 *CIDs* *17895*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 17895 | 27.5.3.2.3 | 248.1 | For accurate timing synchronization at each STA responding a trigger frame, the legacy part preamble (L-STF, L-LTF, ...) of the PPDU carrying trigger frame shall not be beamformed. There are existing implementations that may beamform the legacy preamble or the whole non-HT PPDU, but it is better to be disallowed if the PPDU is carrying a trigger frame. | Add a note: "Beamforming the non-HT preamble of the PPDU carrying a Trigger Frame is not recommended" | **Revised.**Change to as in doc IEEE802.11-17/1731r1. |

TGax editor: please make the following change P248L4

An HE AP shall not use the short guard interval for an HT or VHT PPDU that carries a Trigger frame. A Trigger frame shall not be carried in a DSSS or HR/DSSS PPDU. An HE AP shall not use STBC encoding for a PPDU that carries a Trigger frame. An HE AP shall not apply transmit beamforming on a non-HT PPDU that carries a Trigger Frame. An HE AP shall not apply transmit beamforming on the non-HT portion preamble of an HT mixed format PPDU that carries a Trigger Frame. An HE AP shall not apply transmit beamforming on the non-VHT portion preamble of a VHT PPDU that carries a Trigger Frame. HE AP shall not apply transmit beamforming on the non-HE portion preamble of an HE PPDU that carries a Trigger Frame.