IEEE P802.11
Wireless LANs

|  |
| --- |
| PHY CID 11895 Resolution |
| Date: 2017-11-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Hongyuan Zhang | Marvell |  |  | hongyuan@marvell.com |

Abstract: This document addresses the following CID:

 *CIDs* *11895*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 11895 | 27.5.3.2.3 | 248.1 | For accurate timing synchronization at each STA responding a trigger frame, the legacy part preamble (L-STF, L-LTF, ..) of the PPDU carrying trigger frame shall not be beamformed. There are existing implementations that may beamform the legacy preamble or the whole non-HT PPDU, but it is better to be disallowed if the PPDU is carrying a trigger frame. | Add a note: "Beamforming the non-HT preamble of the PPDU carrying a Trigger Frame is not recommended" | **Revised.**Change to as in doc IEEE802.11-17/1731r3. |

TGax editor: please make the following change P248L4

An HE AP shall not use the short guard interval for an HT or VHT PPDU that carries a Trigger frame or an UMRS Control field. A Trigger frame shall not be carried in a DSSS or HR/DSSS PPDU. An HE AP shall not use STBC encoding for a PPDU that carries a Trigger frame or an UMRS Control field.

When transmitting PPDUs carrying a Trigger frame or an UMRS Control field, an HE AP should not apply transmit beamforming on:

* Non-HT PPDUs
* Fields prior to the HT-STF field of an HT mixed format PPDU
* Pre-VHT modulated fields of an VHT PPDU
* Pre-HE modulated fields of an HE PPDU

An HE AP shall set the Beam Change field in the HE-SIG-A field to 1 in an HE PPDU that carries a Trigger frame or an UMRS Control field.