IEEE P802.11  
Wireless LANs


|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Addressing the Inconsistence of Assigning CCF0 Value For BSS Bandwidth Is Less Than 80MHz in The Table 11-25 | | | | |
| Date: 2017-11-06 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Huizhao Wang | Quantenna Communications | Quantenna Communications, Inc. 1704 Automation Parkway, San Jose, CA 95131, USA |  | hwang@quantenna.com |

Abstract


This submission is to address the incosistence of assigning CCF0 value when the BSS bandwidth is less than 80MHz in the Table 11-25.

**Discussion**

In the Table 11-25, in the second row specifies that: for BSS bandwidth “20, 40 MHz”, the “setting of the Channel Center Frequency Segment 0 subfield” is set to the value of dot11CurrentChannelCenterFrequencyIndex0:



But clause 9.4.2.159, Table 9-252, the CCF0 subfield is “reserved” for BSS bandwidth is less than 80MHz:



In order to be consistent to the Table 9-252, in the Table 11-25, the value of “setting of the Channel Center Frequency Segment 0 subfield” should be specified as 0 (zero) for BSS bandwidth of “20, 40 MHz”.

***Instruct the editor to modify the Table 11-25 as indicated:***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **BSS**  **Bandwidth** | **VHT Operation element Channel Width field** | **Setting of the Channel Center Frequency Segment 0 subfield** | **Setting of the Channel Center Frequency Segment 1 subfield** | **Setting of the Channel Center Frequency Segment 2 subfield** |
| 20, 40 MHz | 0 | ~~dot11CurrentChannelCenterFrequencyIndex0~~ 0 | 0 | 0 |