IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Update on RXTIME Computation for Control Mode | | | | |
| Date: 2018-04-18 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Artyom Lomayev | Intel | Turgeneva 30, Nizhny Novgorod 603024, Russia | +7 (831) 2969444 | artyom.lomayev@intel.com |
| Alexander Maltsev | Intel |  |  | alexander.maltsev@intel.com |
| Claudio da Silva | Intel |  |  | claudio.da.silva@intel.com |
| Carlos Cordeiro | Intel |  |  | carlos.cordeiro@intel.com |
|  |  |  |  |  |

Abstract

This document proposes the update on the RXTIME computation formula for control mode PPDU defined in [1].

*Editor: update the formulas for RXTIME computation as proposed below, page 425, line 5*

For an EDMG STA and EDMG control mode PPDU, the RXTIME parameter shall be computed using the Length and Training Length fields defined in the L-Header (see Table 20-11). The minimum value for the Length field is equal to 14 octets and the Training Length (TRN\_LEN) can be equal to zero. In the latter case, the TRN field is not appended to the PPDU.

The RXTIME parameter shall be defined in microseconds as follows:









where:



 = 5 octets



*Editor: update the formula as proposed below, page 427, line 4*



**SP:**

Do you agree to accept the proposed changes for RXTIME computation for control mode PPDU as defined in (11-18-0641-01-00ay Update on RXTIME Computation for Control Mode)?

**References:**

1. Draft P802.11ay\_D1.1