IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed resolution for CID 1095 |
| Date: 2018-09-10 |
| Author: |
| Name | Affiliation | Address | Phone | Email |
| Edward Au | Huawei Technologies | 303 Terry Fox Drive, Suite 400, Ottawa, Ontario K2K 3J1 |  | edward.ks.au@huawei.com  |

##### This submission present a resolution for CID 1095. The proposed changes are based on REVmd/D1.4.

##### Revision history:

##### R0 – initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Clause | Page | Line | Comment | Proposed Change |
| 1095 | 11.1.3.8 | 1943 | 53 | Only one type of STA (the WMN STA) requires dot11WirelessManagement=true as a precondition for multiple BSSID capability. However, doesn't the WMN STA by definition have dot11WirelessManagement=true? | Delete "When dot11MultiBSSIDImplemented is true, dot11WirelessManagementImplemented shall be equal to true except for a DMG STA (11ah)and for an S1G STA, in which case it may be equal to false." |

***Discussion:***





***Proposed resolution:***

**Accepted**