IEEE P802.11  
Wireless LANs

|  |
| --- |
| **Resolutions for Miscellaneous CIDs** |
| **Date:** 2018-11-12 |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Yasuhiko Inoue | NTT | 1-1 Hikari-no-oka, Yokosuka, Kanagawa 239-0847 Japan | +81 46 859 5097 | inoue.yasuhiko@lab.ntt.co.jp |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolution for the following 9 CIDs:

* 15000, 16130
* 15001, 16100, 16101, 16102
* 15929, 16170

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

# CID 15000 and 16130

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **PP.LL** | **Comment** | **Proposed Change** | **Resolution** |
| 15000 | Abhishek Patil | 36.60 | It is possible that a STA is in coverage range of an OBSS AP that has assigned the same AID value to one of it's associated STA. Therefore, "STA-ID in HE-SIG-B" is not sufficient to identify the desired STA. | STA-ID should be referred to in conjunction with a particular BSS color to identify the user in a particular BSS. | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 15000. |
| 16130 | Mark RISON | 36.60 | "user: An individual station or group of stations (STAs) identified by a single receiver address (RA) or a STA-ID in HE-SIG-B in the context of single-user multiple input, multiple output (SU-MIMO), multi-user multiple input, multiple output (MU-MIMO), or orthogonal frequency division multiple access (OFDMA)." has confusing precedence. Also it omits SISO users and the signalling for users for VHT DL MU-MIMO, which does not use a STA-ID | Change the definition to "An individual station or group of stations (STAs) using a single identifier, in the context of single input single output (SISO), single-user multiple input, multiple output (SU-MIMO), multi-user  multiple input, multiple output (MU-MIMO), or orthogonal frequency division multiple access (OFDMA)." | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 16130. |
|  |  |  |  |  |  |

**Discussion**

None

**Proposed Text Changes Re: CID 15000 and 16130**

* Definitions specific to IEEE 802.11

***TGax Editor: Update definition of user in subclause 3.2 as shown below:***

**user**: An individual station or group of stations (STAs) identified by a single identifier such as a single receiver address or a STA-ID in HE-SIG-B for a particular BSS Color in HE-SIG-A (#15000, #16130) in the context of single-user multiple input, multiple output (SU-MIMO), multi-user multiple input, multiple output (MU-MIMO), or orthogonal frequency division multiple access (OFDMA).

# CID 15001, 16100, 16101 and 16102

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **PP.LL** | **Comment** | **Proposed Change** | **Resolution** |
| 15001 | Abhishek Patil | 37.54 | Definition of HE ER SU PHY appears twice | Consolidate the two definitions. | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 15001. |
| 16100 | Mark RISON | 37.00 | There are two definitions of "high efficiency (HE) extended range (ER) single user (SU) physical layer (PHY) protocol data unit (PPDU)" | Delete the first | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 16100. |
| 16101 | Mark RISON | 37.00 | There are two definitions of "high efficiency (HE) extended range (ER) single user (SU) physical layer (PHY) protocol data unit (PPDU)" | Delete the second | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 16101. |
| 16102 | Mark RISON | 37.00 | There are two definitions of "high efficiency (HE) extended range (ER) single user (SU) physical layer (PHY) protocol data unit (PPDU)" | Delete the one that does not match the form used for other PPDUs | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 16102. |
|  |  |  |  |  |  |

**Discussion**

None

**Proposed text changes Re: CID 15001, 16100, 16101 and 16102**

* Definitions, acronyms, and abbreviations
* Definitions specific to IEEE 802.11

***TGax Editor: Delete the first definition of the HE ER SU PPDU as shown below:***

(#15001, #16100, #16101, #16102)**high efficiency (HE) extended range (ER) single-user (SU) physical layer (PHY) protocol data unit (PPDU):** An HE PPDU transmitted with HE ER SU PPDU format that carries one PHY service data units (PSDU) for one user.

# CID 15929, 16170

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **PP.LL** | **Comment** | **Proposed Change** | **Resolution** |
| 15929 | Mark Hamilton | 33.10 | The intention seems to be that A-MSDUs can now be fragmented. There are assumptions in legacy MAC/PHY that will likely break (because the baseline text now assumes all A-MSDUs could be a fragment unless stated otherwise, so it needs to be clearly stated otherwise where things will break), and there are other places in the text that are inconsistent with this. | Add to the definition of GCR frame, that it must be an unfragmented A-MSDU. Correct the statement in the Note following the defintion of MMPDU that says, "An A-MSDU is trasmitted in one MPDU." In the first sentence of 10.4, add that the MAC may fragment and reassemble A-MSDUs, also, (but only if it is HE and the peer is HE and both support A-MSDU Fragmentation). Clarify the extent of the Editor's instruction at P109.6. Does this apply to \_every\_ occurance of A-MSDU in the entire rest of the Standard? (Surely, not.) There are probably more examples. | Revised.  Agreed in principle.  TGax Editor: Please implement the proposed changes in 11-18/1807r3 for CID 15929. |
| 16170 | Mark RISON | 33.10 | The baseline definition "aggregate medium access control (MAC) service data unit (A-MSDU): A structure that contains one or more MSDUs and is transported within a single (unfragmented) data medium access control (MAC) protocol data unit (MPDU)." is no longer true with dynamic fragmentation. | Extend the definition to allow for dynamic fragmentation. | Revised.  Agreed in principle.  The suggested change has been already made in the D3.2. |
|  |  |  |  |  |  |

##### Discussion

None

**Proposed Text Updates: CID 15929**

* Definitions specific to IEEE 802.11

***TGax Editor: Update the definition of concealed groupcast with retries (GCR) frame as follow:***

**concealed groupcast with retries (GCR) frame:** A group addressed frame that is transmitted using the aggregate medium access control (MAC) service data unit (A-MSDU) frame format which is not fragmented (#15929) with the destination address (DA) field set to the GCR concealment address.

* MSDU and MMPDU fragmentation(#1070)(11ai)

***TGax Editor: Modify the first paragraph of the subclause 10.4 as follows:***

The MAC may fragment and reassemble MSDUs or MMPDUs that are carried in individually addressed MPDUs. The fragmentation and defragmentation mechanisms allow for fragment retransmission. The MAC may fragment and reassemble A-MSDUs as well, if both of the transmitting and receiving MAC entities support A-MSDU Fragmentation (#15929).