IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed spec text for CID 296 |
| Date: 2018-10-25 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Gaurav Patwardhan | HPE |  |  | gaurav.patwardhan@hpe.com |
| Eldad Perahia | HPE |  |  | eldad.perahia@hpe.com  |

Abstract

This submission proposes the spec text for a solution to the lost WUR non-AP STA problem in reference to CID 296 in 11-18-1794-00-00ba-comments-on-tgba-d1-0.xlsx.

Comment submitted:

“When a WUR non-AP STA is operating in Duty Cycled mode and goes to sleep state for more than the agreed duty cycle period, there is a mismatch of the STA state at the AP where the AP does not know if the STA is still within the BSS range and still in sleep mode or it has moved outside the BSS range. At the AP, the knowledge of whether the STA is within the BSS range is an integral part of Usage model numbers 2 and 7 from the usage model document (11-17-0029-10-00ba-wur-usage-model-document.pptx).”

R0 – Initial Draft based on D1.0

R1 – Revised Initial Draft.

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

|  |  |  |
| --- | --- | --- |
|  |  |  |
|  |  |  |

TGba Editor: Please modify this section as follows:

**9.4.2.275 WUR Operation element**

The WUR Operation element contains the set of parameters necessary to support the WUR operation. The format of the WUR Operation element is defined in Figure 9-751g (WUR Operation element format).

|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | **Element****ID** | **Length** | **Element****ID****Extension** | **Minimum****Wake-up****Duration** | **Duty****Cycle****Period****Units** | **WUR****Operation****Class** | **WUR****Channel** | **WUR****Beacon****Period** | **Offset of Target WUR Beacon Transmission Time (TWBTT)** |
| Octets: | 1 | 1 | 1 | 1 | 2 | 1 | 1 | 2 | 2 |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  | **WUR****Parameters** | **WUR Connectivity Timeout** |  |  |  |  |
|  |  |  | Octets: | 1 | 1 |  |  |  |  |

**Figure 9-751g—WUR Operation element format**

The Element ID, Length, and Element ID Extension fields are defined in 9.4.2.1 (General).

…

…

The Counter field indicates the current value of the Counter subfield included in the broadcast WUR Wake-up frames.

The WUR Connectivity Timeout field indicates the time after which the WUR connectivity with a WUR non-AP STA will be considered to be lost by the WUR AP with which the STA has negotiated WUR mode negotiation (see 31.11 WUR Connectivity Timeout). The WUR Connectivity Timeout field is set to 0 to indicate that the AP does not support indicating a connectivity timeout value. The WUR Connectivity Timeout field is set to a nonzero value to indicate the time, in units of 10 TUs, after which the WUR connectivity will be lost, wherein the timeout starts from the most recent successful frame exchange between the STA and the AP.

TGba Editor: Please modify this section as follows:

**31.11 WUR Connectivity Timeout**

A WUR capable AP can indicate to a WUR non-AP STA the timeout in units of 10 TUs after which the AP considers the connection to the WUR non-AP STA to be lost. The WUR Connecivity Timeout field in the WUR Operation Element is used to indicate this timeout. This helps the AP to determine whether the WUR non-AP STA has moved outside the AP’s range or is in WUR Mode and non-responsive. The timeout starts from the most recent successful frame exchange between the STA and the AP and is reset for every frame exchanged.

The action to be taken after determining that the connection to the WUR non-AP STA is lost is implementation specific and outside the scope of this standard.