IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| D3.0 Comment Resolution on MAC Miscellaneous | | | | |
| Date: 2018-11-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Jae Seung Lee | ETRI | 161 Gajeong-dong,  Yuseong-gu, Daejeon, Korea | +82 42 860 1326 | jasonlee@etri.re.kr |
| Moon-Sik Lee | ETRI | 161 Gajeong-dong,  Yuseong-gu, Daejeon, Korea | +82 42 860 5966 | moonsiklee@etri.re.kr |
| Yeong Jin Kim | ETRI | 161 Gajeong-dong,  Yuseong-gu, Daejeon, Korea | +82 42 860 5617 | yjkim@etri.re.kr |
| Tae Joong Kim | ETRI | 161 Gajeong-dong,  Yuseong-gu, Daejeon, Korea | +82 42 860 6240 | aisma@etri.re.kr |

Abstract

This document proposes resolutions for following CIDs:

10 CIDs: 15210, 15875, 16581, 16582, 16583, 16556, 16558, 15038, 15064 and 15065.

* CIDs 15210 and 15875: Clause 9.3.3.3
* CIDs 16581, 16582 and 16583: page 116 (Clause 9.4.1.53)
* CIDs 16556 and 16558: page 168 & 169 (Clause 9.4.2.238)
* CID 15038: Clause 9.6.8.36
* CIDs 15064 and 15065: Clause 11.24.7.5

Changes in the text refer to: Draft P802.11ax/D3.2 and 802.11-2016.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 15210 | 9.3.3.3 | 109 | 25 | Are these cumulative requirements, in the sense that dot11QoSOptionImplemented and dot11MeshActivated have to both be false, while both the EDCA Parameter Set element and the MU EDCA Parameter Set element are not set, or would subsets and combinations of these elements being false or unset also cause QoS Capability elements to be present? | Not sure. | Revise.  The current wording is not clear about the condition on the presence of QoS Capability.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |

**Discussion on CID 15210**:

In the baseline (802.11-2016), the presence of QoS Capability is specified as follows: (Table 9-27 Beacon frame body)

*“The QoS Capability element is present if dot11QosOptionImplemented is true, and dot11MeshActivated is false, and EDCA Parameter Set element is not present.”*

In 27.2.7 EDCA operation using MU EDCA parameters (802.11ax D3.2), it is stated that *the QoS Capability element is only present in a Beacon frame if the EDCA Parameter Set element and the MU EDCA Parameter Set element are not present*

802.11ax Draft text should clearly describe the above behaviour in the table.

**Proposed text changes**:

***Change the Table 9-34 (Beacon frame body) in Section 9.3.3.3 (Beacon frame format) of TGax Draft D3.2 (P115L25) as follows:***

**Table 9-27—Beacon frame body**

|  |  |  |
| --- | --- | --- |
| **Order** | **Information** | **Notes** |
| 21 | QoS Capability | The QoS Capability element is present if dot11QosOptionImplemented is true, and dot11MeshActivated is false, and neither the EDCA Parameter Set element nor the MU EDCA Parameter Set element are ~~is not~~ present. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 15875 | 9.3.3.3 | 109 | 63 | An HE STA always has dot11QoSOptionImplemented being 1. So "dot11QosOption-  Implemented and" should be removed from he sentence. | As in the comment | Revise.  Agree with the commenter.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |

**Proposed text changes**:

***Change the Table 9-34 (Beacon frame body) in Section 9.3.3.3 (Beacon frame format) of TGax Draft D3.2 (P116L38) as follows:***

**Table 9-27—Beacon frame body**

|  |  |  |
| --- | --- | --- |
| **Order** | **Information** | **Notes** |
| 85 | HE BSS Load | The HE BSS Load element is optionally present if ~~dot11QosOptionImplemented,~~(#15623) dot11QBSSLoadImplemented and dot11HEOptionImplemented are true. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 16581 | 9.4.1.53 | 116 |  | Incorrect reference to the Table 9-75 that indicates Setting of the Channel Width subfield | Change "Table 9-75" to "Table 9-81". | Reject.  The description that references Table 9-75 is from the baseline. It is out of scope of TGax to modify it. |
| 16582 | 9.4.1.53 | 116 |  | Incorrect reference to the Table 9-75 that indicates Setting of the Channel Width subfield | Change "Table 9-75" to "Table 9-81". | Reject.  The description that references Table 9-75 is from the baseline. It is out of scope of TGax to modify it. |
| 16583 | 9.4.1.53 | 116 |  | HE STA is required to support LDPC if it supports certain features such as transmitting and receiving bandwidth > 20 MHz, no. of spatial streams is > 4 etc... | Add to the description of the No LDPC subfield: "Set to 0 for an HE STA that supports any of the following: - bandwidth > 20 Mhz - transmitting and receiving more than 4 spatial streams - transmitting and receiving HE MCS 10 and 11" | Revise.  Agree with the commenter in principle.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |

**Proposed text changes (CID 16583)**:

***Change the Table 9-83 (Subfield values of the Operating Mode field) in Section 9.4.1.53 (Operating Mode field) of TGax Draft D3.2 (P122L53) as follows:***

**Table 9-83****—Subfield values of the Operating Mode field**

|  |  |
| --- | --- |
| **Subfield** | **Description** |
| No LDPC | Set to 1 to indicate that the STA transmitting this field prefers not to receive LDPC-encoded PPDUs; set to 0 otherwise.  NOTE – An HE STA always sets this field to 0 if it supports at least one of HE 40/80/160/80+80 SU PPDU bandwidths, or supports more than 4 spatial streams, or supports HE-MCSs 10 and 11. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 16556 | 9.4.2.238 | 168 |  | Contradictory statements in the same paragraph. | The second statement of this paragraph contradicts with the first statement. Remove the second statement. It should read:"The VHT Operation Information Present subfield is set to 1 to indicate that the VHT Operation Information  field is present in the HE Operation element and set to 0 otherwise." | Reject.  The second statement is about how to set the field when the VHT Operation element (which is not VHT Operation Information field) is contained in the frame and it is not a contradiction. In D3.2, the second statement has been removed and the paragraph references clause 27.16.  It is not necessary to change the current text in D3.2. |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 16558 | 9.4.2.238 | 169 |  | Almost identical paragraphs appear in different places, here and on page 354, lines 49-54. It's not relevant for this paragraph to be placed in this section. | Remove this paragraph (An HE STA that transmits ..... BSS Color subfield) | Revise.  Agree with the commenter in principle.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |

**Proposed text changes**:

***Change the following paragraph in Section 9.4.2.242 (HE Operation element) of TGax Draft D3.2 (P176L37) as follows:***

~~An HE STA that transmits an HE Operation element sets the BSS Color Disabled subfield to 1 if the HE STA decides to temporarily disable the use of color for the BSS to which it belongs, for example, after detecting a BSS Color overlap in the neighborhood as described in 27.11.4 (BSS\_COLOR); otherwise the HE STA sets the BSS Color Disabled subfield to 0.NOTE—While the BSS Color Disabled subfield is set to 1, an HE STA continues to advertise a nonzero value in the BSS Color subfield.~~

The BSS Color Disabled subfield is set as described in 27.11.4 (BSS\_COLOR).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 15038 | 9.6.8.36 | 183 | 50 | FD frame may carry OPS element. Description of OPS is missing | Add description for OPS element | Revise.  Agree with the commenter.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |

**Proposed text changes**:

***Add the following paragraph at the end of the Section 9.6.7.36 (FILS Discovery frame format) of TGax Draft D3.2 (P191L49) as follows:***

The FILS Discovery frame may include an OPS element, which is defined in 9.4.2.250 (OPS element), for operation as defined in 27.14.3 (Opportunistic power save).

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Proposed**  **Resolution** |
| 15064 | 11.24.7.5 | 244 | 28 | Change to normative text | Update the first paragraph of this section to remove any declarative text. | Revise.  Agree with the commenter.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |
| 15065 | 11.24.7.5 | 244 | 33 | The second paragraph is making reference to fields within ESS Report element without explicitly mentioning ESS Report element. | Change the second paragraph to: "The Planned ESS subfield in the ESS Information field of the ESS Report element indicates ..." | Accept.  Changed the text accordingly.  See the proposed text change in 11-18/1987r0 |

**Proposed text changes**:

***Change the following two paragraphs in the Section 11.24.7.5 (Planned ESS) of TGax Draft D3.2 (P255L54 and P255L59) as follows:***

**11.24.7.5 Planned ESS**

The AP ~~can~~may indicate that it is in a planned ESS to assist associated STAs' roaming. If it does, it indicates whether it is at the physical edge of the ESS, and ~~can~~may provide a recommendation on the RSSI level to consider for BSS transition.

The Planned ESS subfield in the ESS Information field of the ESS Report element indicates whether the AP is part of an ESS which is planned with several BSSs in overlapping configuration, whereby an associated STA may adjust its BSS transition algorithms accordingly.