IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolution to CID20718 | | | | |
| Date: 2019-07-14 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yujin Noh | Newracom |  |  | yujin.noh at newracom.com |
|  |  |  |  |  |

Abstract

This submission shows

* Resolution for comments received from TGax comment collection (11ax D4.0)
* The proposed changes are based on 11ax D4.1.
* The submission provides resolutions to 1 CID: 20718

Revisions:

* Rev 0: Initial version of the document.
* Rev 1: resolution is updated based on SP at PHY ad-hoc
* Rev 2: resolution is updated based on comment at PHY ad-hoc

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 20718 |  | Re CID 16008: "a" is a terrible name for the pre-FEC padding factor because it cannot be searched for. The spec is so large that the only realistic way to process it is to search for terms; so "a" does do harm | Change all uses of "a" as the pre-FEC padding factor to "PFPF" | Rejected.  Based on the SP results in 11ax PHY ad-hoc meeting, it is decided to be “Rejected”.  Many represented concerns that those modification at the moment would give unnecessary efforts for readers who already get used to these terms in terms of technology and implementation. |