IEEE P802.11
Wireless LANs

|  |
| --- |
| **Ack related CRs**  |
| **Date:** 2019-07-11 |
| **Author(s):** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| George Cherian | Qualcomm | 5775 Morehouse Dr. San Diego, CA, USA |   | gcherian@qti.qualcomm.com |
| Alfred Asterjadhi |  |  |  |  |
| Abhishek Patil |  |  |  |  |
| Raja Banerjea |  |  |  |  |

Abstract

Resolved the following **3 CIDs**

21179, 21185, 20792

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Page** | **Comment** | **Proposed Change** | **Resolution** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 21179 | Pooya Monajemi | 262.06 | When changing the text from a single bit field to a BA Type, errors were inserted into this section. The 2 statements of the form "shall be set to 0 otherwise" now prohibits most of the types in Table 9-30. | Remove those restrictions. | Revised. Remove the phrase "and shall be set to 0 otherwise" from both lines 6 and line 8 |
| 21185 | Pooya Monajemi | 313.03 | The list appears to be missing the All ACK case | Add it to the list | Rejected.The paragraph is about a Multi-STA BA that is sent as a response to frames requiringacknowledgment but that do not belong to an established a block ack agreement |
| 20792 | Mark RISON |  | Re CID 16378: for Management frames, if in MU PPDU, then since no Ack Policy Indicator field, only respond if got TF/TRS. So could apply same rule for Data frames. The benefit of being able to get an SU response to Data frames sent in MU PPDU is rather limited (only one STA can respond) | Delete the references to HTP Ack throughout the draft and instead state that the rules previously described as pertaining to that ack policy instead pertain to frames received by a non-AP STA in an HE MU PPDU | Rejected.HTP Ack differentates QoS Data frame to be responded either through HE TB PPDU from that is sent through SU PPDU.  |