IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for 29.4 | | | | |
| Date: 2019-08-20 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Woojin Ahn | WILUS | 216, Hwangsaeul-ro, Seongnam-si, Gyeonggi-do, Korea | +82-31-712-0523 | [woojin.ahn@wilusgroup.com](mailto:woojin.ahn@wilusgroup.com) |
| John Son | [john.son@wilusgroup.com](mailto:john.son@wilusgroup.com) |

Abstract

This submission proposes resolutions for comments related to TGba D3.0 with the following CIDs (4 CIDs):

* 3077, 3117, 3154, 3209

Revisions:

* Rev 0: Initial version of the document.

***Editing instructions formatted like this are intended to be copied into the TGba Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGba Editor: Editing instructions preceded by “TGba Editor” are instructions to the TGax editor to modify existing material in the TGba draft. As a result of adopting the changes, the TGba editor will execute the instructions rather than copy them to the TGba Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 3077 | Graham Smith | 106.34 | This appears to lay down a lot of conditions when the CCARESET is issued but not when it is not issued. What happens if any of these is not met? It requires an "otherwise" statement | Add what happens otherwise. | REJECTED  As defined in 30.3.15 (WUR receive procedure), the PHY shall keep decoding until receive signal strength drops significantly. |
| 3117 | Jeongki Kim | 106.41 | When a WUR non-AP STA is in the awake state as well as the doze state and the STA receives a WUR frame, the WUR non-AP STA should be able to filter the PPDU (i.e., issue a PHY-CCARESET.request primitive) if one of the indicated conditions is met. Therefore, delete the "if the WUR non-AP STA is in the doze state" in the sentence. | Remove the "if the WUR non-AP STA is in the doze state" in the sentence. | REJECTED  If the WUR MAC issues CCARESET while the STA is in awake state, it risks that an ongoing OFDM PPDU reception is cancelled or an existing NAV is cancelled. On the other hand, the benefit of the proposal is small, since if a STA is in WUR Mode, the STA is expected in doze state for much longer time than awake state. In case, a STA enters awake state frequently, it is better to use WUR Suspend Mode. |
| 3154 | Joseph Levy | 106.40 | A WUR non-AP STA that is in doze state is in Power Management mode, not in WUR mode. Please clarify that the actions/restrictions below are perinate to a WUR non-AP STA that is in WUR awake state. As that is the only time when a WUR non-AP STA will receives WRU PPDUs. | "Replace: ""If the PHY of a WUR non-AP STA issues a PHY-RXSTART.indication due to a WUR PPDU reception, then the MAC sublayer of the WUR non-AP STA should issue a PHY- CARESET.request primitive before the end of the WUR PPDU if the WUR non-AP STA is in the doze state, and the data transferred from the PHY contains any of the followings:"" | REJECTED  WUR STA can use both Power Management mode and WUR mode. The cited sentence is a normative behavior for a WUR STA that is in doze state of Power Management mode and WUR awake state in WUR mode. As a WUR STA receives a WUR PPDU, it implies that the STA is in WUR awake state. No change is required. |
| 3209 | Michael Montemurro | 106.41 | If a WUR capabile STA transition from the awake to the doze state, there is no way for the WUR capable AP to determine whether to use legacy power-save mechanisms or WUR to maintain state. | With: ""If the PHY of a WUR non-AP STA in WUR awake state issues a PHY-RXSTART.indication due to a WUR PPDU reception, then the MAC sublayer of the WUR non-AP STA should issue a PHY- CARESET.request primitive before the end of the WUR PPDU if the data transferred from the PHY contains any of the followings:" | REJECTED  Upon a successful exchange of WUR Mode request/response frame with the status code "Accept", the WUR AP should use WUR operation for the WUR STA unless the events defined in 29.8.3 (29.8.3 WUR power management operation for a WUR AP), 29.9.2 (WUR AP operation) and 29.13 (WUR Short Wake-up frame operation). No action is required for this comment. |

**Discussion: None**