IEEE P802.11
Wireless LANs

|  |
| --- |
| LB249-Clause-11-24-6-4-2-CID-Resolution |
| Date: 2020-01-11 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Assaf Kasher | Qualcomm |  |  | akasher@qti.qualcomm.com |
|  |  |  |  |  |

Abstract

This document proposes resolutions to LB249 comments on clause 11.22.6.4.2. The base is TGaz D2.0

The list of CIDs resolved: 3067, 3068, 3181, 3186, 3938

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 3067 | 129.00 | 11.22.6.4.2.1.1 | The use of "PDMG/PEDMG" is incorrect. Any PEDMG device is also a PDMG device since PDMG includes PEDMG. Meaning that if it should apply to both PDMG and PEDMG it is enough to specify PDMG! (Note that a PDMG which is not supporting PEDMG is named non-PEDMG). | Replace PDMG/PEDMG with PDMG.Lines: 9, 12, 33 |  **Revise: As in 11-20-0137** |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 3068 | 129.00 | 11.22.6.4.2.1.2 | Heading refers to PDMG but section text to DMG. Is this correct? I assume not. | Use correctly DMG and PDMG (same for EDMG and PEDMG). What is the rule? |  **Revised : As in 11-20-0137** |
| 3181 | 129.00 | 11.22.6.4.2.1.1 | Throughout this subclause replace "PDMG" with "DMG" and "PEDMG" with "EDMG" (PDMG/PEDMG are no longer in use" | as in comment |  **Accept** |

 ***TGaz Editor: in subclause 11.22.6.4.2.1 (DMG measurement exchange) and its subclauses replace all occurances of “PDMG” with “DMG”.***

***TGaz Editor: in subclause 11.22.6.4.2.1 (DMG measurement exchange) and its subclauses replace all occurances of “PEDMG” with “EDMG”.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 3186 | 131.00 | 11.22.6.4.2.1.3 | "described in 11.22.6.4.2 (EDCA based ranging measurement exchange) the ISTA needs to send AOD measurement results to the RSTA, so that the RSTA may use these to generate he AOD" - reference should be made more specific, "he" should change to "the" | repalce with "described in 11.22.6.4.2.1.2 (DMG/EDGM AOA/AOD measurement exchange) the ISTA needs to send AOD measurement results to the RSTA, so that the RSTA may use these to generate the AOD" |  **Accept** |

***TGAz Editor: Modify the text in P131L10-13 as follows:***

When an ISTA and RSTA agreed on performing an R2I AOD measurement FTM exchange as described in 11.22.6.4.2.1.2 (DMG/EDGM AOA/AOD measurement exchange) the ISTA needs to send AOD measurement results to the RSTA, so that the RSTA may use these to generate the AOD estimates and send the results back to the ISTA***.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| 3938 | 132.00 | 11.22.6.4.2.1.6 | "... shall be used as described ..." the reference is about negotiation, the protocol is defined in this subclause | replace by "Use of the Secure EDMG Measurement exchange protocol shall be negotiated as described ..." |  **Revise as in 11-10-137**  |

***TGaz Editor: Modify the text in P132L31 as follows:***

Setup of the Secure EDMG Measurement exchange is described in 11.22.6.3.5

**References:**

**P802.11az D2.0**