IEEE P802.11
Wireless LANs

|  |
| --- |
| Resolution Clause 6 CIDs: 43, 66, 67, 68, 69, 70, 71 |
| Date: 2020-05-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Joseph LEVY | InterDigital, Inc. | 111 W 35th St., NY, New York | +1 631.622.4239 | joseph.levy@interdigital.com |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This document provides proposed comment resolutions for some comments submitted in response to the 802.11 TGbd D0.3 internal comment collection. CIDs: 43, 66, 67, 68, 69, 70, and 71 are addressed.

The comments are available in: <https://mentor.ieee.org/802.11/dcn/20/11-20-0701-01-00bd-tgbd-d0-3-comments.xlsx>. The proposed resolutions are grouped by clause, page and line number.

**CIDs for Clause 6.6.1, Pages 19 and 20:**

| CID | P:L | Comment  | Proposed Change | Proposed Resolution |
| --- | --- | --- | --- | --- |
| 43 | 19 | The text could be clarified to indicate whether the MLME-CANCELTX.request primitive removes all untransmitted MSDUs in the indicated access category, or only all non-head-of-line MSDUs. If a HOL MSDU is to be removed, the text should clarify up to what point in the contention process the removal must be achievable. For example, should any HOL MSDU be removed as long as the countdown value > 0? As long as the transmission of the HOL MSDU has not started? | Clarify if head-of-line MSDUs are removed as a result of this primitive? Clarify if there is a point in the HOL MSDU's channel contention after which transmission should proceed even if this primitive is invoked. | Discussion:Was the intent of this primitive to allow the queue to be cleared of MSDUs of a specific access category or was it to clear only the non-HOL MSDUs. If it is the latter, should there be a way to clear all MSDUs including the HOL MSDU? I assume that if the MSDU is still in the MAC buffer it should be cleared. But once it has passed the PHY SAP into the PHY buffer it should not be cleared. Also is there any need for an additional request or modification of this request that would allow all MSDUs of a particular type except for the “latest” MSDU of that type to be cleared. e.g. there are 3 type “A” MSDUs in the queue, only the first 2 are cleared promoting the last MSDU of this type to become HOL.  |
| 66 | 19:12 | This primitive can only cancel transmission of mSDUs that have not bee transmitted, as if they have been transmitted they are no longer in the queue. | Replace: "which have been provided to the MAC entity but not yet transmitted"With: "that are in the MAC entity's transmit queue." | **Accept:** Replace: "which have been provided to the MAC entity but not yet transmitted"With: "that are in the MAC entity's transmit queue." |
| 67 | 19:32 | All MSDUs in the transmit queue are un-transmitted, hence there is no need to state that they are un-transmitted. | Delete: "untransmitted"also delete "untransmitted" on line 39. | **Accept:** Delete: "untransmitted"also delete "untransmitted" on line 39. |
| 68 | 19:45 | The description of the effect of receipt should be clearer. | Replace: "This primitive imitates removal of the mistranslated MSDUs of the specified access category from their transmit queue."with: "The receipt of this primitive by the MAC entity causes the MAC entity to remove MSDUs of the specified access category from thetransmit queue." | **Accept:** Replace: "This primitive imitates removal of the mistranslated MSDUs of the specified access category from their transmit queue."with: "The receipt of this primitive by the MAC entity causes the MAC entity to remove MSDUs of the specified access category from the transmit queue." |
| 69 | 19:53 | All MSDUs in the transmit queue are untransmitted, hence there is no need to state that they are untransmitted. | Delete: "untransmitted" | **Accept:** Delete: "untransmitted" |
| 70 | 19:59 | It seems this primitive does not have any parameters. If so, the semantics text should in line with that of other primitives with no parameters. Though it may be use full for this primitive to return the AccessCategory - so that the SME is aware of which MLME\_CANCELTX.request was successful if more than one request was issues. | Replace: "The primitive parameter is as follows:MLME-CANCELTX.confirm()"with: "This primitive has no paramete | **Revised:**In agreement with the proposed resolutions, but with a typo corrected:Replace: "The primitive parameter is as follows:MLME-CANCELTX.confirm()"with: "This primitive has no parameters.” **Discussion:**Should this primitive return the AccessCategory parameter, to allow the confirmation to indicate which request is being confirmed, in the event that more than one request was made (i.e. requests for different access categories)?  |
| 71 | 20:9 | This text should align with the text in the MLE-CANCELTX.request | Replace: "The SME is notified of the completion of the removal of untransmitted MSDUs."With: "The SME is notified that the MAC entity has removed MSDUs of the specified access category from the transmit queue." | **Accept:** Replace: "The SME is notified of the completion of the removal of untransmitted MSDUs."With: "The SME is notified that the MAC entity has removed MSDUs of the specified access category from the transmit queue." |

**References:**

1. [2014 IEEE Standards Style Manual](https://development.standards.ieee.org/myproject/Public/mytools/draft/styleman.pdf): <https://development.standards.ieee.org/myproject/Public/mytools/draft/styleman.pdf>
2. IEEE Std 802.11-2016: <https://ieeexplore.ieee.org/document/7786995>
3. IEEE Std 802.11md D3.0: <http://www.ieee802.org/11/private/Draft_Standards/11md/Draft%20P802.11REVmd_D3.0.pdf>
4. IEEE Std 802.11bd D0.3: <http://www.ieee802.org/11/private/Draft_Standards/11bd/Draft%20P802.11bd_D0.3.pdf>
5. [802.11-20/0701r1](https://mentor.ieee.org/802.11/dcn/20/11-20-0701-01-00bd-tgbd-d0-3-comments.xlsx), TGbd-D0.3-comments, https://mentor.ieee.org/802.11/dcn/20/11-20-0701-01-00bd-tgbd-d0-3-comments.xlsx