IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| MLME for eBCS Termination Notice | | | | |
| Date: 2020-10-06 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 135 Madison Ave  New York, NY  USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
|  |  |  |  |  |

Abstract

This submission proposes MLME primitives descriptions related to eBCS Termination Notice Procedure.

# 

# TGbc Editor: please modify Clause 6 of TGbc D0.2 spec as follows:

## 6 Layer Management

TGbc editor: Please insert the following paragraphs into Clause 6.3 into the newly proposed subclause 6.3.bc1:

6.3.bc1.4 MLME-EBCTERMINATIONNOTICE.request

6.3.bc1.4.1 Function

This primitive supports the signaling of termination notice of one or more eBCSs.

6.3.bc1.4.2 Semantics of the service primitive

The primitive parameters are as follows:

MLME-EBCSTERMINATIONNOTICE.request(

eBCSTerminationInformationSet

)

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Valid range** | **Description** |
| eBCSTerminationInformationSet | eBCS Termination Information Set field | As defined in 9.6.7.1.bc3 (eBCS Termination Notice frame format) | Specifies the termination information for one or more eBCSs. |

6.3.bc1.4.3 When generated

This primitive is generated by the SME to request that an eBCS Termination Information frame be sent.

6.3.bc1.4.4 effect of receipt

The STA sends an eBCS Termination Notice frame.

6.3.bc1.5 MLME-EBCTERMINATIONNOTICE.indication

6.3.bc1.5.1 Function

This primitive indicates that an eBCS Termination Notice frame is received.

6.3.bc1.5.2 Semantics of the service primitive

The primitive parameters are as follows:

MLME-EBCSTERMINATIONNOTICE.indication(

eBCSTerminationInformationSet

)

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Type** | **Valid range** | **Description** |
| eBCSTerminationInformationSet | eBCS Termination Information Set field | As defined in 9.6.7.1.bc3 (eBCS Termination Notice frame format) | The contents of the eBCS Termination Information Set field in the received eBCS Termination Notice frame. |

6.3.bc1.5.3 When generated

This primitive is generated by the MLME when an eBCS Termination Notice frame is received.

6.3.bc1.5.4 effect of receipt

The SME is notified of the receipt of an eBCS Termination Notice frame.