IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| 11ax D6.0 comment resolution of CID 25076, 25077 | | | | |
| Date: 2020-03-28 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Liwen Chu | NXP |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for multiple comments related to TGax D6.0 with the following CIDs:

* 25076, 25077

Revisions:

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGax Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGax Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGax Editor: Editing instructions preceded by “TGax Editor” are instructions to the TGax editor to modify existing material in the TGax draft. As a result of adopting the changes, the TGax editor will execute the instructions rather than copy them to the TGax Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **PP** | **LL** | **Comment** | **Proposed Change** | Resolution |
| 25076 | 288 | 46 | To meet QoS and fairness principles, frames from the primary AC shall always be transmitted first, except in an HE TB PPDU. | Change "In a non-HE MU PPDU, frames" to "In a PPDU that is not an HE TB PPDU, frames" | Revised  Discussion: The paragraph that the commenter cited is about frame selection from related AC in MU PPDU. The change proposed by the commenter is not in line with the rules defined in subclause 26:  In subclause 26.6, in HE SU, ER SU PPDU or HE MU PPDU from non-AP STA, the frames from primary AC are first transmitted, if no frames from primary AC exist, the frames form AC higher than primary AC can be transmitted. In HE MU PPDUfrom EHT AP, frames from any TIDs can be transmitted. In HE TB PPDU, frames from any TID can be transmitted.  Another observation is that in 802.11baseline the frames transmitted by TXOP responder can from any TIDs in some cases, e.g. in RD operation when the TXOP holder indicates no restriction of the TIDs in RD transmission. This is also true for PSMP.  the frame aggregation rules of TIDs in HE MU PPDU is defined in 26.6.3.  TGax editor please make the changes in 11-20/1571r1 under CID 25076 |
| 25077 | 288 | 48 | "Secondary AC traffic shall not be included in an HE MU PPDU if it would cause the TXOP limit of the primary AC to be exceeded." is duplication of the next sentence (and the rule has been further clarified in md/D4.0) | Delete the cited text | Accepted |

**10.23.2.7 Sharing an EDCA TXOP**

***TGax editor:Change the first paragraph in 10.23.2.7 as follows(#25076):***

The AC associated with the EDCAF that gains an EDCA TXOP is referred to as the primary AC. Frames from ACs other than the primary AC shall not be included in the TXOP, with the following exceptions (TXOP sharing):

* In a PPDU other than an MU PPDU, frames from a higher priority AC may be included when at least one frame from the primary AC has been transmitted and all frames from the primary AC have been transmitted and frames from the AC(s) defined in 26.6.3 (Multi-TID A-MPDU and ack-enabled single-TID A-MPDU) for HE PPDUs.
* When an AP supports ~~DL-MU-MIMO~~ MU PPDUs, frames from a higher or lower priority AC may be included in a VHT or S1G MU PPDU with the TXVECTOR parameter NUM\_USERS > 1 or an HE MU PPDU, when these frames do not increase the duration of the VHT or S1G beyond that required for the transmissions of the frames of the primary AC, targeting up to four STAs if it is transmitted in a VHT MU PPDU. In a non-HE MU PPDU, ~~F~~frames from the primary AC shall be transmitted first. The inclusion of secondary AC traffic in an HE MU PPDU is described in 26.6.3 (Multi-TID A-MPDU and ack-enabled single-TID A-MPDU) Secondary AC traffic shall not be included in an HE MU PPDU if it would cause the TXOP limit of the primary AC to be exceeded.(#24136, #Ed)