IEEE P802.11  
Wireless LANs

|  |  |  |
| --- | --- | --- |
| Resolution to CID 7078 | | |
| Date: 2020-October-13 | | |
| Author(s): | | |
| Name | Affiliation | email |
| Alecsander Eitan | Qualcomm | eitana@qti.qualcomm.com |
| Assaf Kasher | Qualcomm | akasher@qti.qualcomm.com |
| Solomon Trainin | Qualcomm | strainin@qti.qualcomm.com |

Abstract

This submission proposes resolution to CID 7078

The resolutions are in reference to Draft IEEE P802.11ay Draft6.0 &

11-20-1558-01-00ay-comments-on-tgay-d6-0.xlsx

|  |  |  |  |
| --- | --- | --- | --- |
| CID | Clause | Comment | Proposed change |
| 7078 | 28.3.9.10 | Change "The RCPI of the CCI is 6 dB or less than the RCPI of the intended PPDU" to "The RCPI of the CCI is at least 6 dB less than the RCPI of the intended PPDU", or to "The RCPI of the CCI is at least 6 dB below the RCPI of the intended PPDU" | As in the comment. |

**Discussion:**

The commenter suggests improving the phrasing of the condition.

No change in the technical details of the condition.

**Proposed resolution:** **Revised.** (Accept one of the suggested options)

***TGay Editor: Edit the text in 28.3.9.10 P475L7:***

In the presence of CCI originating from a DMG PPDU transmission, a DMG STA operating in a TDD SP should decode an intended PPDU as long as all of the following conditions hold:

⎯ The RCPI of the intended PPDU is at least 3 dB above actual receiver sensitivity; and

⎯ The RCPI of the CCI is at least 6 dB below ~~than~~ the RCPI of the intended PPDU; and

⎯ The intended PPDU has sufficient signal to noise plus interference ratio to be decodable.