IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| PHY (PPDU RX) Abort | | | | |
| Date: 2020-11-03 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Payam Torab | Facebook | 1 Hacker Way  Menlo Park, CA 94025  USA |  | torab@ieee.org |
| Djordje Tujkovic |  | djordjet@fb.com |
|  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Comment resolution for CIDs 7017. Proposed edits are based on 11ay Draft 6.0 and REVmd Draft 5.0.

|  |  |  |  |
| --- | --- | --- | --- |
| **CID** | **Comment** | **Proposed change** | **Resolution** |
| 7017 | The PHY primitive has been defined for PHY-Abort, however, there are no normative behavior described on how this primitive is used. | Please add normative behavior when this primitive should be used. | Revised |

**Discussion:**

The need for receive abort was first discussed in 11-18/0164 (Interference Mitigation in mmWave Distribution Networks) in the context of mitigating co-channel interference by cutting short the reception of any PPDU whose preamble has been acquired before the the TDD slot boundary during which a STA is expected to receive.



The primitive (PHY-ABORT, 8.3.5.17) has been added to PHY SAP, but there is no text to describe where the primitive can be invoked. In the following we add descriptive text.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

***Editor: Add this sententenceto the end of Section 28.3.9.10 (Receiver co-channel interference (CCI) resilience)***

In addition, a DMG STA operating in a TDD SP may abort a PPDU reception (see 8.3.5.17 (PHY-ABORT.request)) at the trailing boundary of any TDD slot after which the STA is scheduled to receive from a different transmitting STA.