IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| PDT: Channel access for Triggered TXOP Sharing | | | | |
| Date: 2021-03-17 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Dibakar Das | Intel |  |  | Dibakar.das@intel.com |
| Laurent Cariou |  |  |  |
| Dmitry Akhmetov |  |  |  |
| Dan Bravo |  |  |  |
| Danny Alexander |  |  |  |

Abstract

This submission proposes channel access rules to the **Triggered TXOP sharing procedure** in 0087r6 and resolve the following TBD:

“After a non-AP STA receives an MU-RTS TXS Trigger frame from its associated AP and addressed to it, the STA shall transmit one or more non-TB PPDUs within the time allocation signaled in the TBD field of the MU-RTS TXS Trigger frame.”

**Discussion:**

1. We propose the signaling and the channel access procedure for the Triggered TXOP sharing procedure.
2. We propose that the time allocation information is carried in the UL Length field of the MU-RTS TX Trigger frame to signal upto ~16ms. However, there can be two options on the signaling format. As such we may want to run a SP.

**SP 1**

Which option do you support for the encoding in the UL Length field in an MU-RTS TX Trigger frame to indicate the time allocated to a non-AP STA:

Option 1: Bits B0-B6 of the UL Length field are used and with unit of 128us

Option 2: Bits B0-B11 of the UL Length field in units of 4us ?

This PDT assumes Option 1 is preferred.

1. In practice, devices today overshoot their TXOP limits in some cases (e.g., when the TXOP limit is too small to fit a frame without aggregation). We expect those cases to arise with Triggered SU/P2P mechanism as well where a STA would like to overshoot its allocation a little to fit a PPDU. So, two possible options to enable this:

Option 1: just define the conditions when a STA is allowed to overshoot to be same as whats allowed for a STA as a TXOP owner.

Option 2: Option 1 + exceed allocation only when AP explicitly informs the STA that it is allowed to overshoot.

In this doc we are assuming Option 1.

**9.3.1.22 Trigger frame format**

**9.3.1.22.1 General**

***TGbe editor: Modify Figure 9-64b in P45L53 of 11ax draft 8.0 as follows:***

**B0 B3 B4 B15 B16 B17 B18 B19 B20 B21 B22 B23 B25**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Trigger Type | UL Length | More TF | CS Required | UL BW | GI And HE-LTF Type/TXOP Sharing Modes | MU-MIMO HE-LTF Mode | Number of HE-LTF Symbols And Midamble Periodicity |

Bits: 4 12 1 1 2 2 1 3

**B26 B27 B28 B33 B34 B35 B36 B37 B52 B53 B54 B62**

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| UL STBC | LDPC  Extra  Symbol  Segment | AP Tx  Power | Pre-FEC  Padding  Factor | PE  Disambiguity | UL Spatial  Reuse | Doppler | UL  HE-SIG-A  2  Reserved |

Bits: 4 12 1 1 2 2 1 3

**B63**

|  |  |
| --- | --- |
| Reserved | Trigger Dependent Common Info |

Bits: 1 variable

**Figure 9-64b—Common Info field format**

***TGbe editor: Insert the following text in P128L48 of 11ax draft 8.0 as follows:***

If the Trigger Type subfield value is 3, then B20–B21 of the Common Info field is the TxOP Sharing Modes subfield, otherwise B20–B21 of the Common Info field is the GI And HE-LTF Type subfield.

**9.3.1.22.5 MU-RTS Trigger frame format**

***TGbe editor: Modify the following text in P129L43 of 11ax draft 8.0 as follows:***

The MU-MIMO HE-LTF Mode, Number Of HE-LTF Symbols And Midamble Periodicity, UL STBC, LDPC Extra Symbol Segment, AP Tx Power, Pre-FEC Padding Factor, PE Disambiguity, UL Spatial Reuse, Doppler and UL HE-SIG-A2 Reserved subfields in the Common Info field are reserved.

***TGbe editor: Modify the following text in P66L52 of draft 0.4 as follows:***

The TxOP Sharing Modes subfield in the Common Info field is set to a nonzero value to signal an MU-RTS Trigger frame from an EHT AP that allocates time within an obtained TXOP to an EHT non-APSTA for transmitting one or more non-TB PPDUs sequentially (see 35.2.1.3 (Triggered TXOP sharing procedure)). The TxOP Sharing Modes subfield encoding in an MU-RTS frame ~~sent from an EHT AP~~ is defined in Table 9-31xxx (TxOP Sharing Modes subfield encoding).

**Table 9-31xxx TxOP Sharing Modes subfield encoding**

|  |  |
| --- | --- |
| **TxOP Sharing Modes subfield value** | **Description** |
| 0 | MU-RTS that does not initiate MU-RTS TXOP Sharing procedure |
| 1 | MU-RTS that initiates MU-RTS TXOP Sharing procedure wherein a scheduled STA can only transmit PPDU addressed to its associated AP |
| 2 | MU-RTS that initiates MU-RTS TXOP Sharing procedure wherein a scheduled STA can transmit PPDU(s) addressed to its associated AP or addressed to another STA |
| 3 | Reserved |

An MU-RTS Trigger frame with the TxOP Sharing Modes subfield set to a nonzero value is called an MU-RTS TXOP Sharing (TXS) Trigger frame for the remainder of this subclause and Clause 35 (Extremely high throughput (EHT) MAC specification).

The UL Length subfield in the Common Info field of the MU-RTS TXS Trigger frame indicates the time duration allocated to the non-AP STA within the TXOP obtained by the AP. The bits B0-B6 of the UL Length subfield in the MU-RTS TXS Trigger frame contain the allocated time duration in units of 128µs; other bits are reserved.

The UL Length subfield is reserved in an MU-RTS Trigger frame that is not a MU-RTS TXS Trigger frame.

***TGbe editor: Insert the following text in P341L48 of 11ax draft 8.0 as follows:***

**26.2.4 Updating two NAVs**

An EHT STA that used information from an MU-RTS TXS Trigger frame as the most recent basis to

update its NAV shall not reset the NAV that is updated by this frame unless it receives a CF-End frame that satisfies the conditions in 26.2.5 (Truncation of TXOP).

***TGbe editor: Modify the following text in P66L52 of draft 0.4 as follows:***

**35.2.1.3 Triggered TXOP sharing procedure**

**35.2.1.3.1 General**

The Triggered TXOP sharing procedure allows an AP to allocate a portion of the time within an obtained TXOP to exactly one non-AP STA for transmitting one or more non-TB PPDUs.  
A STA with dot11TXOPSharingTFOptionImplemented equals to true shall set the Triggered TXOP Sharing Support subfield in EHT Capabilities element to 1; otherwise, it shall set the subfield to 0.

An AP and non-AP STA with dot11TXOPSharingTFOptionImplemented equal to 1 shall follow the rules defined in 26.2.6 (MU-RTS Trigger/CTS frame exchange procedure) when transmitting and responding to a MU-RTS TXS Trigger frame respectively with the exceptions defined in 35.2.1.3.2 (AP behavior) and 35.2.1.3.3 (Non-AP STA behavior).

**35.2.1.3.2 AP behavior**

An AP may allocate time within an obtained TXOP to a non-AP STA by transmitting an MU-RTS TXS Trigger frame as defined in 9.3.1.22.5 (MU-RTS Trigger frame format) parametrized as follows:  
— The Trigger frame has one User Info field that is addressed to the non-AP STA. ~~A User Info field is addressed to a non-AP STA if the AID12 subfield of the User Info field is equal to the 12 LSBs of the AID of the STA and the Trigger frame is sent by the AP with which the non-AP STA is associated.~~

An AP shall not send a MU-RTS TXS Trigger frame with the User Info field that is addressed to an associated non-AP STA from which it has not received an EHT Capabilities element with the Triggered TXOP Sharing Support subfield set to 1.

After transmitting an MU-RTS TXS Trigger frame that allocates time to a non-AP STA and receiving the corresponding CTS frame, an AP that transmitted an MU-RTS TXS Trigger frame with TxOP Sharing Modes subfield value set to 1 shall not transmit any PPDU within the allocated time except under the following conditions:

* The AP received a frame from the non-AP STA that requires an immediate response.
* The CS mechanism indicates that the medium is idle at the TxPIFS slot boundary after the end of either the transmission of the last immediate response frame sent to that STA or the reception of the last frame from that STA that did not require an immediate response.

After transmitting an MU-RTS TXS Trigger frame that allocates time to a non-AP STA and receiving the corresponding CTS frame, an AP that transmitted an MU-RTS TXS Trigger frame with TxOP Sharing Modes subfield value set to 2 shall not transmit any PPDU within the allocated time except if it received a frame from the non-AP STA that requires an immediate response.

NOTE—Error recovery of the Triggered TXOP sharing mechanism is the responsibility of the AP when the TxOP Sharing Modes subfield value in the corresponding MU-RTS TXS Trigger frame is set to 1 and is the responsibility of the scheduled non-AP STA when the TxOP Sharing Modes subfield value in the corresponding MU-RTS TXS Trigger frame is set to 2.

NOTE 2- The AP that transmitted an MU-RTS TXS Trigger frame does not transmit any PPDU without performing a new backoff if the TXNAV timer has expired.

An AP that transmitted an MU-RTS TXS Trigger frame and received the corresponding CTS frame from the non-AP STA that was allocated time in that Trigger frame may transmit a PPDU at the end of the allocated time and before its TXNAV timer has expired if it satisifes one of the following conditions:

* The medium is determined to be idle at the end of the allocated time in which case it may transmit SIFS after the end of the allocated time.
* The medium is determined to be busy at the end of the allocated time and the medium busy event is caused by an individually addressed Data or Management frame transmitted by the scheduled non-AP STA to the AP in which case it may transmit SIFS after the end of reception of that frame.
* The medium is determined to be busy at the end of the allocated time and the medium busy event is not caused by an individually addressed Data or Management frame transmitted by the scheduled non-AP STA to the AP in which case it may transmit after the CS mechanism (see 10.3.2.1 (CS mechanism)) indicates that the medium is idle at the TxPIFS slot boundary.

An AP that transmitted an MU-RTS TX Trigger frame and received the corresponding CTS frame ~~with TxOP Sharing Modes subfield value set to 1~~, and the CS mechanism indicates that the medium is busy at the end of the allocated time and the medium busy event is not caused by an individually addressed Data or Management frame transmitted by the scheduled STA to the AP, then the AP might transmit at TxPIFS slot boundary as described above or invoke the backoff procedure described in 10.23.2.2 (EDCA backoff procedure) or wait for the TXNAV timer to expire and invoke the backoff procedure. How it chooses among these options is implementation dependent.

**35.2.1.3.3 Non-AP STA behavior**

After a non-AP STA receives an MU-RTS TXS Trigger frame from its associated AP that contains a User Info field that is addressed to it, the STA shall transmit one or more non-TB PPDUs within the time allocation signalled in the UL Length subfield of Common Info field of the MU-RTS TXS Trigger frame. The first PPDU of the exchange shall be a CTS frame transmitted per the rules defined in 26.2.6.3 (CTS frame response to an MU-RTS Trigger frame).

.

The time allocation starts at the receipt of the PHY-RXEND.indicate corresponding to the PPDU that contained the MU-RTS TXS Trigger frame.

During this allocated time, the non-AP STA may transmit non-TB PPDUs to its associated AP or another STA if the TxOP Sharing Modes subfield value is 2 and only to its associated AP if the TxOP Sharing Modes subfield value is 1.   
NOTE—For example, the other STA can be a peer STA of a peer-to-peer link.

A non-AP STA addressed by a User Info field in the MU-RTS TX Trigger frame ~~(i.e., the AID12 subfield is equal to the 12 LSBs of the AID of the non-AP STA)~~ shall ensure that its PPDU transmission(s) and any expected responses fit entirely within the allocated time except that:

* The non-AP STA may exceed the allocated time if it satisfies any of the conditions described in 10.23.2.9 (TXOP limits) that allows a TXOP holder STA to exceed the TXOP limit.

­­