### IEEE P802.11 Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| PDT Group address frames reception for non-AP MLD | | | | |
| Date: 2021-03-01 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Ming Gan | Huawei |  |  | ming.gan@huawei.com |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Abstract

Revisions:

* Rev 0: Initial version of the document.
* Rev 2: Remove “decides to”

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe 0.4 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe D0.4 Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

Discussion: The baseline rule of group addressed reception for a STA in PS mode receive both group addressed data frames and group addressed management frames. For MLD, there is no need for a different reception procedure based on additional indication on buffered group addressed management frame. The proposed text is written toward this direction to really follow baseline.

***11.2.3.7 Receive operation for STAs in PS mode***

*e) When dot11FMSActivated is false and ReceiveDTIMs is true, the STA shall wake up early enough  
to be able to receive either every non-STBC DTIM or every STBC DTIM sent by the AP of the BSS.  
……  
A STA that stays awake to receive group addressed BUs shall elect to receive all group addressed  
non-STBC transmissions or all group addressed STBC transmissions and remain awake until the  
More Data subfield of the appropriate type (non-STBC or STBC) of group addressed BUs indicates  
there are no further buffered group addressed BUs of that type, or until a TIM is received indicating  
there are no more buffered group addressed BUs of that type,*

***TGbe editor: Modify the title of 35.3.12 Multi-link group addressed frame delivery as follows:***

### 35.3.12 Multi-link group addressed frame delivery and reception

### 35.3.12.1 Beacon transmission

#### Editor’s Note: It is a placeholder subclause.

### 35.3.12.2 Group addressed frame delivery

#### Editor’s Note: It is a placeholder subclause.

#### Editor’s Note: It is a placeholder subclause.

### *TGbe editor: Insert 35.3.12.3 Group addressed frame reception*

### 35.3.12.3 Group addressed frame reception

If an indication of buffered group addressed frames in the TIM element about an AP in an AP MLD is received by any STA affiliated with a non-AP MLD, the STA affiliated with the non-AP MLD that is associated with the AP and that stays awake to receive group addressed BUs shall elect to receive all group addressed frames that are scheduled for delivery in that link

**Straw Poll: Do you support to incorporate the proposed draft text in 11-21-0349r3 to the TGbe Draft?**