IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Comment Resolution for Section 36.3.12.10 (OFDM modulation) | | | | |
| Date: 2021-03-10 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | Email |
| Rui Cao | NXP | 350 Holger Way, San Jose,CA |  | [rui.cao\_2@nxp.com](mailto:rui.cao_2@nxp.com) |

Abstract

This submission proposes resolution for CID 3117 on Section 36.3.12.10 (OFDM modulation) in TGbe D0.3.

Revisons:

* r0: initial version

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page.Line** | **Comment** | **Proposed Change** | **Resolution** |
| 3117 | 36.3.12.10 | 309.59 | change "Kr,min is the minimum set of the set Kr" to "Kr,min is the minimum value of the set Kr" | as in comment. | Accepted.  11be Editor: please make the changes as in  <https://mentor.ieee.org/802.11/dcn/21/11-21-482-00-00be-comment-resolution-for-ofdm-modulation.docx> |

*TGbe Editor: Please make the following change in P309L59 in Section 36.3.12.10 of D0.3.*

is the minimumvalue of the set