IEEE P802.11
Wireless LANs

|  |
| --- |
| CR for CIDs 1809 and 2368 |
| Date: Mar. 22, 2021 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Jason Yuchen Guo | Huawei |  |  | guoyuchen@huawei.com |
| Ming Gan | Huawei |  |  |  |
| Yunbo Li | Huawei |  |  |  |
| Guogang Huang | Huawei |  |  |  |
| Yiqing Li | Huawei |  |  |  |
| Mengyao Ma | Huawei |  |  |  |
| Hongjia Su | Huawei |  |  |  |
| Jianhui Li | Huawei |  |  |  |

 Abstract

This submission proposes resolutions for following CIDs received for TGbe CC34:

1809, 2368

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Commenter** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** |
| 1809 | James Yee | 81.13 | 10.2.7 | "non-AP MLD with which it has done multi-link setup" is an awkward to say "associated non-AP MLD". One assumes a link has been setup for the MPDU to be received. | As suggested | Revised-Agree with the comment that “associated non-AP MLD” is clearer and simpler.TGbe editor:Please implement changes as shown in this document tagged as 1809. |
| 2368 | Muhammad Kumail Haider | 72.39 | 9.4.2.240 | The phrase "Management frame of the STA" is confusing. | Change "of" to "from" or for more clarification, change to "Management frame transmitted by the STA that carried ..." | Revised-Agree with the comment.TGbe editor:Please implement changes as shown in this document tagged as 2368. |

***TGbe editor: Please note baselines are REVmd D5.0, 11ax D8.0 and 11be D0.4***

**10.2 MAC architecture**

***TGbe editor: Please update the subclause as shown below***

**10.2.7 MAC data service**

***Insert the following two paragraphs after the fifth paragraph (“Unless the MPDU is delivered
via DMS ... ”):***

An AP MLD that broadcasts the group addressed MPDU received from an associated non-AP MLD shall set the SA field of the broadcast group addressed MPDU to the MLD MAC address of the non-AP MLD. (#1809)

A non-AP MLD shall filter out the group addressed MPDU with the SA field set to the MLD MAC address of the non-AP MLD.

**9.4.2.240 Non-Inheritance element**

***Insert the following paragraph as the first paragraph of the subclause:***

The Non-Inheritance element can be present as the last element in the Nontransmitted BSSID Profile subelement of a multiple BSSID element or as the last element in the Per-STA Profile subelement of a Basic variant Multi-Link element when the profile is complete.

***Insert the following paragraph after the now-shifted second paragraph (“The Non-Inheritance
element when present ...”):***

The Non-Inheritance element when present in the Per-STA Profile subelement of a Basic variant Multi-link element identifies one or more elements that are not inherited by the STA corresponding to the per-STA profile. The identified elements are present in the Management frame transmitted by the STA that carried the Basic variant Multi-Link element.(#2368)

**Straw Poll: Do you support to incorporate the proposed draft text in this document 11-21/0544r0 to the next revision of TGbe Draft 0.4?**

**Result: Yes/No/Abstain**