IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Spec Text for CR |
| Date: 2021-4-1 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 2 Huntington Quad, Melville, NY 11747USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |

Abstract

This submission proposes the spec text for resolutions for the CID 1498 and 1560. The baseline for this comment resolution document is 802.11bc Draft 1.01.

***TGbc Editor: Please modify the paragraph at P31L18 as follows (802.11bc Draft 1.01)***

The Content ID subfield contains an unsigned integer indicating the identifier of the content. [#1498]

***TGbc Editor: Please modify Figure 9-bc10 as follows (802.11bc Draft 1.01)***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EBCSResponse Info Control | Content ID | Time To Termination | EBCS SPDuration | EBCS SPInterval |

Octets: 1 1 0 or 2 0 or 2 0 or 2

**Figure 9-bc10 - EBCS Response Info subfield format [#1560]**

***TGbc Editor: Please modify the paragraph at P28L17 as follows (802.11bc Draft 1.01)***

The Time To Termination subfield indicates the time to termination in number of TBTTs during which the EBCS identified by the Content ID included in the same EBCS Request Info subfield is broadcast. The format of the Time To Termination subfield is defined in 9.6.7.102 (EBCS Termination Notice frame format). [#1560]