IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Spec Text for CR |
| Date: 2021-07-06 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd StreetNew York, NY 10120USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |

Abstract

This submission proposes the spec text for resolutions for the CID 1340 and 1341. The baseline for this comment resolution document is 802.11bc Draft 1.03.

* Rev 0: first draft

***TGbc Editor: Please modify the Table 9-94 as follows (802.11bc Draft 1.01)***

***TGbc Editor: Please delete Clause 9.6.2.297 (EBCS Request Element) and Clause 9.6.2.298 (EBCS Response element)***

***TGbc Editor: Please modify the text of 11.55.4 as follows (802.11bc D1.03)***

**11.55.4 EBCS Negotiation Procedure for Associated STAs**

To request one or more EBCS traffic streams provided by an EBCS AP with which an EBCS non-AP STA is associated, the STA shall transmit an EBCS Request frame to the EBCS AP. To request one or more EBCS traffic streams that an EBCS AP has indicated require association, an unassociated EBCS non-AP STA shall associate with the EBCS AP and subsequently transmit an EBCS Request frame. A

request for one or more EBCS traffic streams that does not require association may also be included in the

same EBCS Request frame. When requesting an EBCS using an EBCS Request frame, an EBCS non-AP

STA may request an EBCS with a certain time to termination as indicated in the Requested Time To

Termination field included in the EBCS Request frame. This element optionally allows the non-AP STA to

provide the MAC address of the AP currently serving the EBCS stream, which may not be the same as the

one receiving the request.[#1341, 1340]