IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Spec Text for CR Part 5 |
| Date: 2021-07-15 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd StreetNew York, NY 10120USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |
|  |  |  |  |  |

Abstract

This submission proposes the spec text for resolutions for the CID 1365, 1368, 1369. The baseline for this comment resolution document is 802.11bc Draft 1.03.

* Rev 0: first draft

***TGbc Editor: Please modify the text of 11.55.5 as follows (802.11bc D1.03)***

**11.55.5 EBCS Termination Notice Procedure**

The EBCS STA transmitting an EBCS Termination Notice frame shall indicate in the Time To Termination

subfield in an EBCS Termination Info subfield the number of TBTTs before the EBCS identified by the

content ID contained in the Content ID subfield in the same EBCS Termination Info subfield terminates. [#1365]

The EBCS STA transmitting an EBCS Termination Notice frame shall indicate in the Request Method

subfield in an EBCS Termination Info subfield the request method that a STA should use to negotiate for

the extension of the EBCS identified by the content ID contained in the Content ID subfield in the same

EBCS Termination Info subfield. The EBCS STA transmitting an EBCS Termination Notice frame may

indicate in the Destination Address subfield in an EBCS Termination Info subfield the address associated

with the request method indicated in the Request Method subfield in the same EBCS Termination Info

subfield that a STA should use to negotiate for the extension of the EBCS identified by the content ID

contained in the Content ID subfield in the same EBCS Termination Info subfield.

After transmitting an EBCS Termination Notice frame, an EBCS STA shall transmit an EBCS Termination

 Notice frame with an updated value in the Time To Termination subfield in an EBCS Termination Info

subfield if the EBCS identified by the content ID in the Content ID subfield in the same EBCS Termination

Info subfield has been negotiated to have a new time to termination value. If the negotiated duration for the

EBCS is longer than the maximum time to termination value, the transmitting STA shall set the Time To

Termination subfield to 65535.

An EBCS STA that receives an EBCS Termination Notice frame may negotiate for the extension of an

EBCS if the EBCS indicated in one of the EBCS Termination Info subfields terminates earlier than desired.

If the EBCS STA negotiates the extension of the EBCS traffic stream, it shall use the request method indicated in the Request Method subfield in the EBCS Termination Info subfield (see 11.55.4 (EBCS

Negotiation Procedure for Associated STAs) and 11.55 (Enhanced Broadcast Services Procedures)).[#1368, 1369]