IEEE P802.11
Wireless LANs

|  |
| --- |
| D1.0 CR for Section 36.3.9.3 |
| Date: 2021-7-20 |
| Author(s): |
| Name | Affiliation | Address | Phone | Email |
| Wook Bong Lee | Samsung |  |  | wookbong.lee@samusng.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following comments on section 36.3.9.3 of TGbe D1.0:

* 4553, 4544, 6095

Baseline documents: TGbe D1.01.

Revisions:

* Rev 0: Initial version of the document. Use D1.01 as baseline spec text.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Comment** | **Proposed Change** | **Resolution** |
| 4553 | 36.3.19.3 | 529 | Remove the "and frequency segments" | as in the comment. | Accepted |
| 4554 | 36.3.19.3 | 530 | Wrong reference. Should be "as defined in 36.3.16" | as in the comment. | Accepted |
| 6095 | 36.3.19.3 | 530 | Wrong reference to 36.3.15 (Non-HT duplicate transmission) | Correct reference is 36.3.16 (Transmit requirements for PPDUs sent in response to a triggering frame) | AcceptedNote to editor: 4554 and 6095 are same resolution. |