IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR to 36.3.8 EHT-MCSs and 36.3.9 EHT-SIG-MCSs | | | | |
| Date: 2021-09-13 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Yujin Noh | Senscomm |  |  | yujin.noh@senscomm.com |
| Bo Sun | ZTE |  |  |  |
| Ruchen Duan | Samgsung |  |  |  |
| Youhan Kim | Qualcomm |  |  |  |

Abstract

This submission shows

* Resolutions for comments from TGbe draft 1.0.
  + 3 CIDs: 6832, 8096, and 8097
* Baseline document is TGbe draft 1.2.


Revisions:

* Rev 0: Initial version of the document.
* Rev 1: Baseline document updated to TGbe draft 1.2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **CID** | **P.L** | **Comment** | **Proposed Change** | **Resolution** |
| 6832 | 388.38 | EHT-MCS 14 and EHT-MCS 15 enable DCM on top of EHT-MCS 0. EHT-MCS 14 and EHT-MCS 15 are supported only with 1SS. | Better not use 1SS in text, change to 1 stream | Revised.  Agreed in principle. Same modificaiton is applied to CIDs 6832 and 8096.  To TGbe editor: change 1SS to one spatial stream at P488L39 in 11be draft 1.2. |
| 8096 | 388.39 | 1SS better be 1 spatial stream to improve the text | as in comment | Revised.  Agreed in principle. Same modificaiton is applied to CIDs 6832 and 8096.  To TGbe editor: change 1SS to one spatial stream at P438L39 in 11be draft 1.2. |
| 8097 | 388.45 | EHT-SIG-MCS field and EHT-SIG MCS field are mixed in use. It should be consistent. In the Table Table 36-28, the name of the field is EHT-SIG MCS field. | as in comment | Revised.  Agreed in principle. However more locations are found as below.  To TGbe editor: change EHT-SIG-MCS field to EHT-SIG MCS field at P488L45, P477L34 and P558L6 in 11be draft 1.2. |

***Discussion***


At P488L45



Graphical user interface, text, application

Description automatically generated

At P477L34



At P558L6

