IEEE P802.11  
Wireless LANs


|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Comment Resolution for CID 2249 | | | | |
| Date: 2022-02-14 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Shimi Shilo | Huawei Technologies Co., Ltd | 4 Ha’harash St., Hod Hasharon |  | [shimi.shilo@huawei.com](mailto:shimi.shilo@huawei.com) |

Abstract

This document proposes a comment resolution for CID 2249 (REVme D1.0).

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| | **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** | **Owning Ad-hoc** | | --- | --- | --- | --- | --- | --- | --- | | 2249 | 4368.56 | 27.3.11.7.2 | Add an ‘in’ before the term ‘UL’ in the phrase ‘is sent UL or DL’ | Add ‘in’ before ‘UL’ | Revised; agree in principle.  In order to phrase it better, add ‘in the’ before ‘UL’, and add ‘direction’ at the end of the sentence.  Please make the changes shown in document: <https://mentor.ieee.org/802.11/dcn/22/11-22-336-00-000m-comment-resolution-for-cid-2249.docx> | PHY | |

**Discussion:**



**Proposed Comment Resolution**

Revised: Make the following changes:

Indicates whether the PPDU is sent in the UL or DL. Set to 1 if the PPDU is addressed to an AP. Set to 0 otherwise. See TXVECTOR parameter UPLINK\_FLAG.

Instruction to Editor:

At page 4372 (REVme D1.0) line 30 – make the same change.