IEEE P802.11
Wireless LANs

|  |
| --- |
| CID 1428 concerning BSSMaxIdlePeriod |
| Date: 2022-02-18 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| David Halasz | Morse Micro |  |  | dave.halasz@morsemicro.com |
| Dave Goodall | Morse Micro |  |  | dave@morsemicro.com |

Abstract

This document proposes comment resolutions for LB258 CID 1428.

*Discussion :*

CID 1428 is shown on the next page.

Proposed Resolution:

* CID 1428 : Accept.

|  |  |  |  |
| --- | --- | --- | --- |
| **CID** | **Clause Number** | **Comment** | **Proposed Change** |
| 1428 | 6 | Sometimes BSSMaxIdlePeriod is "optionally present ifdot11WirelessManagementImplementedanddot11BSSMaxIdlePeriodIndicationByNonAPSTA are true, or ifdot11S1GOptionImplemented is true;", sometimes just "present ifdot11WirelessManagementImplementedis true or dot11S1GOptionImplementedis true;" | Make it consistent |

*Proposed change : for clause 6.3.7.3.2*

|  |  |  |  |
| --- | --- | --- | --- |
| BSSMaxIdlePeriod | As defined in BSS Max Idle Period element | As defined in 9.4.2.78 (BSS Max Idle Period element) | Indicates the BSS max idle period parameters of the AP or PCP. This parameter is present if dot11WirelessManagementImplemented (#142) and dot11BSSMaxIdlePeriodIndicationByNonAPSTA are true, or dot11S1GOptionImplemented (#139)is true and the BSS Max Idle Period element was present in the Association Response frame; is not present otherwise. |

*Proposed change : for clause 6.3.7.5.2*

|  |  |  |  |
| --- | --- | --- | --- |
| BSSMaxIdlePeriod | BSS Max Idle Period element | As defined in 9.4.2.78 (BSS Max Idle Period element) | Indicates the BSS max idle period parameters of the AP or PCP. This parameter is present if dot11WirelessManagementImplemented and dot11BSSMaxIdlePeriodIndicationByNonAPSTA are true, ~~is true~~ or dot11S1GOptionImplemented is true; otherwise not present.(#137) |

*Proposed change : for clause 6.3.8.3.2*

|  |  |  |  |
| --- | --- | --- | --- |
| BSSMaxIdlePeriod | BSS Max Idle Period element | As defined in 9.4.2.78 (BSS Max Idle Period element) | Indicates the BSS max idle period parameters of the AP or PCP. This parameter is present if dot11WirelessManagementImplemented and dot11BSSMaxIdlePeriodIndicationByNonAPSTA are true, ~~is true~~ or dot11S1GOptionImplemented is true; otherwise not present. |

*Proposed change : for clause 6.3.8.5.2*

|  |  |  |  |
| --- | --- | --- | --- |
| BSSMaxIdlePeriod | BSS Max Idle Period element | As defined in 9.4.2.78 (BSS Max Idle Period element) | Indicates the BSS max idle period parameters of the AP or PCP. This parameter is present if dot11WirelessManagementImplemented and dot11BSSMaxIdlePeriodIndicationByNonAPSTA are true, ~~is true~~ or dot11S1GOptionImplemented (#139)is true and the BSS Max Idle Period element was present in the Association Response frame; is not present. |

**References:**