IEEE P802.11Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Proposed Resolutions for CID 7211, 7212 and 7217 of 11az SAB1 | | | | |
| Date: 2022-04-26 | | | | |
| Author(s): | | | | |
| Name | Company | Address | Phone | email |
| Tianyu Wu | Apple Inc. |  |  | tianyu@apple.com |
| Qi Wang |  |  | qi\_wang2@apple.com |

Abstract

This submission proposes the resolutions to 11az SA1 CID 7211,7212 and 7217.

The page and line numbers refer to those in 11az Draft 4.1 [1].

**Introduction**

This submission proposes the resolutions to 11az SAB1 CID 7211, 7212 and 7217.

The page and line numbers refer to those in 11az Draft 4.1 [1].

**Comments:**

**CID 7211 and 7212**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page/Line | Clause | Comment | Proposed change | Resolution |
| 7211 | 236/15 | 27.3.18a.1 | Should clarify that pre-HE modulated fields of PPDU in HE Ranging NDP are the same as the pre-HE modulated fields in a HE SU PPDU | Add bullet point before line 15, saying "pre-HE modulated fields in HE Ranging NDP is the same as the pre-modulated fields in a HE SU PPDU" | Revised.  Agree with commenter to clarify the definition for pre-HE modulated fields in HE Ranging NDP.  TGaz editor: please incorporate the text changes in this document (22/0672r1) with tag #7211. |
| 7212 | 236/15 | 27.3.18a.1 | For the HE Ranging NDP, the bits that are assigned in the L-SIG and HE-SIG-A should be the same as the bits assign for an HE SU PPDU, unless otherwise specified this section | Add bullet point before line 15, saying "Bit assignments for L-SIG and HE-SIG-A should be the same as the bit assignments for an HE SU PPDU, unless otherwise specified" | Revised.  Agree with commenter to clarify the definition for pre-HE modulated fields including bit assignments for L-SIG and HE-SIG-A in HE Ranging NDP.  TGaz editor: please incorporate the text changes in this document (22/0672r1) with tag #7212. |

**Proposed resolution**

***TGaz Editors: Please modify the text on page 237/line 7 of D4.1 as shown below: (#7211, #7212 )***

**27.3.18a.1 HE Ranging NDP**

The HE Ranging NDP has the following properties:

— Uses the HE SU PPDU format but without the Data field.

— The L-STF and L-LTF fields in an HE Ranging NDP are the same as the L-STF and L-LTF fields in an HE SU PPDU. The subfields in L-SIG, RL-SIG and HE-SIG-A have same bit assignments and definitions as the subfields in a HE SU PPDU unless specified otherwise.

— No beamforming steering matrix is applied to the waveform. The Beamformed field in HE-SIG-A of an HE Ranging NDP is always set to 0. For transmission of HE-STFs and HE-LTFs, if NSTS = NTx, the Q matrix shall be an Identity matrix, and if NSTS < NTx, the Q matrix shall be based on an antenna selection matrix with no antenna swapping. The Q matrix becomes an Identity matrix when all 0 rows are removed. (#**2302**, #**3270**, #**5090**)

**CID 7217 – Deferred**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CID | Page/Line | Clause | Comment | Proposed change | Resolution |
| 7217 | 267/03 | B.4.37.2 | Annex B needs to be updated. The term NGP is no longer used. Additionally, section B.4.37.2 is missing Tx Window from PHY PICS section | Remove NGP and update with row for Tx Window. Also note p.268 | Revised.  Agree with commenter to update the Annex B.  TGaz editor: please incorporate the text changes in this document (22/0672r0) with tag #7217. |

**~~Proposed resolution~~**

***~~TGaz Editors: Please modify the text on page 264/line 1 of D4.1 as shown below: (#7217)~~***

**~~B.4.37 Enhanced Positioning (Ranging) features~~**

**~~B.4.37.1 EP MAC Features (#3281, #3387)~~**

***~~TGaz Editors: Please change all NGP to EP in B.4.37.1 of D4.1 (#7217)~~***

**~~B.4.37.2 EP PHY Features (#3281, #3387)~~**

***~~TGaz Editors: Please change all NGP to EP in B.4.37.2 of D4.1 (#7217)~~***

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **~~Item~~** | **~~Protocol capability~~** | **~~References~~** | **~~Status~~** | **~~Support~~** |
|  | ~~Are the following PHY protocol features supported?~~ |  |  |  |
| ~~EPP1~~ | ~~EP TB and non-TB measurement exchange waveforms~~ | ~~[27.3](#_bookmark332) (HE PHY)~~ |  |  |
| ~~EPP1.1~~ | ~~HE ranging NDP~~ | ~~[27.3.18a](#_bookmark336) (HE~~  ~~Ranging NDP)~~ | ~~(CFTB OR CFNTB OR CFPTB):M~~ | ~~Yes  No  N/A ~~ |
| ~~EPP1.2~~ | ~~HE ranging NDP with secure HE- LTFs~~ | ~~[27.3.18a](#_bookmark336) (HE~~  ~~Ranging NDP)~~ | ~~(CFTB OR CFNTB):M CFPASN:M CFPSEC:M~~ | ~~Yes  No  N/A ~~ |
| ~~EPP1.3~~ | ~~HE TB ranging NDP~~ | ~~[27.3.18b](#_bookmark341) (HE~~  ~~TB Ranging NDP)~~ | ~~CFTB:M~~ | ~~Yes  No  N/A ~~ |
| ~~EPP1.4~~ | ~~HE TB ranging NDP with secure HE-LTFs~~ | ~~[27.3.18b](#_bookmark341) (HE~~  ~~TB Ranging NDP)~~ | ~~CFPASN:M CFPSEC:M CFTB:M~~ | ~~Yes  No  N/A ~~ |
| ~~EPP2~~ | ~~MIMO operation~~ |  |  |  |
| ~~EPP2.1~~ | ~~Multi transmit streams~~ | ~~[11.21.6.4.3](#_bookmark225)~~  ~~(TB ranging measurement~~ | ~~(CFTB or CFNTB):M~~ | ~~Yes  No  N/A ~~ |

**References**

[1] IEEE P802.11az™/D4.1, Draft Standard for information technology – Telecommunications and information exchange between systems Local and metropolitan area networks – Specific requirements, Part 11: Wireless LAN Medium Access Control (MAC) and Physical Layer (PHY) Specifications, Amendment 4: Enhancements for positioning