IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CR for CID 7727 | | | | |
| Date: 2022-5-11 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Xiaofei Wang | InterDigital Inc. | 111 West 33rd Street  Suite 1420  New York, NY, USA | +1-607-592-2727 | Xiaofei.wang@interdigital.com |
| Rui Yang |  |  |

Abstract

This submission proposes resolutions for the CID 7727.The baseline for this comment resolution document is 802.11be Draft 1.5.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Page** | **Line** | **Comment** | **Proposed Change** | **Resolution** |
| 7727 | 35.3.14.7.2 | 280 | 28 | The note describes normative behavior and should be in regular spec text | as in comment | Rejected:  The group discussed the note vs normative behavior; it is unclear whether transforming the note to normative behavior provides additional clarity. |

***TGbe Editor: Please modify Subclause 35.3.16.8.2 (802.11be D1.5) as follows:***

**35.3.16.8.2 MediumSyncDelay OFDM ED based recovery procedure(#6352)**

A non-AP STA shall initialize dot11MSDOFDMEDthreshold to –72 dBm and MSD\_TXOP\_MAX to 1, respectively. A non-AP STA affiliated with a non-AP MLD shall set MSD\_TXOP\_MAX and dot11MSDOFDMEDthreshold to the most recent values in the Medium Synchronization Maximum Number Of TXOPs and Medium Synchronization OFDM ED Threshold subfields, respectively, if they are present in a (#6700)Basic Multi-Link element received from its associated AP(#4414).

If either the intra-BSS NAV or the Basic NAV(#5106) is nonzero in the non-AP STA affiliated with the non-AP MLD when it starts the MediumSyncDelay timer, the non-AP STA shall not initiate any TXOP and follow the same rules for HE STAs to respond to any RTS or MU-RTS frames until both NAVs expire. [#7727]