IEEE P802.11
Wireless LANs

|  |
| --- |
| Proposed Comment Resolution for CIDs 108 and 109 |
| Date: 2022-06-13 |
| Author(s): |
| Name | Company | Address | Phone | email |
| Stephen McCann | Huawei Technologies Co., Ltd | Southampton, UK |  | stephen.mccann@ieee.org  |

Abstract

This document proposes a comment resolutions for CIDs 108 and 109 (802.11bf D0.1).

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|

| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** | TTT |
| --- | --- | --- | --- | --- | --- | --- |
| 108 | 28.14 | 9.3.1.25 | There is an additional sentence in the baseline (REVme D1.2 P1001L52) that also needs to be updated in this clause as there are now 2 tables. | Commenter will provide a submission. | Revised: Please make the changes shown in document: <https://mentor.ieee.org/802.11/dcn/22/11-22-0824-00-00bf-comment-resolution-for-cids-107-108-109.docx> indicated by #108. | DMG Clause 9 |

 |

**CID 108 Discussion**

*There is a sentence on P1001L52 of REVme D1.2, that discusses Table 9-55. This sentence needs to be extended to include the new Table 9-55a introduced by 11bf D0.1.*

*In addition, it seems strange to title a table “…when the TDD Beamforming frame type subfield is set to 3”. I think this can be easily re-written.*

**Proposed Comment Resolutions**

REVISED: Make the following changes:

**9.3.1 Control frames**

**9.3.1.25 TDD Beamforming frame format**

**9.3.1.25.1 Overview**

***Change the 6th paragraph as follows: (#108)***

If the TDD Beamforming frame type subfield is not equal to 3 ~~Collectively~~, the TDD Group Beamforming, TDD Beam Measurement, and RA field values indicate a TDD Beamforming frame usage, as listed in Table 9-55 (TDD Beamforming frame usage(11ay))~~.~~, otherwise the TDD Group Beamforming and TDD Beam Measurement, indicate a TDD Beamforming frame usage, as listed in Table 9-55a (#108).

***~~Change the title of Table 9-55 (TDD Beamforming frame usage) to “TDD Beamforming frame usage when TDD Beamforming frame type subfield is not set to 3 (DMG Sensing)”.~~***

***Insert the following table after Table 9-55 (TDD Beamforming frame usage):***

**Table 9-55a—TDD Beamforming frame usage for DMG Sensing ~~when the TDD Beamforming frame type subfield is set to 3 (DMG Sensing)~~ (#108)**

****

***Change the last row in Table 9-56 (TDD Beamforming Frame Type subfield definition) as follows:***

**Table 9-56—TDD Beamforming Frame Type subfield definition**

****

| **CID** | **Page** | **Clause** | **Comment** | **Proposed Change** | **Resolution** | TTT |
| --- | --- | --- | --- | --- | --- | --- |
| 109 | 88.4 | 11.21.20.5.5a | It appears that the "DMG Sensing Request" is defined as "DMG Multistatic Sensing Request", but this is not clear. | Either define a "DMG Sensing Request" or change all occurences of "DMG Sensing Request" to "DMG Multistatic Sensing Request". | Revised: Change all occurrences of "DMG Sensing Request" to "DMG Multistatic Sensing Request". | DMG Clause 11 |