IEEE P802.11
Wireless LANs

|  |
| --- |
| LB266 Annex B CIDs |
| Date: 2022-08-23 |
| Author(s): |
| Name | Affiliation | Address | Phone | email |
| Sigurd Schelstraete | MaxLinear |  |  | sschelstraete@maxlinear.com |
|  |  |  |  |  |

Abstract

This submission proposes resolutions for the following CIDs:

* 10391 and 11226

# CIDs

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause Number** | **Page** | **Comment** | **Proposed Change** | **Proposed Resolution** |
| 10391 | AnnexB | 811.60 | should be "... tone RU" instead of "... tone-RU" | Change "... tone-RU" into "... tone RU" | Accepted |
| 11226 | B.4.3 | 805.49 | 80 MHz support is not required for 2.4 GHz. | Make CFEHT80 be conditional mandatory on CFEHT5G or CFEHT6G. | RevisedAgree in principle with commenter.Editor’s instruction: apply changes as proposed in 802.11-22/1390r0 |

# Discussion

The CIDs apply to the following places in the draft:

CID 10391:



This is editorial and proposed resolution is accepted.

CID 11226:



As currently written, this states that 80 MHz is mandatory if the device is an AP and it supports EHT. In reality, 80 MHz is not required when operating in 2.4 GHz, only in 5 GHz and 6 GHz.

To correctly capture this, the proposed resolution is to make the following changes to the Table on page 817 of D2.1:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| \*CFEHT80 | EHT operation with capability of 80 MHz or wider channel width | Clause 36 | CFAP AND CFEHT AND CFEHT5G: MCFAP AND CFEHT AND CFEHT6G: MCFIndepSTA AND CFEHT: O.11 | Yes ☐ No ☐ |