IEEE P802.11  
Wireless LANs

|  |
| --- |
| **LB266 Comment Resolutions for CID 12937** |
| **Date:** 2022-09-05 |
| **Author(s):** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Name** | **Affiliation** | **Address** | **Phone** | **Email** |
| Eunsung Park | LG Electronics | 19, Yangjae-daero 11gil, Seocho-gu, Seoul 137-130, Korea |  | esung.park@lge.com |
| Dongguk Lim |  | dongguk.lim@lge.com |
| Jinyoung Chun |  | jiny.chun@lge.com |
| Jinsoo Choi |  | js.choi@lge.com |

Abstract

This submission proposes a resolution for CID 12937.

Revisions:

* Rev 0: Initial version of the document.

Interpretation of a Motion to Adopt

A motion to approve this submission means that the editing instructions and any changed or added material are actioned in the TGbe D2.1 Draft. This introduction is not part of the adopted material.

***Editing instructions formatted like this are intended to be copied into the TGbe D2.1 Draft (i.e. they are instructions to the 802.11 editor on how to merge the text with the baseline documents).***

***TGbe Editor: Editing instructions preceded by “TGbe Editor” are instructions to the TGbe editor to modify existing material in the TGbe draft. As a result of adopting the changes, the TGbe editor will execute the instructions rather than copy them to the TGbe Draft.***

#### *CID 12937*

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **PP.LL** | **Comment** | **Proposed Change** | **Resolution** |
| 12937 |  |  | Condiser a 20 MHz-only 11be operation |  | Rejected  The comment fails to identify a technical issue and 11be already supports a 20 MHz operating non-AP EHT STA. Please refer to 36.3.2.5. 20 MHz operating non-AP EHT STAs. |