IEEE P802.11  
Wireless LANs

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Resolutions for CIDs in Clause 36.3.2.2.1 | | | | |
| Date: July 26, 2022 | | | | |
| Author(s): | | | | |
| Name | Affiliation | Address | Phone | email |
| Jianhan Liu | MediaTek |  |  | Jianhan.Liu@mediatek.com |
| You-Wei Chen |  |  | you-wei.chen@mediatek.com |

Abstract

This submission proposes resolutions for following 3 CIDs received for TGbe LB266:

10403, 12196, 12569

**Revisions:**

* Rev 0: Initial version of the document.

**TGbe editor: The baseline for this document is 11be D2.0. In the resolution, the page and line in D2.1 are also added as a note to the editor.**

# CID 10403, 12196, 12569

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **CID** | **Clause** | **Pg/Ln** | **Comment** | **Proposed Change** | **Resolution** |
| 10403 | 36.3.2.2.1 | 577.48 | It should be "242-tone RUs" instead of "242-tones RUs" | Change "242-tones RUs" into "242-tone RUs" | **Accepted**  Note: Medications in D2.1 (Page/Line) P589/L48 |
| 12196 | 36.3.2.2.1 | 577.40 | The abbreviation MRU is already defined in 36.1.1 and in the abbreviation list in Section 3. | Remove the definition of this abbreviation from this line. | **Revised.**  Agree with the commentor.  11be Editor: please make the changes according to “Text modification of CID 12196: D2.1 (Page/Line) P589/L40” in doc IEEE 802.11-22/1547r0. |
| 12569 | 36.3.2.2.1 | 577.47 | Inconsistent indication of the RUs, in some cases 242-tones 'tones, plural' is used and in some other cases 242-tone "tone, singular" is used. Multiple occurrences D2.0P577L48 and D2.0P738L53. | Change "242-tones" to "242-tone" | **Accepted**  11be Editor: please make the changes as in the proposed change (in D2.1) (Page/Line):  P589/L48  P750/L53 |

**Text modification of CID 12196: D2.1 (Page/Line) P589/L40**

The EHT PHY supports the usage of ~~multiple resource unit (~~MRU~~)~~ in an EHT PPDU. An MRU consists of selected combinations of multiple RUs of 26-tone RU, 52-tone RU, 106-tone RU, 242-tone RU, 484-tone RU, 996-tone RU, and 2×996-tone RU. The tone indices of the various RUs for different EHT PPDU bandwidths are defined in 36.3.2.1 (Subcarriers and resource allocation in EHT PPDUs).